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	JOSE RAMON ARDAVIN ITUARTE, Sub-Secretary of Environmental Development and Standards of the Secretary of Environment and Natural Resources, and President of the National Consultative Committee of Standardization of Environment and Natural Resources, based on the provision in articles 32 Supp. Sections I, II, IV, and V of the Organic Law of the Federal Public Administration; 6 section XIX and 8 section V of the Internal Regulation of the Secretary of Environment and Natural Resources; 1, sections I, II, III, and VI, 5, sections V and VI, 36, 37 supp. 150, 151, 160, and 171 of the General Law of Ecological Equilibrium and the Protection of the Environment; 7 section II, 15, sections I, III, 16, 22, 31, 42, 43, 45, and 67 section VIII of the General Law of Prevention and Integral Management of Wastes; 4 section I of the Regulation of the General Law of Ecological Equilibrium and Protection of the Environment in matters of Hazardous Wastes; 38 section II, 40, sections X, XIII and XVII, 47 section I 51, and 73 of the Federal Law on Metrology and Standardization; 33 and 40, sections III and IV of the Regulation of the Federal Law on Metrology and Standardization, and 


	CONSIDERANDO
	CONSIDERING


	Que las disposiciones de la Ley General del Equilibrio Ecológico y la Protección al Ambiente y de la Ley General para la Prevención y Gestión Integral de los Residuos son de orden público e interés social y tienen por objeto propiciar el desarrollo sustentable y establecer, entre otras, las bases para garantizar el derecho de toda persona a vivir en un medio ambiente adecuado para su desarrollo, salud y bienestar; definir los principios de la política ambiental y los instrumentos para su aplicación; la preservación, la restauración y el mejoramiento del ambiente, así como la prevención y el control de la contaminación del aire, agua y suelo.
	That the provisions of the General Law of Ecological Equilibrium and the Protection of the Environment and of the General Law of Prevention and Integral Management of Wastes are of public order and social interest and have the purpose of promoting sustainable development and establishing, among other things, the criteria for guaranteeing the right of all persons to live in an environment adequate for their development, health, and wellbeing; define the principles of environmental policy and the instruments for their application; the preservation, the restoration, and the improvement of the environment, as well as the prevention and the control of the contamination of air, water and soil.  


	Que los citados ordenamientos legales establecen que las normas oficiales mexicanas contendrán, entre otros temas, los listados que clasifiquen los materiales y residuos peligrosos considerando sus características.
	That the aforementioned legal ordinances establish that the Official Mexican Standards will contain, among other subjects, the lists that classify hazardous materials and wastes considering their characteristics. 


	Que con fecha 22 de octubre de 1993 se publicó en el Diario Oficial de la Federación la Norma Oficial Mexicana NOM-CRP-001-ECOL/1993, Que establece las características de los residuos peligrosos, el listado de los mismos y los límites que hacen a un residuo peligroso por su toxicidad al ambiente; dicha Norma mediante acuerdo secretarial publicado en el Diario Oficial de la Federación el 29 de noviembre de 1994, actualizó su nomenclatura quedando como NOM-052-ECOL-1993.
	That on the 22nd of October of 1993 the NOM-CRP-001-ECOL/1993, that establishes the characteristics of hazardous wastes, the list of the same, and the limits that make waste hazardous by its toxicity to the environment was published in the Official Daily of the Federation; said Standard through an agreement of the Secretary published in the Official Daily of the Federation on the 29th of November of 1994, updated its nomenclature to remain as NOM-052-ECOL-1993. 

	Que los residuos peligrosos se han diversificado en la medida que se modifican o presentan nuevos procesos de extracción, transformación, producción, uso y tratamiento, por lo que se hizo necesario revisar la NOM-052-ECOL-1993, acorde a las modificaciones de la legislación aplicable.
	That the hazardous wastes have diversified to the measure that they are modified or they present new processes of extraction, manufacture, production, use and treatment, which made it necessary to review the NOM-052-ECOL-1993, according to the modifications of the applicable legislation. 


	Que con fecha 22 de octubre de 1999, se publicó en el Diario Oficial de la Federación el Proyecto de Norma Oficial Mexicana PROY-NOM-052-ECOL-1999, Que establece las características, el procedimiento de identificación, clasificación y el listado de los residuos peligrosos con el fin de que los interesados dentro del plazo legal que establece la ley en la materia presentaran sus comentarios ante el Comité Consultivo Nacional de Normalización para la Protección Ambiental; que durante el citado plazo, los interesados presentaron sus comentarios y modificaciones al proyecto en cuestión, que al ser analizados algunos se consideraron procedentes y como consecuencia se hicieron modificaciones sustanciales al mismo.
	That on the 22nd of October of 1999, the Project of the Official Mexican Standard PROY-NOM-052-ECOL-1999, that establishes the characteristics, the procedure of identification, classification, and the list of the hazardous wastes was published in the Official Daily of the Federation so that the interested parties within the legal time period established in the law might present their comments before the National Consultative Committee of Standardization for Environmental Protection; that during the aforementioned time period, the interested parties might present their comments and modifications to the Project in question, that after being analyzed some were considered appropriate and as a consequence, substantial modifications were made to the same. 


	Que derivado de lo anterior, el mencionado Comité, en cumplimiento con lo establecido por el artículo 33 del Reglamento de la Ley Federal sobre Metrología y Normalización, determinó someter el proyecto modificado al periodo de consulta pública, bajo la denominación de PROY-NOM-052-ECOL-2001, Que establece las características, el procedimiento de identificación, clasificación y el listado de los residuos peligrosos.


	That due to the latter, the aforementioned Committee in compliance with that established in Article 33 of the Regulation of the Federal Law on Metrology and Standardization determined to submit the modified project to the period of public consultation, under the name of PROY-NOM-052-ECOL-2001, That establishes the characteristics, the procedure of identification, classification and the list of the hazardous wastes. 

	Que el PROY-NOM-052-ECOL-2001, Que establece las características, el procedimiento de identificación, clasificación y el listado de los residuos peligrosos, de conformidad con los preceptos antes invocados, se publicó a consulta pública el 26 de julio de 2002, a efecto de que los interesados, dentro de los 60 días naturales siguientes a la publicación en el Diario Oficial de la Federación, emitieran sus comentarios ante el Comité Consultivo Nacional de Normalización de Medio Ambiente y Recursos Naturales, sito en Bulevar Adolfo Ruiz Cortines número 4209, piso 5o., colonia Jardines en la Montaña, código postal 14210, Delegación Tlalpan, México, D.F., vía fax 5628-0632 o al correo electrónico: industria@semarnat.gob.mx  
	That the PROY-NOM-052-ECOL-2001, That establishes the characteristics, the procedure of identification, classification, and the list of the hazardous wastes, in conformity with the previously invoked precepts was published for public consultation on the 26th of July of 2002, so that the interested parties, within the 60 calendar days following its publication in the Official Daily of the Federation might issue their comments before the National Consultative Committee of Standardization of Environment and Natural Resources, located on Boulevard Adolfo Ruiz Cortines number 4209, 5th floor., colonia Jardines en la Montaña, postal code 14210, Delegation Tlalpan, Mexico, Federal District, by fax 5628-0632 or email: 
industria@semarnat.gob.mx  



	Que el día 23 de abril de 2003 apareció en el Diario Oficial de la Federación un acuerdo a través 
del cual se reforma la nomenclatura de las normas oficiales mexicanas expedidas por la Secretaría de 
Medio Ambiente y Recursos Naturales, cambiando el nombre tanto de la NOM-052-ECOL-1993 como 
del PROY-NOM-052-ECOL-2001 a NOM-052-SEMARNAT-1993 y PROY-NOM-052-SEMARNAT-2001, 
respectivamente.


	That on the 23rd of April of 2003 there appeared in the Official Daily of the Federation an agreement by which the nomenclature of the Official Mexican Standards issued by the Secretary of Environment and Natural Resources, changing the name of the NOM-052-ECOL-1993 as well as the PROY-NOM-052-ECOL-2001 to NOM-052-SEMARNAT-1993 and PROY-NOM-052-SEMARNAT-2001, respectively. 

	Que el 8 de octubre de 2003 fue publicada, en el Diario Oficial de la Federación, la Ley General para la Prevención y Gestión Integral de los Residuos.
	That on the 8th of October the General Law for the Prevention and Integral Management of Wastes was published in the Official Daily of the Federation. 


	Que de acuerdo a lo establecido en el artículo 47 fracciones II y III de la Ley Federal sobre Metrología y Normalización, los interesados presentaron sus comentarios al proyecto de norma en cuestión, los cuales fueron analizados por el Comité Consultivo Nacional de Normalización de Medio Ambiente y Recursos Naturales en su sesión del 15 de diciembre de 2005, realizándose las modificaciones procedentes al proyecto, las cuales contemplaron las disposiciones establecidas en la Ley General para la Prevención y Gestión Integral de los Residuos.
	That according to that established in Article 47 sections II and III of the Federal Law on Metrology and Standardization, the interested parties presented their comments to the Project of Standard in question which were analyzed by the National Consultative Committee of the standardization of Environmental and Natural Resources in its session on the 15th of December of 2005, making the appropriate modifications to the project, which considered the provisions established in the General Law for the Prevention and Integral Management of Wastes.


	Que habiéndose cumplido el procedimiento establecido en la Ley Federal sobre Metrología y Normalización para la elaboración de normas oficiales mexicanas y con base en lo dispuesto en el artículo 28 fracción I inciso d) del Reglamento de la Ley Federal sobre Metrología y Normalización, el Comité Consultivo Nacional de Normalización de Medio Ambiente y Recursos Naturales, aprobó las respuestas a los comentarios derivados de la consulta pública, así como la versión definitiva de esta Norma Oficial Mexicana.
	That having complied with the procedure established in the Federal Law on Metrology and Standardization for the creation of Official Mexican Standards and based on the provision in article 28 section I clause d) of the Regulation of the Federal Law on Metrology and Standardization, the National Consultative Committee of Standardization of Environment and Natural Resources approved the responses to the comments derived from the public consultation, as well as the permanent version of this Official Mexican Standard.


	Por lo expuesto y fundado, he tenido a bien expedir la siguiente:
	For that expressed and legally justified, I have seen fit to issue the following: 
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	En la elaboración de esta Norma Oficial Mexicana participaron:
	In the creation of this Official Mexican Standard the following participated:
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	1. Introducción
	1. Introduction

	Los residuos peligrosos, en cualquier estado físico, por sus características corrosivas, reactivas, explosivas, inflamables, tóxicas, y biológico-infecciosas, y por su forma de manejo pueden representar un riesgo para el equilibrio ecológico, el ambiente y la salud de la población en general, por lo que es necesario determinar los criterios, procedimientos, características y listados que los identifiquen.
	Hazardous wastes, in any physical state, by their corrosive, reactive, explosive, flammable, toxic, and biological infectious characteristics, and by their form of handling can represent a risk for ecological balance, the environment and the health of the population in general, for which it is necessary to determine the criteria, procedures, characteristics, and lists that identify them. 


	Los avances científicos y tecnológicos y la experiencia internacional sobre la caracterización de los residuos peligrosos han permitido definir como constituyentes tóxicos ambientales, agudos y crónicos a aquellas sustancias químicas que son capaces de producir efectos adversos a la salud o al ambiente.
	The scientific and technological advances and the international experience on the characterization of the hazardous wastes have permitted defining as toxic environmental ingredients, acute and chronic to those chemical substances that are capable of producing adverse effects on health or the environment. 


	2. Objetivo
	2. Objective

	Esta Norma Oficial Mexicana establece el procedimiento para identificar si un residuo es peligroso, el cual incluye los listados de los residuos peligrosos y las características que hacen que se consideren como tales.
	This Official Mexican Standard establishes the procedure for identifying if a waste is hazardous, which includes the lists of the hazardous wastes and the characteristics that make them be considered as such. 


	3. Campo de aplicación
	3. Field of application

	Esta Norma Oficial Mexicana es de observancia obligatoria en lo conducente para los responsables de identificar la peligrosidad de un residuo.
	This Official Mexican Standard is of obligatory observance applicable for the persons responsible for identifying the hazard of a waste. 


	4. Referencias
	4. References

	4.1 Norma Oficial Mexicana NOM-004-SEMARNAT-2002, Protección Ambiental.-Lodos y biosólidos.- Especificaciones y límites máximos permisibles de contaminantes para su aprovechamiento y disposición final, publicada en el Diario Oficial de la Federación el 15 de agosto de 2003.
	4.1 Official Mexican Standard NOM-004-SEMARNAT-2002, Environmental – Sludge and bio-solids. Specifications and maximum permissible limits of contaminants for their utilization and final disposition, published in the Official Daily of the Federation on the 15th of August of 2003. 


	4.2 Norma Oficial Mexicana NOM-053-SEMARNAT-1993, Que establece el procedimiento para llevar a cabo la prueba de extracción para determinar los constituyentes que hacen a un residuo peligroso por su toxicidad al ambiente, publicada en el Diario Oficial de la Federación (D.O.F.) el 22 de octubre de 1993, la cual ha cambiado de nomenclatura en dos ocasiones, la primera, por el Acuerdo Secretarial publicado en el D.O.F. el 29 de noviembre de 1994, siendo modificada a NOM-053-ECOL-1993 y, la segunda, por el Acuerdo emitido en el mismo órgano de difusión el 23 de abril de 2003, quedando con el nombre que aparece al inicio 
de esta cita.
	4.2 Official Mexican Standard NOM-053-SEMARNAT-1993, That establishes the procedure for carrying out the extraction test to determine the ingredients that make a waste hazardous for its toxicity to the environment, published in the Official Daily of the Federation on the 22nd of October of 1993, which has changed nomenclature on two occasions, the first, by the Secretarial Agreement published in the Official Daily of the Federation on the 29th  of November of 1994, being modified to NOM-053-ECOL-1993 and, the second, by Agreement issued in the same Official Daily of the Federation  on the 23rd of April of 2003, to remain with the name that appears at the beginning of this citation. 


	4.3 Norma Oficial Mexicana NOM-087-SEMARNAT-SSA1-2002, Protección ambiental-Salud ambiental-Residuos peligrosos biológico-infecciosos-Clasificación y especificaciones de manejo, publicada en el Diario Oficial de la Federación (D.O.F.) el 17 de febrero de 2003, la cual cambió de nomenclatura por el Acuerdo Secretarial publicado en el D.O.F. el 23 de abril de 2003, quedando con el nombre que aparece al inicio de esta cita.
	4.3 Official Mexican Standard NOM-087-SEMARNAT-SSA1-2002, Environmental Protection – Environmental Health – biological-infectious wastes – Classification and handling specifications, published in the Official Daily of the Federation on the 17th of February of 2003, which changed nomenclature by the Secretary Agreement published in the Official Daily of the Federation on the 23rd of April of 2003, to remain with the name that appears at the beginning of this citation. 


	4.4 Norma Oficial Mexicana NOM-133-SEMARNAT-2000, Protección Ambiental-Bifenilos Policlorados (BPC’s)-Especificaciones de manejo, publicada en el Diario Oficial de la Federación (D.O.F.) el 10 de diciembre de 2001, la cual cambió de nomenclatura por el Acuerdo Secretarial publicado en el D.O.F. el 23 de abril de 2003, quedando con el nombre que aparece al inicio de esta cita.
	4.4 Official Mexican Standard NOM-133-SEMARNAT-2000, Environmental Protection – Biphenyl Polychlorides (BPC’s) Handling specifications, published in the Official Daily of the Federation on the 10th of December of 2001, which changed nomenclature by the Secretarial Agreement published in the Official Daily of the Federation on the 23rd of April of 2003, to remain with the name that appears at the beginning of this citation. 

	4.5 Norma Oficial Mexicana NOM-138-SEMARNAT/SS-2003, Límites máximos permisibles de hidrocarburos en suelos y las especificaciones para su caracterización y remediación, publicada en el Diario Oficial de la Federación el 29 de marzo de 2005.
	4.5 Official Mexican Standard NOM-138-SEMARNAT/SS-2003, Maximum permissible limits of hydrocarbons in soil and the specifications for its characterization and remediation, published in the Official Daily of the Federation on the 29th of March of 2005. 


	4.6 Norma Oficial Mexicana NOM-141-SEMARNAT-2003, Que establece el procedimiento para caracterizar los jales, así como las especificaciones y criterios para la caracterización y preparación del sitio, proyecto, construcción, operación y postoperación de presas de jales, publicada en el Diario Oficial de la Federación el 13 de septiembre de 2004.
	4.6 Official Mexican Standard NOM-141-SEMARNAT-2003, That establishes the procedure for characterizing the tailings, as well as the specifications and criteria for the characterization, and preparation of the site, project, construction, operation, and post-operation of contained mine tailings, published in the Official Daily of the Federation on the 13th of September of 2004. 


	4.7 Norma Oficial Mexicana NOM-002-SCT/2003, Listado de las Substancias y Materiales Peligrosos más usualmente transportados, publicada en el Diario Oficial de la Federación el 3 de diciembre de 2003.
	4.7 Official Mexican Standard NOM-052-SCT/2003, List of the Hazardous Substances and Materials most usually transported, published in the Official Daily of the Federation on the 3rd of December of 2003. 


	5. Definiciones
	5 Definitions

	Para los efectos de esta Norma Oficial Mexicana se consideran las definiciones contenidas en la Ley General del Equilibrio Ecológico y la Protección al Ambiente, la Ley General para la Prevención y Gestión Integral de los Residuos y en los Reglamentos correspondientes y las siguientes:
	For the purposes of this Official Mexican Standard the definitions contained in the General Law of Ecological Equilibrium and Protection of the Environment, the General Law for the Prevention and Integral Management of Wastes and in the corresponding Regulations and the following are used: 


	5.1 Constituyente Tóxico.- Cualquier sustancia química contenida en un residuo y que hace que éste sea peligroso por su toxicidad, ya sea ambiental, aguda o crónica.


	5.1 Toxic ingredient – Any chemical substance contained in a waste that makes it dangerous by its toxicity, whether environmental, acute or chronic. 

	5.2 CRETIB.- El acrónimo de clasificación de las características a identificar en los residuos peligrosos y que significa: corrosivo, reactivo, explosivo, tóxico ambiental, inflamable y biológico-infeccioso.
	5.2 CRETIB. The acronym of the classification of the characteristics to identify in the hazardous wastes that stand for: Corrosivity, Reactivity, Explosivity, Environmental Toxicity, Flammability and Biological-infectious. 


	5.3 CRIT.- El acrónimo de clasificación de las características a identificar en los residuos peligrosos y que significa: corrosivo, reactivo, inflamable y tóxico ambiental.
	5.3 CRIT – The acronym of the classification of the characteristics to identify in the hazardous wastes that stand for: Corrosivity, Reactivity, Flammability and Environmental Toxicity.


	5.4 Extracto PECT.- El lixiviado a partir del cual se determinan los constituyentes tóxicos del residuo y su concentración con la finalidad de identificar si éste es peligroso por su toxicidad al ambiente.
	5.4 PECT Extract – The leached liquid from which is determined the toxic ingredients of the waste and its concentration for the purpose of identifying if it is hazardous for its toxicity to the environment. 


	5.5 Fuente específica.- Las actividades que generan residuos peligrosos y que están definidas por giro o proceso industrial.
	5.5 Specific source. The activities that generate hazardous wastes and that are defined y industrial classification or process. 


	5.6 Fuente no específica.- Las actividades que generan residuos peligrosos y que por llevarse a cabo en diferentes giros o procesos se clasifican de manera general.
	5.6 Non-specific source. – The activities that generate hazardous wastes and because they are carried out in different industries or processes are classified in a general way. 


	5.7 Ley.- La Ley General para la Prevención y Gestión Integral de los Residuos.
	5.7 Law – The General Law for the Prevention and Integral Management of Wastes. 


	5.8 PECT.- Procedimiento de Extracción de Constituyentes Tóxicos.


	5.8 PECT – Extraction Procedure of Toxic Ingredients. 

	5.9 Residuos peligrosos resultado del desecho de productos fuera de especificaciones o caducos.- Sustancias químicas que han perdido, carecen o presentan variación en las características necesarias para ser utilizados, transformados o comercializados respecto a los estándares de diseño o producción originales.


	5.9 Hazardous wastes resulting from the waste of products outside the specification or effective periods. Chemical substances that have gone bad, lack or present variation in the characteristics necessary for being utilized, manufactured, or marketed with respect to the original standards of design or production. 

	5.10 Reglamento.- El Reglamento de la Ley General para la Prevención y Gestión Integral de los Residuos.
	5.10 Regulation. The Regulation of the General Law for the Prevention and Integral Management of Wastes.


	5.11 Secretaría.- La Secretaría de Medio Ambiente y Recursos Naturales.
	5.11 Secretary. The Secretary of Environment and Natural Resources. 


	5.12 Toxicidad.- La propiedad de una sustancia o mezcla de sustancias de provocar efectos adversos en la salud o en los ecosistemas.
	5.12 Toxicity. The property of a substance or mixture of substances for provoking adverse effects on health or the ecosystems. 


	5.13 Toxicidad Ambiental.- La característica de una sustancia o mezcla de sustancias que ocasiona un desequilibrio ecológico.
	5.13 Environmental Toxicity. The characteristic of a substance or mixture of substances that cause an ecological imbalance. 


	5.14 Toxicidad Aguda.- El grado en el cual una sustancia o mezcla de sustancias puede provocar, en un corto periodo de tiempo o en una sola exposición, daños o la muerte de un organismo.
	5.14 Acute Toxicity. The degree in which a substance or mixture of substances can cause, in a short period of time or in one single exposure, damages or death to an organism. 


	5.15 Toxicidad Crónica.- Es la propiedad de una sustancia o mezcla de sustancias de causar efectos dañinos a largo plazo en los organismos, generalmente a partir de exposiciones continuas o repetidas y que son capaces de producir efectos cancerígenos, teratogénicos o mutagénicos.


	5.15 Chronic Toxicity. Is the property of a substance or mixture of substances for causing long term damaging effects in the organisms, generally from continuous or repeated exposures and that are capable of producing carcinogenic, teratogenic, or mutagenic effects. 

	6. Procedimiento para determinar si un residuo es peligroso


	6. Procedure for determining if a waste is hazardous. 

	6.1 El procedimiento para determinar si un residuo es peligroso se presenta en la Figura 1.
	6.1 The procedure for determining if a waste is hazardous is described in Figure 1. 


	6.2 Un residuo es peligroso si se encuentra en alguno de los siguientes listados:
	6.2 A waste is hazardous if it is found to be on any of the following lists: 


	Listado 1: Clasificación de residuos peligrosos por fuente específica.
	List 1: Classification of hazardous wastes by specific source. 


	Listado 2: Clasificación de residuos peligrosos por fuente no específica.
	List 2: Classification of hazardous waste by non-specific source. 


	Listado 3: Clasificación de residuos peligrosos resultado del desecho de productos químicos fuera de especificaciones o caducos (Tóxicos Agudos).
	List 3: Classification of hazardous wastes resulting from the waste of chemical products outside of specifications or effective periods. (Acute Toxic)


	Listado 4: Clasificación de residuos peligrosos resultado del desecho de productos químicos fuera de especificaciones o caducos (Tóxicos Crónicos).
	List 4: Classification of hazardous wastes resulting from the waste of chemical products outside of specifications or effective period. (Chronic Toxic).


	Listado 5: Clasificación por tipo de residuos, sujetos a Condiciones Particulares de Manejo.
	List 5: Classification by type of wastes, subject to Specific Conditions of Handling. 


	6.2.1 Las Toxicidades aguda y crónica referidas en los Listados 1, 2, 3 y 4 de esta Norma Oficial Mexicana no están contempladas en los análisis a realizar para la determinación de las características CRIT de peligrosidad en los residuos.
	6.2.1 The Toxicities, acute and chronic, referred to in Lists 1, 2, 3, and 4 of this Official Mexican Standard are not contained in the analysis to be made for the determination of the CRIT Characteristics of hazards in wastes. 


	6.2.2 El Anexo 1 de esta Norma Oficial Mexicana contiene las bases para listar residuos peligrosos por “Fuente Específica” y “Fuente No Específica”, en función de sus Toxicidades ambiental, aguda o crónica.
	6.2.2 The Appendix 1 of this Official Mexican Standard contains the criteria for listing hazardous wastes from a “Specific Source” and “Non-specific Source” depending on its environmental toxicity, acute or chronic. 


	6.3 Si el residuo no se encuentra en ninguno de los Listados 1 a 5 y es regulado por alguno de los criterios contemplados en los numerales 6.3.1 a 6.3.4 de esta norma, éste se sujetará a lo dispuesto en el Instrumento Regulatorio correspondiente.
	6.3 If the waste is not found to be on one of the Lists 1 through 5 and is regulated by some of the criteria covered in numbers 6.3.1 through 6.3.4 of this standard, it will be subject to the provision in the corresponding Regulatory Instrument. 


	6.3.1 Los lodos y biosólidos están regulados por la NOM-004-SEMARNAT-2002.
	6.3.1 The sludges and bio-solids are regulated by the NOM-004-SEMARNAT-2002. 


	6.3.2 Los bifenilos policlorados (BPC’s) están sujetos a las disposiciones establecidas en la 
NOM-133-SEMARNAT-2000.
	6.3.2 The biphenyl polychlorides (BPC’s) are subject to the provisions established in the NOM-133-SEMARNAT-2000. 


	6.3.3 Los límites máximos permisibles de hidrocarburos en suelos están sujetos a lo definido en la 
NOM-138-SEMARNAT/SS-2003.
	6.3.3 The maximum permissible limits of hydrocarbons in soils are subject to that defined in the NOM-138-SEMARNAT-SS-2003. 


	6.3.4 Los jales mineros se rigen bajo las especificaciones incluidas en la NOM-141-SEMARNAT-2003.


	6.3.4 The mine tailings are regulated under the specifications included in NOM-141-SEMARNAT-2003. 

	6.4 Si el residuo no está listado o no cumple con las particularidades establecidas en el inciso 6.3 se deberá definir si es que éste presenta alguna de las características de peligrosidad que se mencionan en el numeral 7 de esta Norma Oficial Mexicana. Esta determinación se llevará a cabo mediante alguna de las opciones que se mencionan a continuación:
	6.4 If the waste is not listed or does not comply with the details established in clause 6.3, it should be defined whether some of the characteristics of hazard are present that are mentioned in number 7 of this Official Mexican Standard. This determination will be carried out through one of the options that are mentioned in the following: 


	6.4.1 Caracterización o análisis CRIT de los residuos junto con la determinación de las características de Explosividad y Biológico-Infeccioso.
	6.4.1 CRIT characterization or analysis of the wastes together with the determination of the characteristics of Explosivity and Biological-infectious. 


	6.4.2 Manifestación basada en el conocimiento científico o la evidencia empírica sobre los materiales y procesos empleados en la generación del residuo en los siguientes casos:
	6.4.2 Statement based on scientific knowledge or empirical evidence on the materials and processes employed in the generation of the waste in the following cases: 


	6.4.2.1 Si el generador sabe que su residuo tiene alguna de las características de peligrosidad establecidas en esta norma.
	6.4.2.1 If the generator knows that its waste has any one of the characteristics of hazard established in this Standard. 


	6.4.2.2 Si el generador conoce que el residuo contiene un constituyente tóxico que lo hace peligroso.
	6.4.2.2 If the generator know that the waste contains a toxic ingredient that makes it hazardous. 


	6.4.2.3 Si el generador declara, bajo protesta de decir verdad, que su residuo no es peligroso.
	6.4.2.3 If the generator declares, under oath, that its waste is not hazardous. 


	7. Características que definen a un residuo como peligroso
	7. Characteristics that define a waste as hazardous. 


	7.1 El residuo es peligroso si presenta al menos una de las siguientes características, bajo las condiciones señaladas en los numerales 7.2 a 7.7 de esta Norma Oficial Mexicana:
	7.1 The waste is hazardous is it presents at least one of the following characteristics, under the conditions stipulated in numbers 7.2 through 7.7 of this Official Mexican Standard. 


	- Corrosividad
	- Corrosivity

	- Reactividad
	- Reactivity

	- Explosividad
	- Explosivity

	- Toxicidad Ambiental
	- Environmental Toxicity

	- Inflamabilidad
	- Flammability

	- Biológico-Infecciosa
	- Biological-Infectious 


	7.1.1 Las Toxicidades aguda y crónica quedan exceptuadas de los análisis a realizar para la determinación de la característica de Toxicidad Ambiental en los residuos establecida en el numeral 7.5 de esta Norma Oficial Mexicana.
	7.1.1 Acute and chronic toxicities are exempted from this analysis to be performed for the determination of the characteristic of Environmental Toxicity in the wastes established in number 7.5 of Official Mexican Standard. 


	7.2 Es Corrosivo cuando una muestra representativa presenta cualquiera de las siguientes propiedades:
	7.2 It is corrosive when a representative sample presents any of the following properties: 


	7.2.1 Es un líquido acuoso y presenta un pH menor o igual a 2,0 o mayor o igual a 12,5 de conformidad con el procedimiento que se establece en la Norma Mexicana correspondiente.
	7.2.1 It is an aqueous liquid and presents a pH lower or equal to 2.0 or greater or equal to 12.5 of conformity with the procedure that is established in the corresponding Mexican Standard. 


	7.2.2 Es un sólido que cuando se mezcla con agua destilada presenta un pH menor o igual a 2,0 o mayor o igual a 12,5 según el procedimiento que se establece en la Norma Mexicana correspondiente.
	7.2.2 It is a solid that when mixed with distilled water presents a pH lower or equal to 2.0 or greater or equal to 12.5 following the procedure that is established in the corresponding Mexican Standard. 


	7.2.3 Es un líquido no acuoso capaz de corroer el acero al carbón, tipo SAE 1020, a una velocidad de 6,35 milímetros o más por año a una temperatura de 328 K (55°C), según el procedimiento que se establece en la Norma Mexicana correspondiente.
	7.2.3 It is a non aqueous liquid capable of corroding steel to carbon, type SAE 1020, at a velocity of 6.35 millimeters or more per year at a temperature of 328 K (55°C) following the procedure that is established in the corresponding Mexican Standard. 


	7.3 Es Reactivo cuando una muestra representativa presenta cualquiera de las siguientes propiedades:
	7.3 It is reactive when a representative sample presents any of the following properties: 


	7.3.1 Es un líquido o sólido que después de ponerse en contacto con el aire se inflama en un tiempo menor a cinco minutos sin que exista una fuente externa de ignición, según el procedimiento que se establece en la Norma Mexicana correspondiente.


	7.3.1 It is a liquid or solid that after it makes contact with air it ignites in less than five minutes without an external source of ignition, following the procedure that is established in the corresponding Mexican Standard. 

	7.3.2 Cuando se pone en contacto con agua reacciona espontáneamente y genera gases inflamables en una cantidad mayor de 1 litro por kilogramo del residuo por hora, según el procedimiento que se establece en la Norma Mexicana correspondiente.
	7.3.2 When placed in contact with water, it reacts spontaneously and generates flammable gases in a quantity greater than 1 liter per kilogram of the waste per hour, according the procedure that is established in the corresponding Mexican Standard. 


	7.3.3 Es un residuo que en contacto con el aire y sin una fuente de energía suplementaria genera calor, según el procedimiento que se establece en la Norma Mexicana correspondiente.
	7.3.3 It is a waste that in contact with air and without a supplementary source of energy generates heat, following the procedure that is established in the corresponding Mexican Standard. 


	7.3.4 Posee en su constitución cianuros o sulfuros liberables, que cuando se expone a condiciones ácidas genera gases en cantidades mayores a 250 mg de ácido cianhídrico por kg de residuo o 500 mg de ácido sulfhídrico por kg de residuo, según el procedimiento que se establece en la Norma Mexicana correspondiente.


	7.3.4 Contained in its ingredients are free cyanides or sulfides that when exposed to acid conditions generate gases in quantities greater than 250 mg of hydrogen cyanide per kg of waste or 500 mg of sulfuric acid per kg of waste following the procedure that is established in the corresponding Mexican Standard. 

	7.4 Es Explosivo cuando es capaz de producir una reacción o descomposición detonante o explosiva solo o en presencia de una fuente de energía o si es calentado bajo confinamiento. Esta característica no debe determinarse mediante análisis de laboratorio, por lo que la identificación de esta característica debe estar basada en el conocimiento del origen o composición del residuo.


	7.4 It is explosive when it is capable of producing a detonating or explosive reaction or decomposition only or in presence of a source of energy or if it is heated under confinement. This characteristic must not be determined through laboratory analysis, because the identification of this characteristic must be based on the knowledge of the origin or composition of the waste. 

	7.5 Es Tóxico Ambiental cuando:
	7.5 It is environmentally toxic when: 

	7.5.1 El extracto PECT, obtenido mediante el procedimiento establecido en la NOM-053-SEMARNAT-1993, contiene cualquiera de los constituyentes tóxicos listados en la Tabla 2 de esta Norma en una concentración mayor a los límites ahí señalados, la cual deberá obtenerse según los procedimientos que se establecen en las Normas Mexicanas correspondientes.
	7.5.1 The EP Toxicity extract, obtained through the procedure established in the NOM-053-SEMARNAT-1993, contains any of the toxic components listed in Table 2 of this Standard in a concentration greater than the limits so stipulated, which must be obtained following the procedures that are established in the corresponding Mexican standards. 


	7.6 Es Inflamable cuando una muestra representativa presenta cualquiera de las siguientes propiedades:
	7.6 It is flammable when a representative sample presents any of the following properties:
 

	7.6.1 Es un líquido o una mezcla de líquidos que contienen sólidos en solución o suspensión que tiene un punto de inflamación inferior a 60,5°C, medido en copa cerrada, de conformidad con el procedimiento que se establece en la Norma Mexicana correspondiente, quedando excluidas las soluciones acuosas que contengan un porcentaje de alcohol, en volumen, menor a 24%.


	7.6.1 It is a liquid or mixture of liquids that contain solids in solution or suspension that has a flash point lower than 60.5ºC, measured in a closed cup in conformity to the procedure that is established in the corresponding Mexican Standard, the aqueous solutions that contain a percentage of alcohol, in volume, less than 27% are excluded. 

	7.6.2 No es líquido y es capaz de provocar fuego por fricción, absorción de humedad o cambios químicos espontáneos a 25°C, según el procedimiento que se establece en la Norma Mexicana correspondiente.
	7.6.2 It is not a liquid and is capable of causing fire by friction, absorption of humidity or spontaneous chemical changes at 25ºC, following the procedure that is established in the corresponding Mexican Standard. 


	7.6.3 Es un gas que, a 20°C y una presión de 101,3 kPa, arde cuando se encuentra en una mezcla del 13% o menos por volumen de aire, o tiene un rango de inflamabilidad con aire de cuando menos 12% sin importar el límite inferior de inflamabilidad.
	7.6.3 It is a gas that at 20ºC and at a pressure of 101.3 kPa burns when it is in a mixture of 13% or less per volume of air, or has a range of flammability with air when of at least 12%; it does not matter what the lower limit of flammability. 


	7.6.4 Es un gas oxidante que puede causar o contribuir más que el aire, a la combustión de otro material.
	7.6.4 It is an oxidizing gas that can cause or contribute more than air, to the combustion of another material. 


	7.7 Es Biológico-Infeccioso de conformidad con lo que se establece en la NOM-087-SEMARNAT-SSA1-2002, referida en el punto 4 de esta Norma.
	7.7. It is Biological-Infectious in conformity to that established in NOM-087-SEMARNAT-SSA1-2002, referred to in point 4 of this Standard. 


	8. Procedimiento para la evaluación de la conformidad


	8. Procedure for the evaluation of the conformity. 

	8.1 Las muestras para determinaciones analíticas deben ser tomadas directamente a la salida del proceso o del área de almacenamiento en su caso, de conformidad con los procedimientos establecidos en la Norma Mexicana correspondiente y deberán ser representativas del volumen generado, considerando las variaciones en el proceso y, además, se debe establecer la cadena de custodia para las mismas.
	8.1 The samples for the analytical determinations must be taken directly at the end of the process or from the storage area when applicable, in conformity to the procedures established in the corresponding Mexican Standard and must be representative of the volume generate, considering the variations in the process and, additionally, the chain of custody for the same must be established. 


	8.2 La Secretaría reconocerá las determinaciones analíticas de la prueba CRIT que hayan sido muestreadas y analizadas por un laboratorio acreditado y aprobado conforme a las disposiciones legales aplicables.
	8.2 The Secretary will recognize the analytical determinations of the CRIT (Corrosivity, Reactivity, Flammability and Environmental Toxicity) test that have been sampled and analyzed by an accredited and approved laboratory in conformity to the applicable legal provisions. 


	9. Grado de concordancia con normas y lineamientos internacionales y con las normas mexicanas tomadas como base para su elaboración
	9. Degree of concordance with international standards and guidelines and with the Mexican standards taken as criteria for its creation. 


	Esta Norma Oficial Mexicana no concuerda con ninguna norma internacional ni norma mexicana.
	This Official Mexican Standard does not concord with any international or Mexican Standard. 
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de mayo de 1997.
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	10.3 Code of Federal Regulations, Vol. 40 Part. 261. 1999. U.S.A. (Código de Regulaciones Federales, Vol. 40, Parte 261, 1999, Estados Unidos de América).
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	10.4 Registro Internacional de Sustancias Químicas Potencialmente Tóxicas, Ginebra, Suiza, 1982.
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	11. Vigilancia de esta Norma
	11. Oversight of this Standard


	La vigilancia del cumplimiento de la presente Norma Oficial Mexicana corresponde a la Secretaría de Medio Ambiente y Recursos Naturales, por conducto de la Procuraduría Federal de Protección al Ambiente, cuyo personal realizará los trabajos de inspección y vigilancia que sean necesarios. Las violaciones a la misma se sancionarán en los términos de la Ley General del Equilibrio Ecológico y la Protección al Ambiente, la Ley General para la Prevención y Gestión Integral de los Residuos, sus Reglamentos y demás ordenamientos jurídicos aplicables.
	The oversight to the compliance of this Official Mexican Standard is the responsibility to the Secretary of Environment and Natural Resources through the office of the Federal Prosecutor of Protection of the Environment, whose personnel will perform the work of inspection and oversight that are necessary. The violations to the same will be sanctioned under the terms of the General Law of Ecological Equilibrium and Protection of the Environment, the General Law for the Prevention and Integral Management of the Wastes, its Regulations and all other applicable legal ordinances. 


	TRANSITORIOS
	TRANSITIONAL ARTICLES

	PRIMERO.- La presente Norma Oficial Mexicana entrará en vigor a los noventa días naturales siguientes de su publicación en el Diario Oficial de la Federación.
	FIRST. This Official Mexican Standard will become effective on the ninety calendar days following its publication in the Official Daily of the Federation. 


	SEGUNDO.- A la entrada en vigor de esta Norma Oficial Mexicana se abroga la Norma Oficial Mexicana NOM-052-SEMARNAT-1993, Que establece las características de los residuos peligrosos, el listado de los mismos y los límites que hacen a un residuo peligroso por su toxicidad al ambiente, publicada en el Diario Oficial de la Federación (D.O.F.) el 22 de octubre de 1993.
	SECOND. When this Official Mexican Standard becomes effective it cancels the Official Mexican Standard NOM-052-SEMARNAT-1993, That establishes the characteristics of hazardous wastes, the list of the same and the limits that make it a hazardous waste for its toxicity to the environment, published in the Official Daily of the Federation on the 22nd of October of 1993.
 

	TERCERO.- Las Constancias de No Peligrosidad que estén vigentes a la entrada en vigor de esta Norma Oficial Mexicana tendrán validez hasta el plazo por el cual fueron emitidas.


	THIRD. The Certificates of No Hazards that are current on the effective date of this Official Mexican Standard will remain valid for the term they were issued. 

	Provéase la publicación de esta Norma Oficial Mexicana en el Diario Oficial de la Federación.
	Review the publication of this Official Mexican Standard in the Official Daily of the Federation.


	México, Distrito Federal, al segundo día del mes de junio de dos mil seis.- El Subsecretario de Fomento y Normatividad Ambiental de la Secretaría de Medio Ambiente y Recursos Naturales y Presidente del 
Comité Consultivo Nacional de Normalización de Medio Ambiente y Recursos Naturales, José Ramón Ardavín Ituarte.- Rúbrica.
	Mexico, Federal District, on the second day of the month of June of 2006. The Sub-Secretary of Environmental Development and Legislation of the Secretary of Environment and Natural Resources and President of the National Consultative Committee of Standardization of Environment and Natural Resources, Jose Ramon Ardavin Ituarte. Signed. 


	TABLA 1



	CODIGOS DE PELIGROSIDAD DE LOS RESIDUOS (CPR)



	Características
	Código de Peligrosidad de los Residuos (CPR)

	Corrosividad
	C

	Reactividad
	R

	Explosividad
	E

	Toxicidad

Ambiental

Aguda

Crónica
	T

	
	
Te


Th


Tt

	Inflamabilidad 
	I

	Biológico-Infeccioso 
	B

	H
	

	Cuando se trate de una mezcla de residuos peligrosos de los Listados 3 y 4 se identificarán con la característica del residuo de mayor volumen, agregándole al CPR la letra “M”.




	TABLE 1



	WASTE HAZARD CODE (WHC)



	Characteristics
	Waste Hazard Code (WHC)

	Corrosivity
	C

	Reactivity 
	R

	Explosivity 
	E

	Acute chronic Environmental Toxicity 
	T

	
	Te

Th

Tt

	Flammability
	I

	Biological-Infectious
	B

	H
	

	When dealing with a mixture of hazardous wastes of Lists 3 and 4, they will be identified with the characteristic of the waste of greater volume, adding the letter “M” to the acronym. 




	TABLA 2

	LIMITES MAXIMOS PERMISIBLES PARA LOS CONSTITUYENTES TOXICOS EN EL EXTRACTO PECT

	CAS1
	Contaminante
	LMP2 (mg/L)

	
	

	CONSTITUYENTES INORGANICOS (METALES)

	7440-38-2
	Arsénico
	5.0

	7440-39-3
	Bario
	100.0

	7440-43-9
	Cadmio
	1.0

	7440-47-3
	Cromo 
	5.0

	7439-97-6
	Mercurio
	0.2

	7440-22-4
	Plata 
	5.0

	7439-92-1
	Plomo
	5.0

	7782-49-2
	Selenio
	1.0

	CONSTITUYENTES ORGANICOS SEMIVOLATILES
	

	94-75-7
	Acido 2,4-Diclorofenoxiacético (2,4-D)
	10.0

	93-72-1
	Acido 2,4,5-Triclorofenoxipropiónico (Silvex)
	1.0

	57-74-9
	Clordano
	0.03

	95-48-7
	o-Cresol 
	200.0

	108-39-4
	m-Cresol 
	200.0

	106-44-5
	p-Cresol 
	200.0

	1319-77-3
	Cresol 
	200.0

	121-14-2
	2,4-Dinitrotolueno
	0.13

	72-20-8
	Endrin
	0.02

	76-44-8
	Heptacloro (y su Epóxido)
	0.008

	67-72-1
	Hexacloroetano
	3.0

	58-89-9
	Lindano
	0.4

	74-43-5
	Metoxicloro
	10.0

	98-95-3
	Nitrobenceno
	2.0

	87-86-5
	Pentaclorofenol
	100.0

	8001-35-2
	Toxafeno
	0.5

	95-95-4
	2,4,5-Triclorofenol
	400.0

	88-06-2
	2,4,6-Triclorofenol
	2.0

	CONSTITUYENTES ORGANICOS VOLATILES
	

	71-43-2
	Benceno
	0.5

	108-90-7
	Clorobenceno
	100.0

	67-66-3
	Cloroformo
	6.0

	75-01-4
	Cloruro de Vinilo
	0.2

	106-46-7
	1,4-Diclorobenceno
	7.5

	107-06-2
	1,2-Dicloroetano
	0.5

	75-35-4
	1,1-Dicloroetileno
	0.7

	118-74-1
	Hexaclorobenceno
	0.13

	87-68-3
	Hexaclorobutadieno
	0.5

	78-93-3
	Metil etil cetona
	200.0

	110-86-1
	Piridina
	5.0

	127-18-4
	Tetracloroetileno
	0.7

	56-23-5
	Tetracloruro de Carbono
	0.5

	79-01-6
	Tricloroetileno
	0.5

	1 No. CAS: Número del Chemical Abstracts Service (Servicio de Resúmenes Químicos)



	2 LMP: Límite Máximo Permisible




	TABLE 2

	MAXIMUM PERMISSIBLE LIMITS FOR THE TOXIC COMPONENTS IN THE PECT EXTRACT



	CAS1
	Contaminant
	MPL2 (mg/L)

	
	

	INORGANIC COMPONENTS (METALS)

	7440-38-2
	Arsenic
	5.0

	7440-39-3
	Barium
	100.0

	7440-43-9
	Cadmium
	1.0

	7440-47-3
	Chrome
	5.0

	7439-97-6
	Mercury
	0.2

	7440-22-4
	Silver
	5.0

	7439-92-1
	Lead
	5.0

	7782-49-2
	Selenium
	1.0

	SEMI-VOLATILE ORGANIC COMPONENTS
	

	94-75-7
	2,4-Dichlorophenoxyacetic (2,4-D) Acid
	10.0

	93-72-1
	2,4,5-Trichlorophenoxypropionic (Silvex) Acid
	1.0

	57-74-9
	chlordane
	0.03

	95-48-7
	o-Creosol e
	200.0

	108-39-4
	m-Creosol 
	200.0

	106-44-5
	p-Creosol 
	200.0

	1319-77-3
	Creosol 
	200.0

	121-14-2
	2,4-Dinitro-toluene
	0.13

	72-20-8
	Endrine
	0.02

	76-44-8
	Heptachlorine (and its Epoxide)
	0.008

	67-72-1
	Hexachloroethane
	3.0

	58-89-9
	Lindane
	0.4

	74-43-5
	Metoxichlorine
	10.0

	98-95-3
	Nitrobenzene
	2.0

	87-86-5
	Pentachlorophenol
	100.0

	8001-35-2
	Toxaphene
	0.5

	95-95-4
	2,4,5-Trichlorophenol
	400.0

	88-06-2
	2,4,6- Trichlorophenol
	2.0

	VOLATILE ORGANIC COMPONENTS
	

	71-43-2
	Benzene
	0.5

	108-90-7
	Chlorobenzene
	100.0

	67-66-3
	Chloroform
	6.0

	75-01-4
	Vinyl chloride
	0.2

	106-46-7
	1,4-Dichlorobenzene
	7.5

	107-06-2
	1,2-Dichloroethanol
	0.5

	75-35-4
	1,1-Dichloroethylene
	0.7

	118-74-1
	Hexachlorobenzene
	0.13

	87-68-3
	Hexachlorobutadiene
	0.5

	78-93-3
	Methyl Ethyl Ketone
	200.0

	110-86-1
	Piridine
	5.0

	127-18-4
	Tetrachloroethylene
	0.7

	56-23-5
	Carbon tetrachloride
	0.5

	79-01-6
	Trichlorethylene
	0.5

	1 CAS: Chemical Abstracts Service Number  (Chemical Service Reports)



	2 MPL: Maximum Permissible Limit




	LISTADO 1



	CLASIFICACION DE RESIDUOS PELIGROSOS POR FUENTE ESPECIFICA



	Residuo
	CPR
	Clave

	GIRO 1: BENEFICIO DE METALES

	CUBAS ELECTROLITICAS GASTADAS DE LA REDUCCION PRIMARIA DE ALUMINIO
	(Tt)
	E1/01

	LICOR GASTADO GENERADO POR LAS OPERACIONES DE ACABADO DEL ACERO EN INSTALACIONES PERTENECIENTES A LA INDUSTRIA DEL HIERRO Y DEL ACERO
	(C,Tt)
	E1/02

	LODOS Y POLVOS DEL EQUIPO DE CONTROL DE EMISIONES DE FUNDICION Y AFINADO EN LA PRODUCCION SECUNDARIA DE PLOMO
	(Tt)
	E1/03

	SOLUCION GASTADA PROVENIENTE DE LA LIXIVIACION ACIDA DE LOS LODOS/POLVOS DEL EQUIPO DE CONTROL DE EMISIONES EN LA FUNDICION SECUNDARIA DE PLOMO
	(Tt)
	E1/04

	GIRO 2: PRODUCCION DE COQUE

	RESIDUOS QUE NO SE REINTEGREN AL PROCESO DE LA PRODUCCION DE COQUE Y QUE NO PUEDAN SER REUTILIZADOS
	(Tt)
	E2/01

	GIRO 3: EXPLOSIVOS

	CARBON AGOTADO DEL TRATAMIENTO DE AGUAS RESIDUALES QUE CONTIENEN EXPLOSIVOS
	(R,E)
	E3/01

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES EN LA FABRICACION, FORMULACION Y CARGA DE LOS COMPUESTOS INICIADORES BASE PLOMO
	(Tt)
	E3/02

	RESIDUOS DE AGUA ROSA-ROJA Y DE ACIDOS GASTADOS DE LA MANUFACTURA 
DE TNT
	(R,E)
	E3/03

	GIRO 4: PETROLEO, GAS Y PETROQUIMICA

	CATALIZADORES GASTADOS DEL PROCESO DE “HIDROCRACKING” CATALITICO DE RESIDUALES EN LA REFINACION DE PETROLEO 
	(I,Tt)
	E4/01

	LODOS DE LA SEPARACION PRIMARIA DE ACEITE/AGUA/SÓLIDOS DE LA REFINACION DEL PETROLEO-CUALQUIER LODO GENERADO POR SEPARACION GRAVITACIONAL DE ACEITE/AGUA/SOLIDOS DURANTE EL ALMACENAMIENTO O TRATAMIENTO DE AGUAS RESIDUALES DE PROCESO Y AGUAS RESIDUALES ACEITOSAS DE ENFRIAMIENTO, DE REFINERIAS DE PETROLEO. TALES LODOS INCLUYEN, PERO NO SE LIMITAN, A AQUELLOS GENERADOS EN SEPARADORES DE ACEITE/AGUA/SOLIDOS; TANQUES Y LAGUNAS DE CAPTACION; ZANJAS Y OTROS DISPOSITIVOS DE TRANSPORTE DE AGUA PLUVIAL, LODOS GENERADOS DE AGUAS DE ENFRIAMIENTO SIN CONTACTO, DE UN SOLO PASO, SEGREGADAS PARA TRATAMIENTO DE OTROS PROCESOS O AGUAS DE ENFRIAMIENTO ACEITOSAS Y LODOS GENERADOS EN UNIDADES DE TRATAMIENTOS BIOLOGICOS
	(Tt)
	E4/02

	LODOS DE SEPARACION SECUNDARIA (EMULSIFICADOS) DE ACEITE/AGUA/SÓLIDOS. CUALQUIER LODO Y/O NATA GENERADO EN LA SEPARACION FISICA Y/O QUIMICA DE ACEITE/AGUA/SOLIDOS DE AGUAS RESIDUALES DE PROCESO Y AGUAS RESIDUALES ACEITOSAS DE ENFRIAMIENTO DE LAS REFINERIAS DE PETROLEO. TALES RESIDUOS INCLUYEN, PERO NO SE LIMITAN A, TODOS LOS LODOS Y LAS NATAS GENERADAS EN: UNIDADES DE FLOTACION DE AIRE INDUCIDA, TANQUES Y LAGUNAS DE CAPTACION Y TODOS LOS LODOS GENERADOS EN UNIDADES DAF (FLOTACION CON AIRE DISUELTO). LODOS GENERADOS DE AGUAS DE ENFRIAMIENTO SIN CONTACTO, DE UN SOLO PASO, SEGREGADAS PARA TRATAMIENTO DE OTROS PROCESOS O AGUAS DE ENFRIAMIENTO ACEITOSAS, LODOS Y NATAS GENERADOS EN UNIDADES DE TRATAMIENTOS BIOLOGICOS
	(Tt)
	E4/03

	LODOS DEL SEPARADOR API Y CARCAMOS EN LA REFINACION DE PETROLEO Y ALMACENAMIENTO DE PRODUCTOS DERIVADOS
	(Tt)
	E4/04

	LODOS DE TANQUES DE ALMACENAMIENTO DE HIDROCARBUROS
	(Tt)
	E4/05

	LODOS DE LA LIMPIEZA DE LOS HACES DE TUBOS DE LOS INTERCAMBIADORES DE CALOR, LADO HIDROCARBURO
	(Tt)
	E4/06

	NATAS DEL SISTEMA DE FLOTACION CON AIRE DISUELTO (FAD) EN LA REFINACION DE PETROLEO Y ALMACENAMIENTO DE PRODUCTOS DERIVADOS
	(Tt)
	E4/07

	SOLIDOS DE EMULSION DE ACEITES DE BAJA CALIDAD EN LA INDUSTRIA DE REFINACION DE PETROLEO
	(Tt)
	E4/08

	FONDOS DE LA ETAPA DE DESTILACION EN LA PRODUCCION DE ACETALDEHIDO VIA OXIDACION DE ETILENO
	(C,Tt,I)
	E4/09

	CORTES LATERALES DE LA ETAPA DE DESTILACION EN LA PRODUCCION DE ACETALDEHIDO VIA OXIDACION DE ETILENO
	(C,Tt,I)
	E4/10

	RESIDUOS DE PROCESOS, INCLUYENDO PERO NO LIMITADO A RESIDUOS DE DESTILACION, FONDOS PESADOS, BREAS Y RESIDUOS DE LA LIMPIEZA DE REACTORES DE LA PRODUCCION DE HIDROCARBUROS ALIFATICOS CLORADOS POR PROCESOS DE CATALIZACION DE RADICALES LIBRES QUE TIENEN CADENAS DE HASTA 5 (CINCO) CARBONES CON DIVERSAS CANTIDADES Y POSICIONES DE SUSTITUCION DE CLORO
	(Tt)
	E4/11

	GIRO 5: PINTURAS Y PRODUCTOS RELACIONADOS

	RESIDUOS DE PIGMENTOS BASE CROMO Y BASE PLOMO
	(Tt)
	E5/01

	GIRO 6: PLAGUICIDAS Y HERBICIDAS

	LODOS DE LAS PLANTAS DE TRATAMIENTO DE AGUAS RESIDUALES EN LA PRODUCCION DE CARBAMATOS, HERBICIDAS CLORADOS; PLAGUICIDAS ORGANO-HALOGENADOS; ORGANO-ARSENICALES; ORGANO-METALICOS Y ORGANO-FOSFORADOS
	(Tt)
	E6/01

	RESIDUOS DE LA PRODUCCION DE CARBAMATOS, HERBICIDAS CLORADOS; PLAGUICIDAS ORGANO-HALOGENADOS; ORGANO-ARSENICALES; ORGANO-METALICOS Y ORGANO-FOSFORADOS
	(Tt)
	E6/02

	GIRO 7: PRESERVACION DE LA MADERA

	LODOS SEDIMENTADOS Y SOLUCIONES GASTADAS GENERADOS EN LOS PROCESOS DE PRESERVACION DE LA MADERA 
	(Tt)
	E7/01

	GIRO 8: QUIMICA FARMACEUTICA

	CARBON ACTIVADO GASTADO EN LA PRODUCCION DE FARMACEUTICOS VETERINARIOS DE COMPUESTOS CON ARSENICO Y ORGANO-ARSENICALES
	(Tt)
	E8/01

	RESIDUOS DE BREAS DE LA DESTILACION DE COMPUESTOS A BASE DE ANILINA EN LA PRODUCCION DE PRODUCTOS VETERINARIOS DE COMPUESTOS DE ARSENICO Y ORGANO-ARSENICALES
	(Tt)
	E8/02

	GIRO 9: QUIMICA INORGANICA

	FILTROS DE LAS CASAS DE BOLSAS EN LA PRODUCCION DE OXIDO DE ANTIMONIO, INCLUYENDO LOS FILTROS EN LA PRODUCCION DE PRODUCTOS INTERMEDIOS (ANTIMONIO METALICO Y OXIDO DE ANTIMONIO CRUDO)
	(Te)
	E9/01

	ESCORIAS DE LA PRODUCCION DE OXIDO DE ANTIMONIO, INCLUYENDO AQUELLAS DE LOS PRODUCTOS INTERMEDIOS (ANTIMONIO METALICO Y OXIDO DE ANTIMONIO CRUDO)
	(Tt)
	E9/02

	LODOS DE LA PURIFICACION DE SALMUERA, DONDE LA SALMUERA PURIFICADA SEPARADA NO SE UTILIZA, EN LA PRODUCCION DE CLORO (PROCESO DE CELDAS DE MERCURIO)
	(Tt)
	E9/03

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES EN LA PRODUCCION DE CLORO (PROCESO DE CELDAS DE MERCURIO)
	(Tt)
	E9/04

	RESIDUOS DE HIDROCARBUROS CLORADOS DE LA ETAPA DE PURIFICACION EN LA PRODUCCION DE CLORO (PROCESO DE CELDAS DE DIAFRAGMA USANDO ANODOS DE GRAFITO)
	(Tt)
	E9/05

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE PIGMENTOS NARANJA Y AMARILLO DE CROMO
	(Tt)
	E9/06

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE PIGMENTOS VERDES DE CROMO
	(Tt)
	E9/07

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE PIGMENTOS VERDES DE OXIDO DE CROMO (ANHIDROS E HIDRATADOS)
	(Tt)
	E9/08

	RESIDUOS DEL HORNO DE LA PRODUCCION DE PIGMENTOS VERDES DE OXIDO DE CROMO
	(Tt)
	E9/09

	LODOS DE TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE PIGMENTOS AZULES DE HIERRO
	(Tt)
	E9/10

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE PIGMENTOS NARANJA DE MOLIBDATO
	(Tt)
	E9/11

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE PIGMENTOS AMARILLOS DE ZINC
	(Tt)
	E9/12

	RESIDUOS DE LA MANUFACTURA Y DEL ALMACENAMIENTO EN PLANTA DE CLORURO FERRICO DERIVADO DE ACIDOS FORMADOS DURANTE LA PRODUCCION DE BIOXIDO DE TITANIO MEDIANTE EL PROCESO CLORURO-ILMENITA
	(Tt)
	E9/13

	GIRO 10: QUIMICA ORGANICA

	LODOS DE LAS DESCARGAS DE AGUAS RESIDUALES EN LA PRODUCCION DE ACRILONITRILO 
	(R, Tt)
	E10/01

	FONDOS DE LA COLUMNA DE ACETONITRILO EN LA PRODUCCION DE ACRILONITRILO
	(R, Tt)
	E10/02

	FONDOS DE LA COLUMNA DE PURIFICACION DE ACETONITRILO EN LA PRODUCCION DE ACRILONITRILO
	(Tt)
	E10/03

	DOMOS LIGEROS DE LA DESTILACION INICIAL EN LA PRODUCCION DE ANHIDRIDO FTALICO A PARTIR DE NAFTALENO
	(Tt)
	E10/04

	FONDOS DE LA DESTILACION FINAL EN LA PRODUCCION DE ANHIDRIDO FTALICO A PARTIR DE NAFTALENO
	(Tt)
	E10/05

	DOMOS LIGEROS DE LA DESTILACION INICIAL EN LA PRODUCCION DE ANHIDRIDO FTALICO A PARTIR DE ORTO-XILENO
	(Tt)
	E10/06

	FONDOS DE LA DESTILACION FINAL EN LA PRODUCCION DE ANHIDRIDO FTALICO A PARTIR DE ORTO-XILENO
	(Tt)
	E10/07

	FONDOS DE LA DESTILACION EN LA PRODUCCION DE ANILINA
	(Tt)
	E10/08

	RESIDUOS DEL PROCESO DE EXTRACCION DE ANILINA
	(Tt)
	E10/09

	RESIDUOS PROVENIENTES DEL LAVADO DE GASES, DE CONDENSACION, DE DEPURACION Y SEPARACION EN LA PRODUCCION DE CARBAMATOS Y CARBOMIL OXIMAS
	(Tt)
	E10/10

	MATERIALES ORGANICOS DEL TRATAMIENTO DE RESIDUOS DE TIOCARBAMATO EN LA PRODUCCION DE CARBAMATOS Y CARBOMIL OXIMAS
	(Tt)
	E10/11

	POLVOS DE CASAS DE BOLSAS Y SÓLIDOS DE FILTRADO/SEPARACION DE LA PRODUCCION DE CARBAMATOS Y CARBOMIL OXIMAS
	(Tt)
	E10/12

	RESIDUOS ORGANICOS (INCLUYENDO FONDOS PESADOS, ESTANCADOS, FONDOS LIGEROS, SOLVENTES GASTADOS, RESIDUOS DE LA FILTRACION Y LA DECANTACION) DE LA PRODUCCION DE CARBAMATOS Y CARBOMIL OXIMAS
	(Tt)
	E10/13

	SOLIDOS DE PURIFICACION (INCLUYENDO SOLIDOS DE FILTRACION, EVAPORACION Y CENTRIFUGACION), POLVOS DE CASAS DE BOLSAS Y DE BARRIDO DE PISOS EN LA PRODUCCION DE ACIDOS DE TIOCARBAMATOS Y SUS SALES EN LA PRODUCCION DE CARBAMATOS Y CARBOMIL OXIMAS
	(R,Tt)
	E10/14

	FONDOS DE LA COLUMNA DE DESTILACION O FRACCIONAMIENTO EN LA PRODUCCION DE CLOROBENCENOS
	(Tt)
	E10/15

	CORRIENTES SEPARADAS DEL AGUA DEL REACTOR DE LAVADO DE CLOROBENCENOS
	(Tt)
	E10/16

	FONDOS DE LA ETAPA DE DESTILACION EN LA PRODUCCION DE CLORURO DE BENCILO
	(Tt)
	E10/17

	FONDOS PESADOS DE LA COLUMNA DE FRACCIONAMIENTO EN LA PRODUCCION DE CLORURO DE ETILO
	(Tt)
	E10/18

	FONDOS PESADOS DE LA DESTILACION DE CLORURO DE VINILO EN LA PRODUCCION DE MONOMERO DE CLORURO DE VINILO
	(Tt)
	E10/19

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE DICLORURO DE ETILENO O DE MONOMERO DE CLORURO DE VINILO 
	(Tt)
	E10/20

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES DE LA PRODUCCION DE MONOMERO DE CLORURO DE VINILO EN LA QUE SE UTILICE CLORURO DE MERCURIO COMO CATALIZADOR EN UN PROCESO BASE ACETILENO 
	(Tt)
	E10/21

	RESIDUOS DEL LAVADOR DE GASES DE VENTEO DEL REACTOR EN LA PRODUCCION DE DIBROMURO DE ETILENO VIA BROMACION DEL ETILENO
	(Tt)
	E10/22

	SÓLIDOS ADSORBENTES GASTADOS DE LA ETAPA DE PURIFICACION DEL DIBROMURO DE ETILENO OBTENIDO A PARTIR DE LA BROMACION DEL ETILENO
	(Tt)
	E10/23

	FONDOS DE LA ETAPA DE PURIFICACION DEL DIBROMURO DE ETILENO OBTENIDO A PARTIR DE LA BROMACION DEL ETILENO
	(Tt)
	E10/24

	CONDENSADOS ORGANICOS DE LA COLUMNA DE RECUPERACION DE SOLVENTES EN LA PRODUCCION DE DIISOCIANATO DE TOLUENO VIA FOSGENACION DE LA TOLUENDIAMINA
	(Tt)
	E10/25

	RESIDUOS DE CENTRIFUGACION Y DESTILACION EN LA PRODUCCION DE DIISOCIANATO DE TOLUENO VIA FOSGENACION DE LA TOLUENDIAMINA
	(R,Tt)
	E10/26

	FONDOS DE LA TORRE DE SEPARACION DE PRODUCTOS EN LA PRODUCCION 
DE 1,1-DIMETIL HIDRACINA A PARTIR DE HIDRACINAS DE ACIDO CARBOXILICO
	(C,Tt)
	E10/27

	CABEZAS CONDENSADAS DE LA COLUMNA DE SEPARACION DE PRODUCTOS Y GASES CONDENSADOS DEL VENTEO DEL REACTOR EN LA PRODUCCION DE 1,1-DIMETIL HIDRACINA A PARTIR DE HIDRACINAS DE ACIDO CARBOXILICO
	(Tt,I)
	E10/28

	CARTUCHOS DE LOS FILTROS AGOTADOS DE LA PURIFICACION DE LA 1,1-DIMETIL HIDRACINA OBTENIDA A PARTIR DE HIDRACINAS DE ACIDO CARBOXILICO
	(Tt)
	E10/29

	CABEZAS CONDENSADAS DE LA COLUMNA DE SEPARACION DE INTERMEDIOS EN LA PRODUCCION DE 1,1-DIMETIL HIDRACINA A PARTIR DE HIDRACINAS DE ACIDO CARBOXILICO
	(Tt)
	E10/30

	RESIDUOS PROVENIENTES DEL LAVADO DE DINITROTOLUENO OBTENIDO A PARTIR DE LA NITRACION DE TOLUENO
	(C,Tt)
	E10/31

	FONDOS PESADOS DE LA COLUMNA DE PURIFICACION DE LA EPICLORHIDRINA
	(Tt)
	E10/32

	FONDOS PESADOS (BREA) DE LA ETAPA DE DESTILACION EN LA PRODUCCION DE FENOL/ACETONA A PARTIR DEL CUMENO
	(Tt)
	E10/33

	RESIDUO DE CATALIZADOR AGOTADO DE ANTIMONIO EN SOLUCION ACUOSA EN LA PRODUCCION DE FLUOROMETANOS
	(Tt)
	E10/34

	COLAS DE LAS DESCARGAS EN LA PRODUCCION DE METIL ETIL PIRIDINAS
	(Tt)
	E10/35

	CORRIENTES COMBINADAS DE AGUAS RESIDUALES EN LA PRODUCCION DE NITROBENCENO/ANILINA
	(Tt)
	E10/36

	FONDOS DE LA DESTILACION EN LA PRODUCCION DE NITROBENCENO MEDIANTE LA NITRACION DEL BENCENO
	(Tt)
	E10/37

	FONDOS PESADOS O PRODUCTOS RESIDUALES DE LA ETAPA DE DESTILACION EN LA PRODUCCION DE TETRACLORURO DE CARBONO
	(Tt)
	E10/38

	AGUA DE REACCION (SUBPRODUCTO) DE LA COLUMNA DE SECADO EN LA PRODUCCION DE TOLUENDIAMINA VIA HIDROGENACION DE DINITROTOLUENO
	(Tt)
	E10/39

	FONDOS LIGEROS LIQUIDOS CONDENSADOS DE LA ETAPA DE PURIFICACION DE LA TOLUENDIAMINA OBTENIDA A TRAVES DE LA HIDROGENACION DE DINITROTOLUENO
	(Tt)
	E10/40

	VECINALES DE LA ETAPA DE PURIFICACION DE LA TOLUENDIAMINA OBTENIDA A TRAVES DE LA HIDROGENACION DE DINITROTOLUENO
	(Tt)
	E10/41

	FONDOS PESADOS DE LA ETAPA DE PURIFICACION DE LA TOLUENDIAMINA OBTENIDA A TRAVES DE LA HIDROGENACION DE DINITROTOLUENO
	(Tt)
	E10/42

	FONDOS DE LA DESTILACION EN LA PRODUCCION DE ALFA- (O METIL-) CLORO TOLUENOS, CLORO TOLUENOS CON RADICALES CICLICOS, CLORUROS DE BENZOILO Y MEZCLAS DE ESTOS GRUPOS FUNCIONALES. (ESTE RESIDUO NO INCLUYE FONDOS DE LA DESTILACION DE CLORURO DE BENCILO)
	(Tt)
	E10/43

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES, EXCLUYENDO LODOS DE NEUTRALIZACION Y BIOLOGICOS, GENERADOS EN EL TRATAMIENTO DE AGUAS RESIDUALES EN LA PRODUCCION DE TOLUENOS CLORADOS
	(Tt)
	E10/44

	RESIDUOS ORGANICOS, EXCLUYENDO CARBON ADSORBENTE GASTADO, DEL CLORO GASEOSO GASTADO Y DEL PROCESO DE RECUPERACION DE ACIDO HIDROCLORICO ASOCIADO CON LA PRODUCCION DE ALFA- (O METIL-) CLORO TOLUENOS, CLORO TOLUENOS CON RADICALES CICLICOS, CLORUROS DE BENZOILO Y MEZCLAS DE ESTOS GRUPOS FUNCIONALES 
	(Tt)
	E10/45

	CATALIZADORES GASTADOS DEL REACTOR DE HIDROCLORACION EN LA PRODUCCION DE 1,1,1-TRICLOROETANO
	(Tt)
	E10/46

	FONDOS DE LA ETAPA DE DESTILACION EN LA PRODUCCION DE 1,1,1-TRICLOROETANO
	(Tt)
	E10/47

	FONDOS PESADOS DE LA COLUMNA DE DESTILACION DE PRODUCTOS PESADOS EN LA PRODUCCION DE 1,1,1-TRICLOROETANO
	(Tt)
	E10/48

	RESIDUOS DEL LAVADOR CON VAPOR DEL PRODUCTO EN LA PRODUCCION DE 1,1,1-TRICLOROETANO
	(Tt)
	E10/49

	FONDOS O RESIDUOS PESADOS DE LAS TORRES EN EL PROCESO DE PRODUCCION DE TRICLOROETILENO
	(Tt)
	E10/50


	LIST 1



	CLASSIFICATION OF HAZARDOUS WASTES FROM A SPECIFIC SOURCE 

	WASTE
	CPR
	CODE

	INDUSTRIAL TYPE  1: BENEFICE OF METALS

	SPENT ELECTROLYTE CUBES FROM THE PRIMARY PRODUCTION OF ALUMINUM
	(Tt)
	E1/01

	SPENT LIQUOR GENERATED BY THE STEEL FINISHING OPERATIONS IN INSTALLATIONS BELONGING TO THE IRON AND STEEL INDUSTRY
	(C,Tt)
	E1/02

	SLUDGES AND DUSTS FORM THE CONTROL EQUIPMENT FOR EMISSIONS FROM FOUNDING AND REFINING IN THE SECONDARY PRODUCTION OF LEAD
	(Tt)
	E1/03

	SPENT SOLUTION ORIGINATING FROM THE ACID LEACHING OF THE SLUDGE/DUSTS FROM THE EMISSIONS CONTROL EQUIPMENT IN THE SECONDARY FOUNDING OF LEAD
	(Tt)
	E1/04

	INDUSTRIAL TYPE 2: COKE PRODUCTION

	WASTES THAT ARE NOT REINTEGRATED INTO THE PROCESS OF COKE PRODUCTION AND THAT CANNOT BE REUTILIZED
	(Tt)
	E2/01

	INDUSTRIAL TYPE 3: EXPLOSIVES

	SPENT CARBON FROM THE TREATMENT OF WASTEWATERS THAT CONTAIN EXPLOSIVES
	(R,E)
	E3/01

	SLUDGES FROM THE TREATMENT OF WASTEWATERS IN THE MANUFACTURE, FORMULATION AND LOAD OF THE INITIAL LEAD BASED COMPOUNDS 
	(Tt)
	E3/02

	WASTES OF RED/PINK WATER AND SPENT ACIDS FROM THE MANUFACTURE OF TNT
	(R,E)
	E3/03

	INDUSTRIAL 3: PETROLEUM, GAS AND PETROCHEMICALS

	SPENT CATALYZERS FROM THE PROCESS OF CATALYTIC “HYDROCRACKING” OF WASTES IN THE REFINING OF PETROLEUM 
	(I,Tt)
	E4/01

	SLUDGES FROM THE PRIMARY SEPARATION OF OIL/WATER/SOLIDS FROM THE REFINING OF PETROLEUM- ANY SLUDGE GENERATED BY GRAVITATIONAL SEPARATION OF OIL/WATER/SOLIDS DURING THE STORAGE OR TREATMENT OF WASTEWATERS FROM THE PROCESS AND OILY WASTEWATERS FROM COOLING, FROM PETROLEUM REFINERIES, SUCH SLUDGES INCLUDE BUT ARE NOT LIMITED TO, THOSE GENERATED IN SEPARATORS OF OIL/WATER/SOLIDS; CAPTURING TANKS AND RESERVOIRS; DITCHES AND OTHER SYSTEMS OF RAIN WATER TRANSPORT, SLUDGES GENERATED FROM COOLING WATERS WITHOUT CONTACT, IN ONE SINGLE OPERATION, SEGREGATED FOR TREATMENT WITH OTHER PROCESSES OR OILY COOLING WATERS AND SLUDGES GENERATED IN UNITS OF BIOLOGICAL TREATMENTS. 
	(Tt)
	E4/02

	SLUDGES FROM THE SECONDARY SEPARATION (EMULSIFICATIONS) OF OIL/WATER/SOLIDS. ANY SLUDGE AND/OR SLAG GENERATED IN THE PHYSICAL AND/OR CHEMICAL SEPARATION OF OIL/WATER/SOLIDS FROM WASTEWATERS FROM PROCESSING AND OILY WASTEWATERS FROM COOLING FROM PETROLEUM REFINERIES. SUCH WASTES INCLUDE, BUT ARE NOT LIMITED TO, ALL THE SLUDGES AND SLAGS GENERATED IN: INDUCED AIR FLOTATION UNITS, CAPTURE TANKS AND RESERVOIRS, AND AL LTHE SLUDGES GENERATED IN DAF (DISSOLVED AIR FLOTATION UNITS). SLUDGES GENERATED OF COOLING WATER WITHOUT CONTACT, OF A SINGLE PASS, SEGREGATED FOR TREATMENT OF OTHER PROCESSES OR OILY COOLING WATERS, SLUDGES AND SLAGS GENERATED IN BIOLOGICAL TREATMENT UNITS.
	(Tt)
	E4/03

	SLUDGES FROM THE API SEPARATOR AND TANK PUMPING SYSTEMS IN THE REFINING OF PETROLEUM AND STORAGE OF DERIVATIVE PRODUCTS
	(Tt)
	E4/04

	SLUDGES OF HYDROCARBON STORAGE TANKS
	(Tt)
	E4/05

	SLUDGES FROM THE CLEANING OF THE GROUPS OF PIPES AT THE HEAT INTERCHANGES, HYDROCARBON SIDE
	(Tt)
	E4/06

	SLAGS FROM THE FLOTATION SYSTEM WITH DISSOLVED AIR IN THE REFINING OF PETROLEUM AND STORAGE OF DERIVATIVE PRODUCTS
	(Tt)
	E4/07

	SOLIDS FROM EMULSION OF LOW QUALITY OILS IN THE PETROLEUM REFINING INDUSTRY 
	(Tt)
	E4/08

	RESIDUE FROM THE DISTILLATION STAGE IN THE PRODUCTION OF ACETALDEHYDE BY ETHYLENE OXIDATION
	(C,Tt,I)
	E4/09

	LATERAL CUTS FROM THE DISTILLATION STAGE IN THE PRODUCTION OF ACETALDEHYDE BY ETHYLENE OXIDATION
	(C,Tt,I)
	E4/10

	WASTES FROM PROCESSES, INCLUDING BUT NOT LIMITED TO DISTILLATION WASTES, HEAVY RESIDUE, TARS, AND WASTES FROM CLEANING OF REACTORS OF THE PRODUCTION OF ALIPHATIC CHLORIDE HYDROCARBONS FOR PROCESSES OF CATALYZATION OF FREE RADICALS THAT HAVE CHAINS OF UP TO 5 CARBONS WITH VARIOUS QUANTITIES AND POSITIONS OF SUBSTITUTION OF CHLORINE
	(Tt)
	E4/11

	INDUSTRIAL BRANCH 5: PAINTS AND RELATED PRODUCTS

	WASTES FROM CHROME AND LEAD BASED PIGMENTS
	(Tt)
	E5/01

	INDUSTRIAL BRANCH 6: PESTICIDES AND HERBICIDES

	SLUDGES FROM THE TREATMENT PLANTS OF WASTEWATERS IN THE PRODUCTION OF CARBAMATES, CHLORIDE HERBICIDES; ORGANIC-HALOGENATED PESTICIDES; ORGANIC-ARSENICS; ORGANIC-METALLICS AND ORGANIC PHOSPHATES
	(Tt)
	E6/01

	WASTES FROM THE PRODUCTION OF CARBAMATES, CHLORIDE HERBICIDES; ORGANIC-HALOGENATED PESTICIDES; ORGANIC-ARSENICS; ORGANIC-METALLIC AND ORGANIC PHOSPHATES
	(Tt)
	E6/02

	INDUSTRIAL BRANCH 7: PRESERVATION OF WOOD

	SEDIMENTARY SLUDGES AND SPENT SOLUTIONS GENERATED IN THE PROCESSES OF PRESERVATION OF WOOD 
	(Tt)
	E7/01

	INDUSTRIAL 8: PHARMACEUTICAL CHEMISTRY

	ACTIVATED CARBON SPENT IN THE PRODUCTION OF VETERINARY PHARMACEUTICALS OF COMPOUNDS WITH ARSENIC AND ORGANIC ARSENICS
	(Tt)
	E8/01

	WASTES OF TARS FROM THE DISTILLATION OF ANILINE BASED COMPOUNDS IN THE PRODUCTION OF VETERINARY PRODUCTS OF ARSENIC AND ORGANIC ARSENICS. 
	(Tt)
	E8/02

	INDUSTRIAL BRANCH 9: INORGANIC CHEMICALS

	FILTERS FROM BAGS IN THE PRODUCTION OF ANTIMONY OXIDE, INCLUDING THE FILTERS IN THE PRODUCTION OF INTERMEDIATE PRODUCTS (METALLIC ANTIMONY AND RAW ANTIMONY OXIDE)
	(Te)
	E9/01

	SLAGS FROM THE PRODUCTION OF ANTIMONY OXIDE, INCLUDING THOSE FROM THE INTERMEDIATE PRODUCTS (METALLIC ANTIMONY AND RAW ANTIMONY OXIDE)
	(Tt)
	E9/02

	SLUDGES FROM THE PURIFICATION OF 

LODOS DE LA PURIFICACION OF BRINE, WHERE THE SEPARATED PURIFIED BRINE IS NOT UTILIZED, IN THE PRODUCTION OF CHLORINE (PROCESS OF MERCURY CELLS) 
	(Tt)
	E9/03

	SLUDGES FROM THE TREATMENT OF WASTEWATERS IN THE PRODUCTION OF CHLORINE (PROCESS OF MERCURY CELLS)
	(Tt)
	E9/04

	WASTES FROM CHLORIDE HYDROCARBONS FROM THE STAGE OF PURIFICATION IN THE PRODUCTION OF CHLORIDE (PROCESS OF DIAPHRAGM CELLS USING ANODES OF GRAPHITE
	(Tt)
	E9/05

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF ORANGE PIGMENTS AND YELLOW CHROME
	(Tt)
	E9/06

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF GREEN CHROME PIGMENTS
	(Tt)
	E9/07

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF GREEN PIGMENTS OF CHROME OXIDE (ANHYDRIDES AND HYDRATED)
	(Tt)
	E9/08

	WASTES FROM THE OVEN OF THE PRODUCTION OF GREEN PIGMENTS OF CHROME OXIDE
	(Tt)
	E9/09

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF BLUE IRON PIGMENTS
	(Tt)
	E9/10

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF ORANGE PIGMENTS OF MOLYBDATE
	(Tt)
	E9/11

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF YELLOW ZINC PIGMENTS 
	(Tt)
	E9/12

	WASTES FROM MANUFACTURING AND FROM THE STORAGE OF IRON CHLORIDE DERIVED FROM ACIDS FORMED DURING THE PRODUCTION OF TITANIUM BIOXIDE THROUGH THE CHLORIDE-ILMENITE PROCESS
	(Tt)
	E9/13

	INDUSTRIAL BRANCH 10: ORGANIC CHEMICALS

	SLUDGES FROM THE DISCHARGES OF WASTEWATERS IN THE PRODUCTION OF ACRYLONITRILE
	(R, Tt)
	E10/01

	RESIDUE FROM THE ACETONITRILE COLUMN IN THE PRODUCTION OF ACRYLONITRILE
	(R, Tt)
	E10/02

	RESIDUE FROM THE PURIFICATION COLUMN OF ACETONITRILE IN THE PRODUCTION OF ACRYLONITRILE
	(Tt)
	E10/03

	LIGHT DOMES FROM THE INITIAL DISTILLATION IN THE PRODUCTION OF PHTALIC ANHYDRIDE FROM NAPHTALENE
	(Tt)
	E10/04

	RESIDUE FROM THE FINAL DISTILLATION IN THE PRODUCTION OF PHTALIC ANHYDRIDE FROM NAPHTALENE
	(Tt)
	E10/05

	LIGHT DOMES FROM THE INITIAL DISTILLATION IN THE PRODUCTION OF PHTALIC ANHYDRIDE FROM ORTHO XYLENE
	(Tt)
	E10/06

	RESIDUE FROM THE FINAL DISTILLATION IN THE PRODUCTION OF PHTALIC ANHYDRIDE IN THE PRODUCTION OF PHTALIC ANHYDRIDE FROM ORTHO XYLENE
	(Tt)
	E10/07

	RESIDUE FROM THE FINAL DISTILLATION IN THE PRODUCTION OF ANILINE
	(Tt)
	E10/08

	WASTES FROM THE EXTRACTION PROCESS OF ANILINE
	(Tt)
	E10/09

	WASTES ORIGINATING FROM THE WASHING OF GASES, FROM CONDENSATION, FROM PURGING AND SEPARATION IN THE PRODUCTION OF CARBAMATES AND CARBOMYL OXIMES
	(Tt)
	E10/10

	ORGANIC MATERIALS OF THE TREATMENT OF WASTES OF THIOCARBAMATE IN THE PRODUCTION OF CARBAMATES AND CARBOMYL OXIMES
	(Tt)
	E10/11

	DUSTS FROM BAGS AND SOLIDS FROM FILTERING/SEPARATION OF THE PRODUCTION OF CARBAMATES AND CARBOMYL OXIMES
	(Tt)
	E10/12

	ORGANIC WASTES (INCLUDING HEAVY RESIDUES, STEMS, LIGHT RESIDUES, SPENT SOLVENTS, WASTES FROM FILTRATION AND THE DECANTATION) FROM THE PRODUCTION OF CARBAMATES AND CARBOMYL OXIMES
	(Tt)
	E10/13

	SOLIDS FROM PURIFICATION (INCLUDING SOLIDS OF FILTRATION, EVAPORATION AND CENTRIFUGATION), DUSTS FROM BAGS AND FLOOR SWEEPINGS IN THE PRODUCTION OF THIOCARBAMATE ACIDS AND THEIR CARBAMATES AND CARBOMYL OXIMES
	(R,Tt)
	E10/14

	RESIDUE FROM THE DISTILLATION COLUMN OR SECTIONING IN THE PRODUCTION OF CHLOROBENZENES
	(Tt)
	E10/15

	CURRENTS SEPARATED FROM THE WATER FROM THE REACTOR OF WASHING OF CHLOROBENZENES
	(Tt)
	E10/16

	RESIDUE FROM THE DISTILLATION STAGE IN THE PRODUCTION OF BENZYL CHLORIDE
	(Tt)
	E10/17

	HEAVY WASTES FROM THE SECTIONING COLUMN IN THE PRODUCTION OF ETHYL CHLORIDE
	(Tt)
	E10/18

	HEAVY WASTES FROM THE DISTILLATION OF VINYL CHLORIDE IN THE PRODUCTION OF VINYL CHLORIDE MONOMER
	(Tt)
	E10/19

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF EHTYLENE DICHLORIDE OR VINYL CHLORIDE MONOMER 
	(Tt)
	E10/20

	SLUDGES FROM THE TREATMENT OF WASTEWATERS FROM THE PRODUCTION OF VINYL CHLORIDE MONOMER IN WHICH IS UTILIZED MERCURY CHLORIDE AS A CATALYZER IN AN ACETYLENE BASED PROCESS 
	(Tt)
	E10/21

	WASTES FROM THE CLEANING OF GASES FROM THE VENTING OF THE REACTOR IN THE PRODUCITON OF ETHYLENE DIBROMIDE BY ETHYLENE BROMATION
	(Tt)
	E10/22

	SPENT ABSORBENT SOLIDS FROM THE PURIFICATION STAGE FROM THE ETHYLENE DIBROMIDE OBTAINED FROM ETHYLENE BROMATION
	(Tt)
	E10/23

	RESIDUES FROM THE PURIFICATION STAGE OF ETHYLENE DIBROMIDE OBTAINED FROM ETHYLENE BROMATION
	(Tt)
	E10/24

	ORGANIC CONDENSATIONS FROM THE RECOVERY COLUMN OF SOLVENTS IN THE PRODUCTION OF TOLUENE DIISOCYANATE BY PHOSGENATION OF TOLUENE DIAMINE
	(Tt)
	E10/25

	WASTES FORM CENTRIFUGATION AND DISTILLATION IN THE PRODUCTION OF TOLUENE DIISOCYANATE FROM PHOSGENATION OF TOLUENE DIAMINE
	(R,Tt)
	E10/26

	RESIDUE FROM THE SEPARATION TOWER OF PRODUCTS IN THE PRODUCTION OF 1,1-DIMETHYL HYDRACINE FROM HYDRACINES OF CARBOXILIC ACID
	(C,Tt)
	E10/27

	CONDENSED HEADS FORM THE SEPARATION COLUMN OF PRODUCTS AND CONDENSED GASES FROM THE VENTING OF THE REACTOR IN THE PRODUCTION OF 1,1-DIMETHYL HYDRACINE FROM CARBOXILIC ACID HYDRACINES
	(Tt,I)
	E10/28

	CARTRIDGES FROM THE SPENT FILTERS FROM THE PURIFICATION OF THE 1,1-DIMETHYL HYDRACINE OBTAINED FROM CARBOXILIC ACID HYDRACINES
	(Tt)
	E10/29

	CONDENSED HEADS FORM THE SEPARATION COLUMN OF INTERMEDIATES IN THE PRODUCTION OF 1,1- DIMETHYL HYDRACINE OBTAINED FROM CARBOXILIC ACID HYDRACINES
	(Tt)
	E10/30

	WASTES ORIGINATING FROM THE CLEANING OF DINITROTOLUENE OBTAINED FROM THE NITRATION OF TOLUENE
	(C,Tt)
	E10/31

	HEAVY RESIDUES FROM THE PURIFICATION COLUMN OF EPICHLORHYDRINE
	(Tt)
	E10/32

	HEAVY RESIDUES (TAR) FROM THE DISTILLATION STAGE IN THE PRODUCTION OF PHENOL/ACETONE FROM CUMENE
	(Tt)
	E10/33

	WASTE FROM THE SPENT CATALYZER OF ANTIMONY IN AQUAEOUS SOLUTION IN THE PRODUCTION OF FLOUROMETHANES
	(Tt)
	E10/34

	GLUES FROM THE DISCHARGES IN THE PRODUCTION OF METHYL ETHYL PYRIDINES
	(Tt)
	E10/35

	COMBINED CURRENTS OF WASTEWATERS IN THE PRODUCTION OF NITROBENZENE/ANILINE
	(Tt)
	E10/36

	RESIDUE FROM THE DISTILLATION IN THE PRODUCTION OF NITROBENZENE THROUGH THE NITRATION OF BENZENE
	(Tt)
	E10/37

	HEAVY RESIDUE OR WASTE PRODUCTS FROM THE DISTILLATION STAGE IN THE PRODUCTION OF CARBON TETRACHLORIDE
	(Tt)
	E10/38

	REACTION WATER (BYPRODUCT) FROM THE DRYING COLUMN IN THE PRODUCTION OF TOLUENE DIAMINE BY HYDROGENATION OF DINITROTOLUENE
	(Tt)
	E10/39

	LIGHT LIQUID RESIDUES CONDENSED FROM THE PURIFICATION STAGE OF TOLUENEDIAMINE OBTAINED THROUGH THE HYDROGENATION OF DINITROTOLUENE
	(Tt)
	E10/40

	ROADS FROM THE PURIFICATION STAGE FROM TOLUENE DIAMINE OBTAINED THROUGH HYDROGENATION OF DINITROTOLUENE
	(Tt)
	E10/41

	HEAVY RESIDUES FROM THE PURIFICATION STAGE FROM THE TOLUENE DIAMINE OBTAINED THROUGH THE HYDROGENATION OF DINITROTOLUENE
	(Tt)
	E10/42

	RESIDUES FROM THE DISTILLATION IN THE PRODUCITON OF ALPHA-(O METHYL-) CHLORIDE TOLUENES, CHLORIDE TOLUENES WITH CYCLIC RADICALS, BENZOIL CHLORIDES, AND MIXTURES OF THESE FUNCTIONAL GROUPS, (THIS WASTE DOES NOT INCLUDE RESIDUES FROM THE DISTILLATION OF BENZYL CHLORIDE)
	(Tt)
	E10/43

	SLUDGES FROM THE TREATMENT OF WASTEWATERS, EXCLUDING SLUDGES OF NEUTRALIZATION AND BIOLOGICAL SLUDGES GENERATED IN THE TREATMENT OF WASTEWATERS IN THE PRODUCTION OF CHLORIDE TOLUENES
	(Tt)
	E10/44

	ORGANIC WASTES, EXLUDING SPENT ABSORBENT CARBON, FORM SPENT GASEOUS CHLORIDE, AND FROM THE PROCESS OF HYDROCHLORIC ACID RECOVERY ASSOCIATED WITH THE PRODUCTION OF ALPHA-(O METHL-) CHLORIDE TOLUENES, CHLORIDE TOLUENES WITH CYCLIC RADICALS, BENZOIL CHLORIDES AND MIXTURES OF THESE FUNCTIONAL GROUPS 
	(Tt)
	E10/45

	SPENT CATALYZERS FROM THE REACTOR OF HYDROCHLORATION IN THE PRODUCTION OF 1,1,1-TRICHLOROETHANE
	(Tt)
	E10/46

	RESIDUE FORM THE DISTILLATION STAGE IN THE PRODUCTION OF 1,1,1-TRICHLOROETHANE
	(Tt)
	E10/47

	HEAVY RESIDUE FROM THE DISTILLATION COLUMN OF HEAVY PRODUCTS IN THE PRODUCTION OF 1,1,1-TRICHLOROETHANE
	(Tt)
	E10/48

	WASTES FROM THE CLEANING WITH STEAM OF THE PRODUCT IN THE PRODUCTION OF 1,1,1-TRICHLOROETHANE
	(Tt)
	E10/49

	RESIDUES OR HEAVY WASTES FROM THE TOWERS IN THE PROCESS OF PRODUCTION OF TRICLOROETHYLENE
	(Tt)
	E10/50


	LISTADO 2



	CLASIFICACION DE RESIDUOS PELIGROSOS POR FUENTE NO ESPECIFICA



	Residuo
	CPR
	Clave

	RESIDUOS DEL MANEJO DE LA FIBRA DE ASBESTO PURO, INCLUYENDO POLVO, FIBRAS Y PRODUCTOS FACILMENTE DESMENUZABLES CON LA PRESION DE LA MANO (TODOS LOS RESIDUOS QUE CONTENGAN ASBESTO EL CUAL NO ESTE SUMERGIDO O FIJO EN UN AGLUTINANTE NATURAL O ARTIFICIAL)
	(Tt)
	NE 01

	TODAS LAS BOLSAS QUE HAYAN TENIDO CONTACTO CON LA FIBRA DE ASBESTO, ASI COMO LOS MATERIALES FILTRANTES PROVENIENTES DE LOS EQUIPOS DE CONTROL COMO SON: LOS FILTROS, MANGAS, RESPIRADORES PERSONALES Y OTROS, QUE NO HAYAN RECIBIDO UN TRATAMIENTO PARA ATRAPAR LA FIBRA EN UN AGLUTINANTE NATURAL O ARTIFICIAL
	(Tt)
	NE 02

	TODOS LOS RESIDUOS PROVENIENTES DE LOS PROCESOS DE MANUFACTURA CUYA MATERIA PRIMA SEA EL ASBESTO Y LA FIBRA SE ENCUENTRE EN FORMA LIBRE, POLVO O FACILMENTE DESMENUZABLE CON LA PRESION DE LA MANO
	(Tt)
	NE 03

	LODOS DE TRATAMIENTO DE AGUAS RESIDUALES DE APAGADO DE LAS OPERACIONES DE TRATAMIENTO TERMICO DE METALES DONDE LOS CIANUROS SON USADOS EN LOS PROCESOS
	(Tt)
	NE 04

	LODOS DE TRATAMIENTO DE AGUAS RESIDUALES DE OPERACIONES DE GALVANOPLASTIA EXCEPTO DE LOS SIGUIENTES PROCESOS: (1) ANODIZACION DE ALUMINIO EN ACIDO SULFURICO; (2) ESTAÑADO EN ACERO AL CARBON; (3) ZINCADO EN ACERO AL CARBON; (4) DEPOSITACION DE ALUMINIO O ZINC-ALUMINIO EN ACERO AL CARBON; (5) LIMPIEZA ASOCIADA CON ESTAÑADO, ZINCADO O ALUMINADO EN ACERO AL CARBON; Y (6) GRABADO QUIMICO Y ACABADO DE ALUMINIO DEPOSITADO EN ACERO AL CARBON
	(Tt)
	NE 05

	LODOS DE LOS BAÑOS DE ANODIZACION DEL ALUMINIO Y LODOS DE TRATAMIENTO DE AGUAS RESIDUALES DEL REVESTIMIENTO DE ALUMINIO POR CONVERSION QUIMICA
	(Tt)
	NE 06

	RESIDUOS DE LOS BAÑOS EN OPERACIONES DE GALVANOPLASTIA DONDE LOS CIANUROS SON USADOS EN LOS PROCESOS
	(R,Tt)
	NE 07

	SOLUCIONES GASTADAS DE BAÑOS DE CIANURO DE LAS OPERACIONES DE GALVANOPLASTIA
	(R,Tt)
	NE 08

	SOLUCIONES GASTADAS DE LOS BAÑOS DE LIMPIEZA Y EN OPERACIONES DE GALVANOPLASTIA DONDE LOS CIANUROS SON USADOS EN LOS PROCESOS
	(R,Tt)
	NE 09

	RESIDUOS DE LOS BAÑOS DE ACEITE EN LAS OPERACIONES DE TRATAMIENTO TERMICO DE METALES
	(R,Tt)
	NE 10

	SOLUCIONES GASTADAS DE CIANUROS DE LA LIMPIEZA DE TANQUES DE BAÑOS DE SAL EN LAS OPERACIONES DE TRATAMIENTO TERMICO DE METALES
	(R,Tt)
	NE 11

	RESIDUOS GENERADOS EN LA PRODUCCION DE TRI-, TETRA- O PENTACLOROFENOL
	(Th)
	NE 12

	RESIDUOS DE TETRA-, PENTA O HEXACLOROBENCENO PROVENIENTES DE SU USO COMO REACTANTE, PRODUCTO INTERMEDIO O COMPONENTE DE UNA FORMULACION, BAJO CONDICIONES ALCALINAS 
	(Th)
	NE 13

	RESIDUOS, EXCEPTO AGUAS RESIDUALES Y CARBON GASTADO DE LA PURIFICACION DE CLORURO DE HIDROGENO, DE LA PRODUCCION DE MATERIALES EN EQUIPOS PREVIAMENTE USADOS EN LA MANUFACTURA (COMO REACTIVO, PRODUCTO QUIMICO INTERMEDIO O COMPONENTE EN UN PROCESO DE FORMULACION) DE TRI- Y TETRACLOROFENOLES. ESTE RESIDUO NO INCLUYE DESECHOS DE EQUIPOS UTILIZADOS EN LA PRODUCCION O USO DE HEXACLOROFENO A PARTIR DEL 2,4,5-TRICLOROFENOL ALTAMENTE PURIFICADO
	(Th)
	NE 14

	FONDOS LIGEROS CONDENSADOS, FILTROS GASTADOS Y FILTROS AYUDA Y RESIDUOS DE DESECANTE GASTADO DE LA PRODUCCION DE CIERTOS HIDROCARBUROS ALIFATICOS CLORADOS A TRAVES DE LOS PROCESOS CATALITICOS DE RADICALES LIBRES. ESTOS HIDROCARBUROS ALIFATICOS CLORADOS SON AQUELLOS CON CADENAS DE UNO HASTA CINCO CARBONOS Y QUE CONTIENEN CLORO EN CANTIDADES Y SUSTITUCIONES VARIADAS 
	(Tt)
	NE 15

	RESIDUOS DE LA PRODUCCION DE MATERIALES EN EQUIPOS PREVIAMENTE USADOS EN LA PRODUCCION O MANUFACTURA DE TETRA-, PENTA- O HEXACLOROBENCENOS (COMO REACTIVO, PRODUCTO QUIMICO INTERMEDIO O COMPONENTE EN UN PROCESO DE FORMULACION) BAJO CONDICIONES ALCALINAS, EXCEPTO AGUAS RESIDUALES Y CARBON GASTADO DE LA PURIFICACION DE CLORURO DE HIDROGENO
	(Th)
	NE 16

	RESIDUALES DE PROCESO, FORMULACIONES GASTADAS DE PROCESOS DE PRESERVACION DE LA MADERA EN PLANTAS QUE UTILIZAN ACTUALMENTE O HAYAN UTILIZADO FORMULACIONES DE CLOROFENOL, EXCEPTO AQUELLOS QUE NO HAYAN ESTADO EN CONTACTO CON CONTAMINANTES DE PROCESO
	(Tt)
	NE 17

	RESIDUALES DE PROCESO Y FORMULACIONES GASTADAS DE PROCESOS DE PRESERVACION DE LA MADERA EN PLANTAS QUE UTILICEN FORMULACIONES DE CREOSOTA, EXCEPTO AQUELLOS QUE NO HAYAN ESTADO EN CONTACTO CON CONTAMINANTES DE PROCESO
	(Tt)
	NE 18

	RESIDUALES DE PROCESO Y FORMULACIONES GASTADAS DE PROCESOS DE PRESERVACION DE LA MADERA EN PLANTAS QUE UTILICEN FORMULACIONES INORGANICAS QUE CONTENGAN ARSENICO O CROMO PARA PRESERVAR LA MADERA, EXCEPTO AQUELLOS QUE NO HAYAN ESTADO EN CONTACTO CON CONTAMINANTES DE PROCESO
	(Tt)
	NE 19

	LIXIVIADOS (LIQUIDOS QUE HAN PERCOLADO A TRAVES DE RESIDUOS DISPUESTOS EN TIERRA) RESULTANTES DE LA DISPOSICION DE UNO O MAS DE LOS RESIDUOS PELIGROSOS SEÑALADOS EN ESTA NORMA
	(Tt)
	NE 20

	RESIDUOS RESULTANTES DE LA INCINERACION O DE TRATAMIENTO TERMICO DE SUELOS CONTAMINADOS CON LOS RESIDUOS PELIGROSOS CON CLAVES NE 12, NE 13, NE 14 Y NE 16 
	(Tt)
	NE 21


	LIST 2



	CLASSIFICATION OF HAZARDOUS WASTES FROM NON SPECIFIC SOURCE



	WASTE
	CPR
	Clave

	WASTES FROM THE HANDLING OF PURE ASBESTOS FIBER, INCLUDING DUST, FIBERS AND PRODUCTS EASILY CRUMBLED WITH THE PRESSURE OF THE HAND (ALL THE WASTES THAT CONTAIN ASBESTOS WHICH ARE NOT SUBMERGED OR SET IN A NATURAL OR ARTIFICIAL ADHESIVE MATERIAL)
	(Tt)
	NE 01

	ALL THE BAGS THAT HAVE HAD CONTACT WITH ASBESTOS FIBER, AS WELL AS THE FILTERING MATERIALS ORGINATING FROM THE CONTROL EQUIPMENT SUCH AS: FILTERS, SLEEVES, PERSONAL RESPIRATORS AND OTHERS THAT HAVE NOT RECEIVED A TREATMENT FOR TRAPPING THE FIBER IN A NATURAL OR ARTIFICIAL ADHESIVE MATERIAL
	(Tt)
	NE 02

	ALL THE WASTES ORIGINATING FROM THE MANUFACTURING PROCESSES WHOSE RAW MATERIAL IS ASBESTOS AND THE FIBER IS LOOSE, DUST, OR EASILY CRUMBLED WITH PRESSURE FROM THE HAND
	(Tt)
	NE 03

	SLUDGES FROM TREATMENT OF WASTEWATERS OF RESULTING FROM THE THERMAL TREATMENT OPERATIONS OF METALS WHERE CYANIDES ARE USED IN THE PROCESS
	(Tt)
	NE 04

	SLUDGES OF TREATMENT FROM WASTEWATERS OF OPERATIONS OF GALVANOPLASTY EXCEPT FROM THE FOLLOWING PROCESSES: 

(1) ANODIZATION OF ALUMINUM IN SULFURIC ACID; 

(2) SOLDERED STEEL TO CARBON; 

(3) ZINCE IN STEEL TO CARBON;

(4) DEPOSIT OF ALUMINUM OR ZINC-ALUMINUM IN STEEL TO CARBON; 

(5) CLEANING ASSOCIATED WITH SOLDERING, ZINC PLATING, OR ALUMINUM IN STEEL TO CARBON; AND

(6) CHEMICAL ENGRAVING AND FINISHING OF ALUMINUM DEPOSITED IN STEEL TO CARBON


	(Tt)
	NE 05

	SLUDGES FROM THE ANODIZATION BATHS OF ALUMINUM AND SLUDGES OF WASTEWATERS TREATMENTS FROM THE COATING OF ALUMINUM BY CHEMICAL CONVERSION
	(Tt)
	NE 06

	WASTES FROM BATHS IN OPERATIONS OF GALVANOPLASTY WHERE CYANIDES ARE USED IN THE PROCESS
	(R,Tt)
	NE 07

	SPENT SOLUTIONS FROM CYANIDE BATHS FROM THE OPERATIONS OF GALVANOPLASTY
	(R,Tt)
	NE 08

	SPENT SOLUTIONS FROM THE CLEANING BATHS IN OPERATIONS OF GALVANOPLASTY WHERE CYANIDES ARE USED IN THE PROCESS
	(R,Tt)
	NE 09

	WASTES FROM OIL BATHS IN THE THERMAL TREATMENT OPERATIONS OF METALS
	(R,Tt)
	NE 10

	SPENT SOLUTIONS OF CYANIDES FROM THE CLEANING OF TANKS OF SALT BATHS IN THE THERMAL TREATMENT OPERATIONS OF METALS
	(R,Tt)
	NE 11

	WASTES GENERATED IN THE PRODUCTION OF TRI-, TETRA-, 0 PENTACHLOROPHENOL
	(Th)
	NE 12

	WASTES OF TETRA-, PENTA-, OR HEXACHLOROBENZENE ORIGINATING FROM THEIR USE AS A REACTIVE, INTERMEDIATE PRODUCT OR COMPONENT OF A FORMULA, UNDER ALKALINE CONDITIONS. 
	(Th)
	NE 13

	WASTES, EXCEPT WASTEWATERS AND SPENT CARBON FROM THE PURIFICATION OF HYDROGEN CHLORIDE FROM THE PRODUCTION OF MATERIASL IN EQUIPMENT OF HYDROGEN CHLORIDE FROM THE PRODUCTION OF MATERIALS IN EQUIPMENT PREVIOUSLY USED IN THE MANUFACTURING (AS A REACTIVE, INTERMEDIARY CHEMICAL PRODUCT OR COMPONENT IN A PROCESS OF FORMULA) OF TRI- AND TETRACHLOROPHENOLS. THIS WASTE DOES NOT INCLUDE DISCARDED MATERIAL FROM EQUIPMENT UTILIZED IN THE PRODUCITON OR USE OF HEXACHLOROPHENE FROM HIGHLY PURIFIED 2,4,5-TRICHLOROPHENOL 
	(Th)
	NE 14

	LIGHTLY CONDENSED RESIDUES, SPENT FILTERS AND SECONDARY FILTERS AND WASTES FROM SPENT DESICANT FROM THE PRODUCTION OF CERTAIN CHLORIDE ALIPHATIC HYDROCARBONS FROM CATALYTIC PROCESSES OF FREE RADICALS. THESE CHLORIDE ALIPHATIC HYDROCARBONS ARE THOSE WITH CHAINS OF ONE TO FIVE CARBONS AND THAT CONTAIN CHLORIDE IN VARIED QUANTITIES AND SUBSTITUTIONS. 
	(Tt)
	NE 15

	WASTES FROM THE PRODUCTION OF MATERIALS IN EQUIPMENT PREVIOUSLY USED IN THE PRODUCTION OR MANUFACTURE OF TETRA-, PENTA-, OR HEXACHLOROBENZENES (SUCH AS REACTIVE, INTERMEDIARY CHEMICAL PRODU CT OR COMPONENT IN A FORMULATION PROCESS) UNDER ALKALINE CONDITIONS, EXCET WASTEWATERS AND SPENT CARBON FROM THE PURIFICATION OF HYDROGEN CHLORIDE
	(Th)
	NE 16

	WASTES FROM PROCESSING, SPENT FORMULATIONS FROM PROCESSES OF PRESERVATION OF WOOD IN PLANTS THAT PRESENTLY USE OR HAVE USED CHLOROPHENOL FORMULATIONS, EXCEPT THOSE THAT HAVE NOT BEEN IN CONTACT WITH CONTAMINANTS OF PROCESS
	(Tt)
	NE 17

	WASTES FROM THE PROCESS AND SPENT FORMULATIONS OF PROCESSES OF PRESERVATION OF WOOD IN PLANTS THAT UTILIZE FORMULATIONS OF CREOSOTE, EXCEPT THOSE THAT HAVE NOT BEEN IN CONTACT WITH CONTAMINANTS OF PROCESS
	(Tt)
	NE 18

	WASTES OF PROCESS AND SPENT FORMULATIONS FROM PROCESSES OF PRESERVATION OF WOOD IN PLANTS THAT UTILIZE INORGANIC FORMULATIONS THAT CONTAIN ARSENIC OR CHROME FOR PRESERVING WOOD, EXCEPT THOSE THAT HAVE NOT BEEN IN CONTACT WITH CONTAMINANTS IN THE PROCESS. 
	(Tt)
	NE 19

	LEACHED LIQUIDS (THAT HAVE PERCOLATED THROUGH WASTES DISPOSED OF IN SOIL) RESULTING FROM THE DISPOSAL OF ONE OR MORE OF THE HAZARDOUS WASTES STIPULATED IN THIS STANDARD
	(Tt)
	NE 20

	WASTES RESULTING FROM THE INCINERATION OR THERMAL TREATMENT OF SOIL CONTAMINATED WITH THE HAZARDOUS WASTES WITH THE CODES NE12, NE 13, NE 14, AND NE 16. 
	(Tt)
	NE 21


	LISTADO 3



	CLASIFICACION DE RESIDUOS PELIGROSOS RESULTADO DEL DESECHO DE PRODUCTOS QUIMICOS FUERA DE ESPECIFICACIONES O CADUCOS (TOXICOS AGUDOS)



	No. CAS
	Nombre
	CPR
	Clave

	5344–82–1
	1-(o-Clorofenil)tiourea/2-Clorofeniltiourea
	(Th)
	H026

	58-90-2
	2,3,4,6-Tetraclorofenol
	(Th)
	H1000

	95-95-4
	2,4,5-Triclorofenol
	(Th)
	H1001

	93-76-5
	2,4,5-Triclorofenoxiacético, ácido/2,4,5-T
	(Th)
	H1002

	88-06-2
	2,4,6-Triclorofenol
	(Th)
	H1003

	51–28–5
	2,4-Dinitrofenol
	(Th)
	H048

	131–89–5
	2-Ciclohexil-4,6-dinitrofenol
	(Th)
	H034

	542–76–7
	3-Cloropropionitrilo
	(Th)
	H027

	(1) 534–52–1
	4,6-Dinitro-o-cresol, y sales
	(Th)
	H047

	504–24–5
	4-Aminopiridina
	(Th)
	H008

	2763–96–4
	5-(Aminometil)-3-isoxazolol
	(Th)
	H007

	591–08–2
	Acetamida, G1159N-(aminotioxometil)-/1-Acetil-2-tiourea
	(Th)
	H002

	107–02–8
	Acroleína/2-Propenal
	(Th)
	H003

	116–06–3
	Aldicarb
	(Th)
	H070

	1646–88–4
	Aldicarb sulfona
	(Th)
	H203

	309–00–2
	Aldrín
	(Th)
	H004

	122–09–8
	alfa,alfa-Dimetilfenetilamina/Bencenoetanamina, alfa,alfa-dimetil 
	(Th)
	H046

	86–88–4
	alfa-Naftiltiourea/Tiourea, 1-naftalenil 
	(Th)
	H072

	107–18–6
	Alílico, alcohol/2-Propen-1-ol
	(Th)
	H005

	20859–73–8
	Aluminio, fosfuro de 
	(R,Th)
	H006

	131–74–8
	Amonio, picrato de/Fenol, 2,4,6-trinitro-, amonio sal
	(R,Th)
	H009

	7803–55–6
	Amonio, vanadato de 
	(Th)
	H119

	7778–39–4
	Arsénico, ácido H3AsO4
	(Th)
	H010

	1327–53–3
	Arsénico, óxido As2O3
	(Th)
	H012

	1303–28–2
	Arsénico, óxido As2O5
	(Th)
	H011

	75–55–8
	Aziridina, 2-Metil-/1,2-Propilenimina
	(Th)
	H067

	151–56–4
	Aziridina/Etilenoimina
	(Th)
	H054

	542–62–1
	Bario, cianuro de 
	(Th)
	H013

	108–98–5
	Bencenotiol/Tiofenol
	(Th)
	H014

	100–44–7
	Benzilo, cloruro de/Clorometilbenceno
	(Th)
	H028

	7440–41–7
	Berilio, polvo de (todas las formas)
	(Th)
	H015

	598–31–2
	Bromoacetona/2-Propanona, 1-bromo-
	(Th)
	H017

	357–57–3
	Brucina
	(Th)
	H018

	592–01–8
	Calcio, cianuro de Ca(CN)2
	(Th)
	H021

	1563–66–2
	Carbofurano
	(Th)
	H127

	75–15–0
	Carbono, disulfuro de 
	(Th)
	H022

	55285–14–8
	Carbosulfan
	(Th)
	H189

	74–90–8
	Cianhídrico, ácido 
	(Th)
	H063

	506–77–4
	Cianógeno, cloruro de (CN)Cl
	(Th)
	H033

	460–19–5
	Cianógeno/Etanodinitrilo
	(Th)
	H031

	----
	Cianuro, sales solubles de (no especificadas de otra manera)
	(Th)
	H030

	107–20–0
	Cloracetaldehído
	(Th)
	H023

	544–92–3
	Cobre, cianuro de Cu(CN)
	(Th)
	H029

	696–28–6
	Diclorofenilarsina
	(Th)
	H036

	542–88–1
	Diclorometil éter/Metano, oxibis[cloro
	(Th)
	H016

	60–57–1
	Dieldrín
	(Th)
	H037

	692–42–2
	Dietilarsina
	(Th)
	H038

	311–45–5
	Dietil-p-nitrofenil fosfato/Fosfórico ácido, dietil 4-nitrofenil éster
	(Th)
	H041

	55–91–4
	Diisopropilfluorofosfato (DFP)/Fosforofluorhídrico ácido, bis(1-metiletil) éster
	(Th)
	H043

	644–64–4
	Dimetilán
	(Th)
	H191

	60–51–5
	Dimetoato
	(Th)
	H044

	88-85-7
	Dinoseb/Fenol, 2-(1-metilpropil)-4,6-dinitro 
	(Th)
	H020

	298–04–4
	Disulfotón
	(Th)
	H039

	541–53–7
	Ditiobiuret
	(Th)
	H049

	115–29–7
	Endosulfan
	(Th)
	H050

	145–73–3
	Endotal
	(Th)
	H088

	(1) 72–20–8
	Endrín, y sus metabolitos
	(Th)
	H051

	51–43–4
	Epinefrina 
	(Th)
	H042

	(1) 57–24–9
	Estricnidín-10-ona, y sales/Estricnina, y sales
	(Th)
	H108

	52–85–7
	Famfur
	(Th)
	H097

	62–38–4
	Fenilmercurio, acetato de/Mercurio, (acetato-o)fenil-
	(Th)
	H092

	103–85–5
	Feniltiourea
	(Th)
	H093

	57–47–6
	Fisostigmina
	(Th)
	H204

	57–64–7
	Fisostigmina, salicilato de
	(Th)
	H188

	7782–41–4
	Fluorina
	(Th)
	H056

	640–19–7
	Fluoroacetamida/2-Fluoroacetamida
	(Th)
	H057

	62–74–8
	Fluoroacético, ácido, sal de sodio
	(Th)
	H058

	298–02–2
	Forato
	(Th)
	H094

	23422–53–9
	Formetanato, hidrocloruro de 
	(Th)
	H198

	17702–57–7
	Formparanato
	(Th)
	H197

	7803–51–2
	Fosfina/Fosfhídrico, ácido 
	(Th)
	H096

	75–44–5
	Fosgeno
	(Th)
	H095

	76–44–8
	Heptacloro
	(Th)
	H059

	757–58–4
	Hexaetil tetrafosfato/Tetrafósforico, ácido, hexaetil éster
	(Th)
	H062

	465–73–6
	Isodrín
	(Th)
	H060

	119–38–0
	Isolan
	(Th)
	H192

	15339–36–3
	Manganeso dimetilditiocarbamato
	(Th)
	H196

	64–00–6
	M-cumenil metilcarbamato/3-Isopropilfenil n-metilcarbamato
	(Th)
	H202

	628-86-4
	Mercurio fulminato
	(R,Th)
	H065

	60–34–4
	Metil hidrazina
	(Th)
	H068

	624–83–9
	Metil isocianato/Metano, isocianato-
	(Th)
	H064

	298–00–0
	Metil paration/Fosforotioico ácido, o,o-dimetil o-(4-nitrofenil) éster
	(Th)
	H071

	75–86–5
	Metilactonitrilo/Propanonitrilo, 2-hidroxi-2-metil-
	(Th)
	H069

	2032–65–7
	Metiocarb.
	(Th)
	H199

	1129–41–5
	Metolcarb/Carbámico ácido, metil-, 3-metilfenil éster
	(Th)
	H190

	16752–77–5
	Metomil
	(Th)
	H066

	315–8–4
	Mexacarbato
	(Th)
	H128

	(1) 54–11–5
	Nicotina, y sales/Piridina, 3-(1-metil-2-pirrolidinil)-, (s)-, y sales
	(Th)
	H075

	13463–39–3
	Níquel carbonil Ni(CO)4, (t-4)-
	(Th)
	H073

	557–19–7
	Níquel, cianuro de Ni(CN)2
	(Th)
	H074

	10102–43–9
	Nitrógeno, óxido de/Nítrico, óxido (NO)
	(Th)
	H076

	10102–44–0
	Nitrógeno, dióxido de 
	(Th)
	H078

	55–63–0
	Nitroglicerina/1,2,3-Propanotriol, trinitrato de
	(E,Th)
	H081

	62–75–9
	n-Nitrosodimetilamina
	(Th)
	H082

	4549–40–0
	n-Nitrosometilvinilamina
	(Th)
	H084

	297–97–2
	o,o-dietil o-pirazinil fosforotioato
	(Th)
	H040

	152–16–9
	Octametilpirofosforamida/Difosforamida, octametil
	(Th)
	H085

	20816–12–0
	Osmio óxido OsO4, (T-4)-
	(Th)
	H087

	23135–22–0
	Oxamil
	(Th)
	H194

	56–38–2
	Paration
	(Th)
	H089

	106–47–8
	p-Cloroanilina/Bencenamina, 4-cloro-
	(Th)
	H024

	87-86-5
	Pentaclorofenol
	(Th)
	H1004

	506–64–9
	Plata, cianuro de Ag(CN)
	(Th)
	H104

	78–00–2
	Plumbano, tetraetil-/Tetraetilo de plomo
	(Th)
	H110

	100–01–6
	p-Nitroanilina/Bencenamina, 4-nitro-
	(Th)
	H077

	151–50–8
	Potasio, cianuro de K(CN)
	(Th)
	H098

	506–61–6
	Potasio plata, cianuro de/Argentato(1-), bis(ciano-c)-, potasio
	(Th)
	H099

	2631–37–0
	Promecarb/Fenol, 3-metil-5-(1-metiletil)-, metil carbamato
	(Th)
	H201

	107–12–0
	Propanonitrilo
	(Th)
	H101

	107–19–7
	Propargil alcohol/2-Propin-1-ol
	(Th)
	H102

	630–10–4
	Selenourea
	(Th)
	H103

	93-72-1
	Silvex (2,4,5-TP)/Propanoico ácido, 2-(2,4,5-triclorofenoxi)-
	(Th)
	H1005

	26628–22–8
	Sodio, azida de 
	(Th)
	H105

	143–33–9
	Sodio, cianuro de Na(CN)
	(Th)
	H106

	1314–32–5
	Talio, óxido de/Tálico, óxido Tl2O3
	(Th)
	H113

	12039–52–0
	Talio, selenita de 
	(I,Th)
	H114

	7446–18–6
	Talio, sulfato de 
	(I,Th)
	H115

	107–49–3
	Tetraetilpirofosfato/Difosfórico ácido, tetraetil éster
	(Th)
	H111

	3689–24–5
	Tetraetilditiopirofosfato/Tiodifosfórico ácido, tetraetil éster
	(Th)
	H109

	509–14–8
	Tetranitrometano 
	(R,Th)
	H112

	39196–18–4
	Tiofanax
	(Th)
	H045

	79–19–6
	Tiosemicarbazida/Hidrazinacarbotioamida
	(Th)
	H116

	26419–73–8
	Tirpato
	(Th)
	H185

	8001–35–2
	Toxafeno
	(Th)
	H123

	75–70–7
	Triclorometanotiol
	(Th)
	H118

	1314–62–1
	Vanadio, óxido de V2O5
	(Th)
	H120

	(1) 81–81–2
	Warfarina, y sales, cuando están presentes en concentraciones mayores que 0.3%
	(Th)
	H001

	557–21–1
	Zinc, cianuro de Zn(CN)2
	(Th)
	H121

	1314–84–7
	Zinc, fosfuro de Zn3P2, cuando está presente en concentraciones mayores que 10%
	(R,Th)
	H122

	137-30-4
	Ziram
	(Th)
	H205

	1.- En el caso de familias de isómeros de compuestos orgánicos, sólo se menciona el nombre del grupo, todos los isómeros se deben considerar constituyentes tóxicos (p.e. diclorobencenos, incluye al 1,2 1,3 y 1,4 diclorobencenos).

	2.- La llamada (1) indica el número CAS de un compuesto equivalente


	LIST 3



	CLASSIFICATION OF HAZARDOUS WASTES RESULTING FROM THE WASTE OF CHEMICAL PRODUCTS OUTSIDE OF SPECIFICATIONS OR EXPIRED (ACUTE TOXICS)



	CAS
	NAME
	WASTE HAZARD CODE
	CODE

	5344–82–1
	1-(o-chlorophenyl) 
	(Th)
	H026

	58-90-2
	2,3,4,6-Tetrachlorophenol
	(Th)
	H1000

	95-95-4
	2,4,5-Trichlorophenol
	(Th)
	H1001

	93-76-5
	2,4,5-Trichlorophenoxyacetic acid/2,4,5-T
	(Th)
	H1002

	88-06-2
	2,4,6-Trichlorophenol
	(Th)
	H1003

	51–28–5
	2,4-Dinitrophenol
	(Th)
	H048

	131–89–5
	2-Cychlohexil-4,6-dinitrophenol
	(Th)
	H034

	542–76–7
	3-Chloropropionitrile
	(Th)
	H027

	(1) 534–52–1
	4,6-Dinitro-o-cresol, and salts
	(Th)
	H047

	504–24–5
	4-Aminopiridine
	(Th)
	H008

	2763–96–4
	5-(Aminomethyl)-3-isoxazolol
	(Th)
	H007

	591–08–2
	Acetamide, G1159N-(aminothyoxomethyl)-/1-Acetyl-2-thiourea
	(Th)
	H002

	107–02–8
	Acrolein/2-Propenal
	(Th)
	H003

	116–06–3
	Aldicarb
	(Th)
	H070

	1646–88–4
	Aldicarb sulphone
	(Th)
	H203

	309–00–2
	Aldrin
	(Th)
	H004

	122–09–8
	alfa,alpha-Dimethylphenethylamine/Benzenethanamine, alpha, alpha-dimethyl 
	(Th)
	H046

	86–88–4
	alpha-Naphtilthiourea/Thiourea, 1-naphtalenile
	(Th)
	H072

	107–18–6
	Alilyc, alcohol/2-propen-1-ol
	(Th)
	H005

	20859–73–8
	Aluminum phosphorus
	(R,Th)
	H006

	131–74–8
	Ammonium picrate/phenyl, 2,4,6-trinitro-amonium salt.
	(R,Th)
	H009

	7803–55–6
	Ammonium vanadate
	(Th)
	H119

	7778–39–4
	Arsenic acid H3AsO4
	(Th)
	H010

	1327–53–3
	Arsenic oxide As2O3
	(Th)
	H012

	1303–28–2
	Arsénico oxide As2O5
	(Th)
	H011

	75–55–8
	Aziridine, 2-Methyl-/1,2-Propylenimine
	(Th)
	H067

	151–56–4
	Aziridine/Ethylenoimine
	(Th)
	H054

	542–62–1
	Barium cyanide 
	(Th)
	H013

	108–98–5
	Benzenthiol/ thiophenol
	(Th)
	H014

	100–44–7
	Benzyl chloride /chloromethylbenzene
	(Th)
	H028

	7440–41–7
	Berilium dust (all forms)
	(Th)
	H015

	598–31–2
	Bromoacetone/2-Propanone, 1-bromo-
	(Th)
	H017

	357–57–3
	Brucine
	(Th)
	H018

	592–01–8
	Calcium cyanide Ca(CN)2
	(Th)
	H021

	1563–66–2
	Carbophurane
	(Th)
	H127

	75–15–0
	Carbon disulfide 
	(Th)
	H022

	55285–14–8
	Carbosulfan
	(Th)
	H189

	74–90–8
	Hydrocyanic acid
	(Th)
	H063

	506–77–4
	Cyanogen chloride (CN) CI 
	(Th)
	H033

	460–19–5
	Cyanogen ethanedinitrile
	(Th)
	H031

	----
	Cyanide, soluble salts, (not specified in another way)
	(Th)
	H030

	107–20–0
	chloracetaldehyde
	(Th)
	H023

	544–92–3
	Copper cyanide Cu(CN)
	(Th)
	H029

	696–28–6
	dichlorophenylarsine
	(Th)
	H036

	542–88–1
	Dichloromethyl ether/methane oxybis
	(Th)
	H016

	60–57–1
	Dieldrin
	(Th)
	H037

	692–42–2
	diethylarsine
	(Th)
	H038

	311–45–5
	Diethyl-p-nitrophenyl phosphorus/ phosphorics, acid, diethyl-4-nitrophenyl ether
	(Th)
	H041

	55–91–4
	Diisopropyelfluorophosphorus (DFP) phosphorusfluorhydric acid, bid(1-methylethyl) ether
	(Th)
	H043

	644–64–4
	Dimethylamine
	(Th)
	H191

	60–51–5
	dimethoate
	(Th)
	H044

	88-85-7
	Dinoseb phenol,    2-(methylpropyl)-4,6-dinitrite
	(Th)
	H020

	298–04–4
	Disulfoton
	(Th)
	H039

	541–53–7
	Dithiobiurea
	(Th)
	H049

	115–29–7
	Endosulfan
	(Th)
	H050

	145–73–3
	Endothal
	(Th)
	H088

	(1) 72–20–8
	Endrin and its metabolites
	(Th)
	H051

	51–43–4
	Epinephrine
	(Th)
	H042

	(1) 57–24–9
	strychnine-10-ona and salts/strychnine and salts
	(Th)
	H108

	52–85–7
	Phamphur
	(Th)
	H097

	62–38–4
	Phenylmercuric acetate mercuric (acetate-o) phenyl
	(Th)
	H092

	103–85–5
	Phenyltiuorea
	(Th)
	H093

	57–47–6
	Physostigmine
	(Th)
	H204

	57–64–7
	Physostigmine salicylite
	(Th)
	H188

	7782–41–4
	Flourine
	(Th)
	H056

	640–19–7
	Fluuoroacetamida/2-fluoroacetamide
	(Th)
	H057

	62–74–8
	Fluoroaceti sodium acid
	(Th)
	H058

	298–02–2
	Phorate
	(Th)
	H094

	23422–53–9
	Formethanate hydrochloride
	(Th)
	H198

	17702–57–7
	Formica paranate
	(Th)
	H197

	7803–51–2
	Phosphine phosphydric acid
	(Th)
	H096

	75–44–5
	Phosgene
	(Th)
	H095

	76–44–8
	Heptachloride 
	(Th)
	H059

	757–58–4
	Hexaethyl tetraphosphate/ tetraphosphoric, acid hexaethyl ester
	(Th)
	H062

	465–73–6
	isodrine
	(Th)
	H060

	119–38–0
	Isolan
	(Th)
	H192

	15339–36–3
	Manganese dimethyldithiocarbomate
	(Th)
	H196

	64–00–6
	m-cumenyl methylcarbamato/3-isopropylphenyl n-methylcarbomate
	(Th)
	H202

	628-86-4
	Mercury fulminate
	(R,Th)
	H065

	60–34–4
	Methyl hydrazine
	(Th)
	H068

	624–83–9
	methyl isociantate/methane, isocianate-methyl
	(Th)
	H064

	298–00–0
	Methyl parathion/phosphorotioic acid, o,o-dimethyl o-(4-nitrophenyl) ester
	(Th)
	H071

	75–86–5
	Methylactonitrile/propanoitrile, 2-hydroxy-2-methyl 
	(Th)
	H069

	2032–65–7
	Methyocarb
	(Th)
	H199

	1129–41–5
	Metholcarb/ carbamic acid, methyl-, 3-methylphenyl esther.
	(Th)
	H190

	16752–77–5
	Methomyl
	(Th)
	H066

	315–8–4
	Mexacarbate
	(Th)
	H128

	(1) 54–11–5
	Nicotine salts/ pyridine, 3-(1- methyl-2- pyrrolidinyl)-,(s), and salts
	(Th)
	H075

	13463–39–3
	Nickel cyanide Ni(CO) 4, (t-4)- 
	(Th)
	H073

	557–19–7
	Nickel cyanide Ni(CN)2
	(Th)
	H074

	10102–43–9
	Nitrogen oxide nitric oxide (NO)
	(Th)
	H076

	10102–44–0
	Nitrogen dioxide
	(Th)
	H078

	55–63–0
	Nitroglycerin/ 1,2,3-propanetriol, trinitrate
	(E,Th)
	H081

	62–75–9
	n-nitrosodiethanolamine
	(Th)
	H082

	4549–40–0
	n-nitrosodiethylamine
	(Th)
	H084

	297–97–2
	O,o-diethyl o-pyrazinil phosphorothioate
	(Th)
	H040

	152–16–9
	Octamethylpirophosphoramide/ octamethyl diphosphoramide 
	(Th)
	H085

	20816–12–0
	Osmium oxide OsO4, (T-4)-
	(Th)
	H087

	23135–22–0
	Oxamil
	(Th)
	H194

	56–38–2
	Parathion
	(Th)
	H089

	106–47–8
	p-chloroaniline/4-chloro benzenamine
	(Th)
	H024

	87-86-5
	Pentachlorophenol
	(Th)
	H1004

	506–64–9
	Silver cyanide Ag(CN)
	(Th)
	H104

	78–00–2
	Plumbane tetraethyl-/ tetraethyl lead
	(Th)
	H110

	100–01–6
	p-nitroaniline / 4-nitro-benzenamine
	(Th)
	H077

	151–50–8
	Potassium, cyanide  K(CN) 
	(Th)
	H098

	506–61–6
	Silver  potassium cyanide/Argentate(1-), bis(cyano-c)-, potassium
	(Th)
	H099

	2631–37–0
	Promecarb/phenol, 3-methyl-5-(1-methyethyll)-, methyl carbamate
	(Th)
	H201

	107–12–0
	Propanonitrile
	(Th)
	H101

	107–19–7
	Propargil alcohol/2-Propin-1-ol
	(Th)
	H102

	630–10–4
	Selenourea
	(Th)
	H103

	93-72-1
	Silbes (2,4,5-TP) propanoic acid 2-(2,4,5,-trichlorophenoxyl)-
	(Th)
	H1005

	26628–22–8
	Sodium azide
	(Th)
	H105

	143–33–9
	Sodium cyanide Na(CN) 
	(Th)
	H106

	1314–32–5
	Thallium oxide/thallic oxide Tl2O3
	(Th)
	H113

	12039–52–0
	Thallium selenite 
	(I,Th)
	H114

	7446–18–6
	Thallium sulfate
	(I,Th)
	H115

	107–49–3
	Tetraethylpyrophosphate / diphosphoric  acid tetraethyl esther
	(Th)
	H111

	3689–24–5
	Tetraethyldithiopyrosphosphate / thiodiophosphoric acid tetraethyl ester
	(Th)
	H109

	509–14–8
	Tetranitromethane
	(R,Th)
	H112

	39196–18–4
	Thiophanax
	(Th)
	H045

	79–19–6
	Thiosemicarbazide/ hydrazinacarbothiomide
	(Th)
	H116

	26419–73–8
	Thirphate
	(Th)
	H185

	8001–35–2
	toxaphene
	(Th)
	H123

	75–70–7
	trichloromethanethiol
	(Th)
	H118

	1314–62–1
	Vanadium oxide V2O5
	(Th)
	H120

	(1) 81–81–2
	warpharin  and salts, when they are present in concentrations greater than 0.3% 
	(Th)
	H001

	557–21–1
	Zinc cyanide Zn(CN)2
	(Th)
	H121

	1314–84–7
	Zinc phosphuros Zn3P2, when it is present in concentrations greater than 10% 
	(R,Th)
	H122

	137-30-4
	Ziram
	(Th)
	H205

	1.- In the case of familias of isomers from organic compounds, only the name of the group is mentioned, all the isomers must be considered toxic compounds (p.e. dichlorobenzenes, includes 1.2, 1.3, and 1.4 dichlorobenzenes). 



	2.- the 1 indicates the CAS number of an equivalent compound


	LISTADO 4



	CLASIFICACION DE RESIDUOS PELIGROSOS RESULTADO DEL DESECHO DE PRODUCTOS QUIMICOS FUERA DE ESPECIFICACIONES O CADUCOS (TOXICOS CRONICOS)



	No. CAS
	Nombre
	CPR
	Clave

	630–20–6
	1,1,1,2-Tetracloroetano
	(Tt)
	T208

	79–34–5
	1,1,2,2-Tetracloroetano
	(Tt)
	T209

	79–00–5
	1,1,2-Tricloroetano
	(Tt)
	T227

	75–35–4
	1,1-Dicloroetileno
	(Tt)
	T078

	57–14–7
	1,1-Dimetilhidracina
	(Tt)
	T098

	95–94–3
	1,2,4,5-Tetraclorobenceno
	(Tt)
	T207

	1464–53–5
	1,2:3,4-Diepoxibutano 
	(I,Tt)
	T085

	96–12–8
	1,2-Dibromo-3-cloropropano
	(Tt)
	T066

	106-93-4
	1,2-Dibromoetano
	(Tt)
	T067

	122–66–7
	1,2-Difenilhidracina
	(Tt)
	T109

	540–73–8
	1,2-Dimetilhidracina
	(Tt)
	T099

	99–35–4
	1,3,5-Trinitrobenceno 
	(R,Tt)
	T234

	542–75–6
	1,3-Dicloropropileno/1-Propileno, 1,3-dicloro-
	(Tt)
	T084

	1120–71–4
	1,3-Propano sultona/1,2-Oxatiolano, 2,2-dióxido
	(Tt)
	T193

	764–41–0
	1,4-Dicloro-2-butileno 
	(I,Tt)
	T074

	123-91-1
	1,4-Dioxano/1,4-Dietilenóxido
	(Tt)
	T108

	130–15–4
	1,4-Naftoquinona/1,4-Naftalendiona
	(Tt)
	T166

	504–60–9
	1-Metilbutadieno/1,3-Pentadieno
	(I,Tt)
	T186

	118–79–6
	2,4,6-Tribromofenol
	(Tt)
	T408

	120–83–2
	2,4-Diclorofenol
	(Tt)
	T081

	(1) 94-75-7
	2,4-Diclorofenoxiacético ácido/2,4-D, sales y ésteres
	(Tt)
	T240

	121–14–2
	2,4-Dinitrotolueno
	(Tt)
	T105

	106–51–4
	2,5-Ciclohexadien-1,4-diona
	(Tt)
	T197

	87–65–0
	2,6-Diclorofenol
	(Tt)
	T082

	606–20–2
	2,6-Dinitrotolueno/2-metil-1,3-dinitrobenceno
	(Tt)
	T106

	105-67-9
	2-4-Dimetil fenol
	(Tt)
	T101

	53-96-3
	2-Acetilaminofluoreno/acetamida, n-9h-fluoren-2-il-
	(Tt)
	T005

	110–75–8
	2-Cloroetil vinil éter/eteno, (2-cloroetoxi)- 
	(Tt)
	T042

	91-58-7
	2-Cloronaftaleno/beta-Cloronaftaleno
	(Tt)
	T047

	79–46–9
	2-Nitropropano 
	(I,Tt)
	T171

	109–06–8
	2-Picolina/Piridina, 2-metil-
	(Tt)
	T191

	91–94–1
	3,3'-Diclorobenzidina
	(Tt)
	T073

	119–93–7
	3,3'-Dimetilbenzidina
	(Tt)
	T095

	119–90–4
	3,3'-Dimetoxibenzidina
	(Tt)
	T091

	56–49–5
	3-Metilclorantreno
	(Tt)
	T157

	101-14-4
	4,4'-Metilenbis(2-cloroanilina)
	(Tt)
	T158

	3165-93-3
	4-Cloro-o-toluidina, hidrocloruro de
	(Tt)
	T049

	99–55–8
	5-Nitro-o-toluidina
	(Tt)
	T181

	57–97–6
	7,12-Dimetilbenzo[a]antraceno
	(Tt)
	T094

	30558-43-1
	A2213/Etanimidotioico ácido, 2-(Dimetilamino)-n-hidroxi-2-oxo-, metil éster
	(Tt)
	T394

	75-36-5
	Acetilo, cloruro de 
	(C,R,Tt)
	T006

	98-86-2
	Acetofenona/1-Fenil-etanona
	(Tt)
	T004

	67-64-1
	Acetona
	(I,Tt)
	T002

	75-05-8
	Acetonitrilo/2-Propanona
	(I,Tt)
	T003

	79-06-1
	Acrilamida/2-Propenamida
	(Tt)
	T007

	79–10–7
	Acrílico ácido/2-Propenoico ácido
	(I,Tt)
	T008

	107-13-1
	Acrilonitrilo/2-Propennitrilo
	(Tt)
	T009

	80–15–9
	alfa,alfa-Dimetil bencilhidroperóxido
	(R,Tt)
	T096

	134–32–7
	alfa-Naftilamina/1-Naftalenamina
	(Tt)
	T167

	61–82–5
	Amitrol/1H-1,2,4-Triazol-3-amina
	(Tt)
	T011

	62-53-3
	Anilina/Bencenamina
	(I,Tt)
	T012

	492-80-8
	Auramina
	(Tt)
	T014

	115–02–6
	Azaserina/L-serina, diazoacetato(éster)
	(Tt)
	T015

	101-27-9
	Barban
	(Tt)
	T280

	71-43-2
	Benceno
	(I,Tt)
	T019

	72-43-5
	Benceno, 1,1’-(2,2,2-tricloroetiliden)bis[4-metoxi-
	(Tt)
	T247

	98-09-9
	Bencensulfonilo, cloruro de 
	(C,R,Tt)
	T020

	22781-23-3
	Bendiocarb
	(Tt)
	T278

	22961-82-6
	Bendiocarb fenol
	(Tt)
	T364

	17804-35-2
	Benomil
	(Tt)
	T271

	98-87-3
	Benzal, cloruro de/Diclorometilbenceno
	(Tt)
	T017

	92-87-5
	Benzidina/[1,1'-Bifenil]-4,4'-diamina
	(Tt)
	T021

	56-55-3
	Benzo(a)antraceno
	(Tt)
	T018

	50-32-8
	Benzo(a)pireno
	(Tt)
	T022

	225-51-4
	Benzo(c)acridina
	(Tt)
	T016

	98-07-7
	Benzotricloro/Triclorometilbenceno
	(C,R,Tt)
	T023

	91–59–8
	Beta-Naftilamina/2-Naftalenamina/2-Naftilamina
	(Tt)
	T168

	101-55-3
	Bromofenil fenil éter
	(Tt)
	T030

	74-83-9
	Bromometano/Bromuro de metilo
	(Tt)
	T029

	75–60–5
	Cacodílico, ácido
	(Tt)
	T136

	13765–19–0
	Calcio, cromato de
	(Tt)
	T032

	111–54–6
	Carbamoditioico, ácido, 1,2-etanodiilbis, sales y ésteres/Etilenbisditiocarbámico, ácido, sales y ésteres
	(Tt)
	T114

	63–25–2
	Carbaril
	(Tt)
	T279

	10605–21–7
	Carbendazim
	(Tt)
	T372

	1563–38–8
	Carbofurano fenol
	(Tt)
	T367

	56–23–5
	Carbono, tetracloruro de/Tetraclorometano
	(Tt)
	T211

	353–50–4
	Carbono, oxifluoruro de 
	(R,Tt)
	T033

	506–68–3
	Cianógeno, bromuro de (CN)Br
	(Tt)
	T246

	50–18–0
	Ciclofosfamida
	(Tt)
	T058

	110–82–7
	Ciclohexano
	(I,Tt)
	T056

	108–94–1
	Ciclohexanona 
	(I,Tt)
	T057

	75–87–6
	Cloral/Acetaldehído, tricloro 
	(Tt)
	T034

	305–03–3
	Clorambucil
	(Tt)
	T035

	57–74–9
	Clordano, alfa y gamma isómeros
	(Tt)
	T036

	494–03–1
	Clornafacina/Naftalenamina, n,n'-bis(2-Cloroetil)-
	(Tt)
	T026

	108–90–7
	Clorobenceno
	(Tt)
	T037

	510–15–6
	Clorobenzilato
	(Tt)
	T038

	67–66–3
	Cloroformo/Triclorometano
	(Tt)
	T044

	107–30–2
	Clorometil metil éter/Clorometoximetano
	(Tt)
	T046

	8001-58-9
	Creosota
	(Tt)
	T051

	1319–77–3
	Cresol (cresílico ácido)/Metilfenol
	(Tt)
	T052

	218–01–9
	Criseno
	(Tt)
	T050

	4170–30–3
	Crotonaldehído/2-Butenal
	(Tt)
	T053

	98–82–8
	Cumeno/Benceno, (1-metiletil)- 
	(Tt)
	T055

	20830–81–3
	Daunomicina
	(Tt)
	T059

	72-54-8
	DDD
	(Tt)
	T060

	50-29-3
	DDT
	(Tt)
	T061

	2303–16–4
	Dialato
	(Tt)
	T062

	53–70–3
	Dibenz[a,h]antraceno
	(Tt)
	T063

	189–55–9
	Dibenzo[a,i]pireno
	(Tt)
	T064

	84-74-2
	Dibutil ftalato
	(Tt)
	T069

	75–71–8
	Diclorodifluorometano
	(Tt)
	T075

	111-44-4
	Dicloroetil éter/Etano, 1,1’-oxibis[2-cloro-
	(Tt)
	T025

	108–60–1
	Dicloroisopropil éter/Propano, 2,2'-oxibis[2-cloro-
	(Tt)
	T027

	111–91–1
	Diclorometoxi etano
	(Tt)
	T024

	84–66–2
	Dietil ftalato
	(Tt)
	T088

	5952–26–1
	Dietilen glicol, dicarbamato/Etanol, 2,2’-oxibis-, dicarbamato
	(Tt)
	T395

	117-81-7
	Dietilhexil ftalato
	(Tt)
	T028

	56–53–1
	Dietilstilbesterol/Fenol, 4,4’-(1,2-dietil- 1,2-etenediil)bis-
	(Tt)
	T089

	94–58–6
	Dihidrosafrole
	(Tt)
	T090

	131–11–3
	Dimetil ftalato
	(Tt)
	T102

	77–78–1
	Dimetil sulfato/Sulfúrico ácido, Dimetil éster
	(Tt)
	T103

	124–40–3
	Dimetilamina/Metanamina, n-metil 
	(I,Tt)
	T092

	79–44–7
	Dimetilcarbamil, cloruro de/Carbámico cloruro de, dimetil 
	(Tt)
	T097

	117–84–0
	Di-n-octil ftalato
	(Tt)
	T107

	621–64–7
	Di-n-propilnitrosamina/1-Propanamina, n-nitroso-n-propil-
	(Tt)
	T111

	142–84–7
	Dipropilamina/1-Propanamina, n-propil-
	(I,Tt)
	T110

	106–89–8
	Epiclorohidrín/Oxirano, (clorometil)-2-
	(Tt)
	T041

	18883–66–4
	Estreptozotocina/D-glucosa, 2-deoxi-2-[[(metilnitrosoamino)-carbonoil]amino]
	(Tt)
	T206

	75–07–0
	Etanal/Acetaldehído
	(I,Tt)
	T001

	127–18–4
	Eteno, tetracloro- 
	(Tt)
	T210

	51-79-6
	Etil carbamato (uretano)/Carbámico ácido, etil éster
	(Tt)
	T238

	60-29-7
	Etil éter
	(I,Tt)
	T117

	97-63-2
	Etil metacrilato/2-Propenoico ácido, 2-metil-, etil éster
	(Tt)
	T118

	62-50-0
	Etil metanosulfonato/Metanosulfónico ácido, etil éster
	(Tt)
	T119

	110–80–5
	Etilen glicol monoetil éter/Etanol, 2-etoxi- 
	(Tt)
	T359

	107-06-2
	Etileno dicloruro de/1,2-Dicloroetano
	(Tt)
	T077

	96–45–7
	Etilenthiourea/2-imidazolidintiona
	(Tt)
	T116

	75–34–3
	Etilideno, dicloruro de/Etano 1,1-dicloro- 
	(Tt)
	T076

	141–78–6
	Etilo, acetato de/Acético ácido, etil éster
	(I,Tt)
	T112

	140–88–5
	Etilo, acrilato de/2-Propenoico ácido, etil éster
	(I,Tt)
	T113

	62–44–2
	Fenacetina
	(Tt)
	T187

	108–95–2
	Fenol
	(Tt)
	T188

	206–44–0
	Fluoranteno
	(Tt)
	T120

	7664–39–3
	Fluorhídrico, ácido 
	(C,Tt)
	T134

	50–00–0
	Formaldehído
	(Tt)
	T122

	64–18–6
	Fórmico, ácido 
	(C,Tt)
	T123

	1314–80–3
	Fósforo, sulfuro de 
	(R,Tt)
	T189

	85–44–9
	Ftálico anhídrido/1,3-Isobenzofurandiona
	(Tt)
	T190

	98–01–1
	Furfural
	(I,Tt)
	T125

	110–00–9
	Furfurano/Furan
	(I,Tt)
	T124

	58-89-9
	Gamma-BHC/Lindano
	(Tt)
	T129

	118–74–1
	Hexaclorobenceno
	(Tt)
	T127

	87–68–3
	Hexaclorobutadieno/1,3-Butadieno, 1,1,2,3,4,4-hexacloro
	(Tt)
	T128

	77–47–4
	Hexaclorociclopentadieno/1,3-Ciclopentadieno, 1,2,3,4,5,5-hexacloro-
	(Tt)
	T130

	67–72–1
	Hexacloroetano
	(Tt)
	T131

	70–30–4
	Hexaclorofeno/2,2’-Metilenobis[3,4,6-triclorofenol
	(Tt)
	T132

	1888–71–7
	Hexacloropropeno/1-Propeno, 1,1,2,3,3,3-hexacloro-
	(Tt)
	T243

	302–01–2
	Hidrazina 
	(R,Tt)
	T133

	1615–80–1
	Hidrazina, 1,2-dietil-
	(Tt)
	T086

	193–39–5
	Indeno[1,2,3-cd]pireno
	(Tt)
	T137

	78–83–1
	Isobutil alcohol/1-Propanol, 2-metil-
	(I,Tt)
	T140

	120–58–1
	Isosafrola
	(Tt)
	T141

	143–50–0
	Kepona
	(Tt)
	T142

	303–34–1
	Lasiocarpina
	(Tt)
	T143

	123–33–1
	Maleica, hidracida/3,6-Piridazinediona, 1,2-dihidro-, 
	(Tt)
	T148

	108–31–6
	Maleico, anhídrido/2,5-Furandiona
	(Tt)
	T147

	109–77–3
	Malononitrilo/Propanodinitrilo
	(Tt)
	T149

	541–73–1
	M-diclorobenceno/Benceno, 1,3-dicloro-
	(Tt)
	T071

	148–82–3
	Melfalan/L-fenilalanina, 4-[bis(2-Cloroetil)amino] 
	(Tt)
	T150

	7439-97-6
	Mercurio (todas las formas)
	(Tt)
	T151

	126–98–7
	Metacrilonitrilo/2-Propenenitrilo, 2-metil
	(I,Tt)
	T152

	67–56–1
	Metanol 
	(I,Tt)
	T154

	91–80–5
	Metapirileno
	(Tt)
	T155

	79–22–1
	Metil clorocarbonato/carbonoclorídico ácido, metil éster
	(I,Tt)
	T156

	71-55-6
	Metil cloroformo/1,1,1-tricloroetano
	(Tt)
	T226

	78–93–3
	Metil etil cetona (MEK)/2-butanona 
	(I,Tt)
	T159

	1338–23–4
	Metil etil cetona peróxido/2-butanona, peróxido
	(R,Tt)
	T160

	108–10–1
	Metil isobutil cetona/4-Metil-2-pentanona/4-Metilpentanol
	(I,Tt)
	T161

	80–62–6
	Metil metacrilato/2-Propenoico ácido, 2-metil-, metil éster
	(I,Tt)
	T162

	74-95-3
	Metileno bromuro de 
	(Tt)
	T068

	75–09–2
	Metileno cloruro de/Metano, dicloro-
	(Tt)
	T080

	74-87-3
	Metilo cloruro de
	(I,Tt)
	T045

	74-88-4
	Metilo, ioduro de
	(Tt)
	T138

	56–04–2
	Metiltiouracilo
	(Tt)
	T164

	2385-85-5
	Mirex 
	(Tt)
	T1000

	50–07–7
	Mitomicín C
	(Tt)
	T010

	70–25–7
	MNNG/Guanidina, n-metil-n'-nitro-n-nitroso-
	(Tt)
	T163

	91–20–3
	Naftaleno
	(Tt)
	T165

	71–36–3
	n-Butil alcohol/1-Butanol
	(I,Tt)
	T031

	98–95–3
	Nitrobenceno 
	(I,Tt)
	T169

	1116–54–7
	n-Nitrosodietanolamina
	(Tt)
	T173

	55–18–5
	n-Nitrosodietilamina
	(Tt)
	T174

	924–16–3
	n-Nitrosodi-n-butilamina
	(Tt)
	T172

	759–73–9
	n-Nitroso-n-etilurea
	(Tt)
	T176

	684–93–5
	n-Nitroso-n-metilurea
	(Tt)
	T177

	615–53–2
	n-Nitroso-n-metiluretano/Carbámico ácido, metilnitroso-, etil éster
	(Tt)
	T178

	100–75–4
	n-Nitrosopiperidina/Piperidina, 1-nitroso
	(Tt)
	T179

	930–55–2
	n-Nitrosopirrolidina/Pirrolidina, 1-nitroso
	(Tt)
	T180

	107–10–8
	n-Propilamina/1-Propanamina
	(I,Tt)
	T194

	3288–58–2
	o,o-dietil s-metil ditiofosfato
	(Tt)
	T087

	95-57-8
	o-Clorofenol/2-Clorofenol
	(Tt)
	T048

	95–50–1
	o-Diclorobenceno
	(Tt)
	T070

	95–53–4
	o-Toluidina
	(Tt)
	T328

	636-21-5
	o-Toluidina, hidrocloruro de 
	(Tt)
	T222

	75–21–8
	Oxirano/Etileno, óxido de 
	(I,Tt)
	T115

	765–34–4
	Oxiranocarboxialdehído/Glicidilaldehído
	(Tt)
	T126

	123–63–7
	Paraldehído/1,3,5-Trioxano, 2,4,6-trimetil-
	(Tt)
	T182

	59–50–7
	p-Cloro-m-cresol/4-Cloro-3-metilfenol
	(Tt)
	T039

	106–46–7
	p-Diclorobenceno
	(Tt)
	T072

	60–11–7
	p-Dimetilaminoazobenceno
	(Tt)
	T093

	608–93–5
	Pentaclorobenceno
	(Tt)
	T183

	76–01–7
	Pentacloroetano
	(Tt)
	T184

	82–68–8
	Pentacloronitrobenceno (PCNB)
	(Tt)
	T185

	110–86–1
	Piridina
	(Tt)
	T196

	1335–32–6
	Plomo, subacetato/Plomo, bis(acetato-o)tetrahidroxitri-
	(Tt)
	T146

	301–04–2
	Plomo, acetato de 
	(Tt)
	T144

	7446–27–7
	Plomo, fosfato de 
	(Tt)
	T145

	100–02–7
	p-Nitrofenol/4-Nitrofenol
	(Tt)
	T170

	122–42–9
	Profam/Carbámico ácido, fenil-,1-metiletil éster
	(Tt)
	T373

	23950–58–5
	Pronamida
	(Tt)
	T192

	78-87-5
	Propileno, dicloruro de/1,2-Dicloropropano
	(Tt)
	T083

	114–26–1
	Propoxur/Fenol, 2-(1-metiletoxi)-, metilcarbamato
	(Tt)
	T411

	52888–80–9
	Prosulfocarb/Carbamotioico ácido, dipropil-, s-(fenilmetil) éster
	(Tt)
	T387

	106–49–0
	p-Toluidina
	(Tt)
	T353

	50–55–5
	Reserpina
	(Tt)
	T200

	108–46–3
	Resorcinol
	(Tt)
	T201

	(1) 81–07–2
	Sacarina, y sales/1,2-Benzisotiazol-3(2h)-ona, 1,1-dióxido, y sales
	(Tt)
	T202

	94–59–7
	Safrole
	(Tt)
	T203

	7783–00–8
	Selenio, dióxido de 
	(Tt)
	T204

	7488–56–4
	Selenio, sulfuro de SeS2
	(R,Tt)
	T205

	7783–06–4
	Sulfhídrico, ácido 
	(Tt)
	T135

	563–68–8
	Talio, acetato de 
	(I,Tt)
	T214

	6533–73–9
	Talio, carbonato de/Carbonoico ácido, ditalio(1+) sal
	(I,Tt)
	T215

	7791–12–0
	Talio, cloruro de 
	(Tt)
	T216

	10102–45–1
	Talio, nitrato de/Nítrico ácido, sal de talio (1+)
	(I,Tt)
	T217

	127–18–4
	Tetracloroetileno
	(Tt)
	T210

	109–99–9
	Tetrahidrofurano 
	(I,Tt)
	T213

	62–55–5
	Tioacetamida/Etanotioamida
	(Tt)
	T218

	59669–26–0
	Tiodicarb
	(Tt)
	T410

	23564–05–8
	Tiofanato-metil
	(Tt)
	T409

	74–93–1
	Tiometanol/Metanotiol
	(I,Tt)
	T153

	62–56–6
	Tiourea
	(Tt)
	T219

	137–26–8
	Tiram
	(Tt)
	T244

	25376–45–8
	Toluendiamina
	(Tt)
	T221

	26471–62–5
	Tolueno, diisocianato de
	(R,Tt)
	T223

	108–88–3
	Tolueno/Metilbenceno
	(Tt)
	T220

	156-60-5
	Trans-1,2-dicloroetileno/1,2-dicloroetileno
	(Tt)
	T079

	2303–17–5
	Trialato
	(Tt)
	T389

	75-25-2
	Tribromometano/Bromoformo
	(Tt)
	T225

	79–01–6
	Tricloroetileno
	(Tt)
	T228

	75–69–4
	Tricloromonofluorometano
	(Tt)
	T121

	121–44–8
	Trietilamina/Etanamina, n,n-dietil-
	(I,Tt)
	T404

	72–57–1
	Tripan, azul de 
	(Tt)
	T236

	126–72–7
	Tris (2,3-dibromopropil) fosfato/1-propanol, 2,3-dibromo-, fosfato (3:1)
	(Tt)
	T235

	66–75–1
	Uracilo, mostaza de 
	(Tt)
	T237

	75–01–4
	Vinilo, cloruro de/Cloroeteno
	(Tt)
	T043

	(1) 81–81–2
	Warfarina, y sales, cuando están presentes en concentraciones menores que 0.3%
	(Tt)
	T248

	1330–20–7
	Xileno, isómeros
	(Tt)
	T239

	1314–84–7
	Zinc, fosfuro de Zn3P2, cuando está presente en concentraciones menores o iguales a 10%
	(Tt)
	T249

	NOTAS:

	1.- En el caso de familias de isómeros de compuestos orgánicos, sólo se menciona el nombre del grupo, todos los isómeros se deben considerar constituyentes tóxicos (p.e. diclorobencenos, incluye al 1,2 1,3 y 1,4 diclorobencenos).

	2.- La llamada (1) indica el número CAS de un compuesto equivalente.
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	CLASSIFICATION OF HAZARDOUS WASTES RESULTING FORM THE WASTE FROM CHEMICAL PRODUCTS OUTSIDE OF SPECIFICATIONS OR EXPIRED (CHRONIC TOXICS) 



	CAS
	NAME
	CPR
	CODE

	630–20–6
	1,1,1,2-Tetrachlorethane
	(Tt)
	T208

	79–34–5
	1,1,2,2-Tetrachlorethane
	(Tt)
	T209

	79–00–5
	1,1,2-Trichloroethane
	(Tt)
	T227

	75–35–4
	1,1-Dichloroethylene
	(Tt)
	T078

	57–14–7
	1,1-Dimethylhidracine
	(Tt)
	T098

	95–94–3
	1,2,4,5-Tetrachlorobenzene
	(Tt)
	T207

	1464–53–5
	1,2:3,4-Diepoxybutane 
	(I,Tt)
	T085

	96–12–8
	1,2-Dibromo-3-chloropropane
	(Tt)
	T066

	106-93-4
	1,2-Dibromoethanol
	(Tt)
	T067

	122–66–7
	1,2-Difenilhydracine
	(Tt)
	T109

	540–73–8
	1,2-Dimethylhydracine
	(Tt)
	T099

	99–35–4
	1,3,5-Trinitrobenzene 
	(R,Tt)
	T234

	542–75–6
	1,3-Dichloropropilene/1-Propilene, 1,3-dichloro-
	(Tt)
	T084

	1120–71–4
	1,3-Propane sultone/1,2-Oxathiolane, 2,2-dioxide
	(Tt)
	T193

	764–41–0
	1,4-Dichloro-2-butylene 
	(I,Tt)
	T074

	123-91-1
	1,4-Dioxane/1,4-Diethylene oxide
	(Tt)
	T108

	130–15–4
	1,4-Naphtoquinone/1,4-Naphtalendione
	(Tt)
	T166

	504–60–9
	1- methyl butadiene/1,3-Pentadiene
	(I,Tt)
	T186

	118–79–6
	2,4,6-Tribromophenol
	(Tt)
	T408

	120–83–2
	2,4-Dichlorophenol
	(Tt)
	T081

	(1) 94-75-7
	2,4-Diclorophenoxiacetic acid/2,4-D, salts and esters
	(Tt)
	T240

	121–14–2
	2,4-Dinitrotoluene
	(Tt)
	T105

	106–51–4
	2,5-cyclohexadiene-1,4-dione
	(Tt)
	T197

	87–65–0
	2,6-Dichlorophenol
	(Tt)
	T082

	606–20–2
	2,6-Dinitrotoluene/2-methyl-1,3-dinitrobenzene
	(Tt)
	T106

	105-67-9
	2-4-Dimethyl phenol
	(Tt)
	T101

	53-96-3
	2-Acetilaminofluorene/acetamide, n-9h-fluorene-2-il-
	(Tt)
	T005

	110–75–8
	2-Cloroethyl vinyl ether/etene, (2-cloro etoxy)- 
	(Tt)
	T042

	91-58-7
	2-Cloronaphatalene/beta-Cloronaphatalene
	(Tt)
	T047

	79–46–9
	2-Nitropropane 
	(I,Tt)
	T171

	109–06–8
	2-Picoline/Piridine, 2-methyl-
	(Tt)
	T191

	91–94–1
	3,3'-Dichlorobenzidine
	(Tt)
	T073

	119–93–7
	3,3'-Dimethylbenzidine
	(Tt)
	T095

	119–90–4
	3,3'-Dimetoxybenzidine
	(Tt)
	T091

	56–49–5
	3-Methylchloranthene
	(Tt)
	T157

	101-14-4
	4,4'-Methylenbis(2-chloroaniline)
	(Tt)
	T158

	3165-93-3
	4-Chloro-o-toluidine, hydrochloride
	(Tt)
	T049

	99–55–8
	5-Nitro-o-toluidine
	(Tt)
	T181

	57–97–6
	7,12-Dimethylbenzo[a]anthracene
	(Tt)
	T094

	30558-43-1
	A2213/Ethanimidothioic acid, 2-(Dimethylamine)-n-hidroxy-2-oxo-, methyl ester
	(Tt)
	T394

	75-36-5
	Acetyl chloride
	(C,R,Tt)
	T006

	98-86-2
	Acetophenone/1-phenyl-ethanone
	(Tt)
	T004

	67-64-1
	Acetone
	(I,Tt)
	T002

	75-05-8
	Acetonitrile/2-Propanone
	(I,Tt)
	T003

	79-06-1
	Acrilamide/2-Propenamide
	(Tt)
	T007

	79–10–7
	Acrylic acid/2-Propenoic acid
	(I,Tt)
	T008

	107-13-1
	Acrilonitrile/2-Propennitrile
	(Tt)
	T009

	80–15–9
	alpha,alpha-Dimethyl benzylhydroperoxide
	(R,Tt)
	T096

	134–32–7
	alpha-Naphtalamine/1-Naphtalenamine
	(Tt)
	T167

	61–82–5
	Amitrol/1H-1,2,4-Triazol-3-amine
	(Tt)
	T011

	62-53-3
	Aniline/Benzenamine
	(I,Tt)
	T012

	492-80-8
	Auramine
	(Tt)
	T014

	115–02–6
	Azaserine/L-serine, diazoacetate(ester)
	(Tt)
	T015

	101-27-9
	Barban
	(Tt)
	T280

	71-43-2
	Benzene
	(I,Tt)
	T019

	72-43-5
	Benzene, 1,1’-(2,2,2-trichloroethyliden)bis[4-metoxy-
	(Tt)
	T247

	98-09-9
	Benzensulphonile chloride 
	(C,R,Tt)
	T020

	22781-23-3
	Bendiocarb
	(Tt)
	T278

	22961-82-6
	Bendiocarb phenol
	(Tt)
	T364

	17804-35-2
	Benomil
	(Tt)
	T271

	98-87-3
	Benzal, chloride/Dichloromethylbenzene
	(Tt)
	T017

	92-87-5
	Benzidine/[1,1'-Biphenyl]-4,4'-diamine
	(Tt)
	T021

	56-55-3
	Benzo(a)anthracene
	(Tt)
	T018

	50-32-8
	Benzo(a)pyrene
	(Tt)
	T022

	225-51-4
	Benzo(c)acridine
	(Tt)
	T016

	98-07-7
	Benzotrichloro/Trichloromethylbenzene
	(C,R,Tt)
	T023

	91–59–8
	Beta-Naphtalamine/2-Naphtalenamine/2-Naphtalamine
	(Tt)
	T168

	101-55-3
	Bromophenyl phenyl ether
	(Tt)
	T030

	74-83-9
	Bromomethane/Methyl bromide
	(Tt)
	T029

	75–60–5
	Cacodilic, acid
	(Tt)
	T136

	13765–19–0
	Calcium, chromate 
	(Tt)
	T032

	111–54–6
	Carbamodithioic acid, 1,2-ethanodiilbis, salts and esters/Ethylenbisdithiocarbamic acid, salts and esters
	(Tt)
	T114

	63–25–2
	Carbaril
	(Tt)
	T279

	10605–21–7
	Carbendazim
	(Tt)
	T372

	1563–38–8
	Carbofuran, phenol
	(Tt)
	T367

	56–23–5
	Carbon tetrachloruride/Tetrachloromethane
	(Tt)
	T211

	353–50–4
	Carbon oxyfluoride 
	(R,Tt)
	T033

	506–68–3
	Cyangen bromide (CN)Br
	(Tt)
	T246

	50–18–0
	Cyclophosphamide
	(Tt)
	T058

	110–82–7
	Cyclohexane
	(I,Tt)
	T056

	108–94–1
	Cyclohexanone 
	(I,Tt)
	T057

	75–87–6
	Chloral/Acetaldehyde, trichloro 
	(Tt)
	T034

	305–03–3
	Chlorambucil
	(Tt)
	T035

	57–74–9
	Chlordane, alpha and gamma isomers
	(Tt)
	T036

	494–03–1
	Chlornaphacine/Naphtalenamine, n,n'-bis(2-Cloroethyl)-
	(Tt)
	T026

	108–90–7
	Chlorobenzene
	(Tt)
	T037

	510–15–6
	Clorobenzilate
	(Tt)
	T038

	67–66–3
	Chloroform/Trichloromethane
	(Tt)
	T044

	107–30–2
	Cloromethyl methyl ether/Clorometoxymethane
	(Tt)
	T046

	8001-58-9
	creosote
	(Tt)
	T051

	1319–77–3
	Cresol (cresílic acid)/Methylphenol
	(Tt)
	T052

	218–01–9
	Crisene
	(Tt)
	T050

	4170–30–3
	Chrotonaldehyde/2-Butenal
	(Tt)
	T053

	98–82–8
	Cumene/Benzene, (1-methylethyl)- 
	(Tt)
	T055

	20830–81–3
	Daunomicine
	(Tt)
	T059

	72-54-8
	DDD
	(Tt)
	T060

	50-29-3
	DDT
	(Tt)
	T061

	2303–16–4
	Dialate
	(Tt)
	T062

	53–70–3
	Dibenz[a,h]anthracene
	(Tt)
	T063

	189–55–9
	Dibenzo[a,i]pyrene
	(Tt)
	T064

	84-74-2
	Dibutyl phtalate
	(Tt)
	T069

	75–71–8
	Dichlorodifluoromethane
	(Tt)
	T075

	111-44-4
	Dichloroethyl ether/Ethane, 1,1’-oxibis[2-chloro-
	(Tt)
	T025

	108–60–1
	Dichloroisopropyl ether/Propane, 2,2'-oxibis[2-chloro-
	(Tt)
	T027

	111–91–1
	Dichlorometoxy ethane
	(Tt)
	T024

	84–66–2
	Diethyl phtalate
	(Tt)
	T088

	5952–26–1
	Diethylen glycol, dicarbamate/Ethanol, 2,2’-oxibis-, dicarbamate
	(Tt)
	T395

	117-81-7
	Diethylhexyl phtalate
	(Tt)
	T028

	56–53–1
	Diethylstilbesterol/Phenol, 4,4’-(1,2-diethyl- 1,2-etenediil)bis-
	(Tt)
	T089

	94–58–6
	Dihidrosafrole
	(Tt)
	T090

	131–11–3
	Dimethyl phtalate
	(Tt)
	T102

	77–78–1
	Dimethyl sulphate/Sulfuric acid, Dimethyl ester
	(Tt)
	T103

	124–40–3
	Dimethylamine/Metanamina, n-methyl 
	(I,Tt)
	T092

	79–44–7
	Dimethylcarbamil, chloride/Carbamic chloride, dimethyl 
	(Tt)
	T097

	117–84–0
	Di-n-octyl phtalate
	(Tt)
	T107

	621–64–7
	Di-n-propylnitrosamine/1-Propanamine, n-nitrose-n-propyl-
	(Tt)
	T111

	142–84–7
	Dipropylamine/1-Propanamine, n-propyl-
	(I,Tt)
	T110

	106–89–8
	Epiclorohidrín/Oxyrane, (chloromethyl)-2-
	(Tt)
	T041

	18883–66–4
	streptozotocine/D-glucose, 2-deoxy-2-[[(methylnitrosoamine)-carbonil]amine]
	(Tt)
	T206

	75–07–0
	Ethanal/Acetaldehyde
	(I,Tt)
	T001

	127–18–4
	Ethene, tetrachloro- 
	(Tt)
	T210

	51-79-6
	Ethyl carbamate (urethane)/Carbamic acid, ethyl ester
	(Tt)
	T238

	60-29-7
	Ethyl ether
	(I,Tt)
	T117

	97-63-2
	Ethyl metacrylate/2-Propenoic acid, 2-methyl-, ethyl ester
	(Tt)
	T118

	62-50-0
	Ethyl methane sulfonate/Methane sulphonico acid, ethyl ester
	(Tt)
	T119

	110–80–5
	Ethylene glycol monoethyl ether/Ethanol, 2-etoxy- 
	(Tt)
	T359

	107-06-2
	Ethylene dichloride/1,2-Dichloroethane
	(Tt)
	T077

	96–45–7
	Ethylenethiourea/2-imidazolidinthione
	(Tt)
	T116

	75–34–3
	Ethyldene dichloride/Ethane 1,1-dichloro- 
	(Tt)
	T076

	141–78–6
	Ethyl acetate/Acetic acid, ethyl ester
	(I,Tt)
	T112

	140–88–5
	Ethyl acrylate/2-Propenoic acid, ethyl ester
	(I,Tt)
	T113

	62–44–2
	phenacetine
	(Tt)
	T187

	108–95–2
	Phenol
	(Tt)
	T188

	206–44–0
	Flouranthene
	(Tt)
	T120

	7664–39–3
	Fluorohhydric acid 
	(C,Tt)
	T134

	50–00–0
	Formaldehyde
	(Tt)
	T122

	64–18–6
	formic acid 
	(C,Tt)
	T123

	1314–80–3
	Phosphorus sulphide 
	(R,Tt)
	T189

	85–44–9
	Phtalic anhydride/1,3-Isobenzofurandione
	(Tt)
	T190

	98–01–1
	Furfural
	(I,Tt)
	T125

	110–00–9
	Furfurane/Furan
	(I,Tt)
	T124

	58-89-9
	Gamma-BHC/Lindane
	(Tt)
	T129

	118–74–1
	Hexachlorobenzene
	(Tt)
	T127

	87–68–3
	Hexachlorobutadiene/1,3-Butadiene, 1,1,2,3,4,4-hexachlorine
	(Tt)
	T128

	77–47–4
	Hexachlorocyclopentadiene/1,3-Cyclopentadiene, 1,2,3,4,5,5-hexachlorine
	(Tt)
	T130

	67–72–1
	Hexachlorethane
	(Tt)
	T131

	70–30–4
	Hexachlorophene/2,2’-Methylenobis[3,4,6-trichlorophenol
	(Tt)
	T132

	1888–71–7
	Hexachloropropene/1-Propene, 1,1,2,3,3,3-hexachlorine
	(Tt)
	T243

	302–01–2
	Hidrazine 
	(R,Tt)
	T133

	1615–80–1
	Hidrazine, 1,2-diethyl-
	(Tt)
	T086

	193–39–5
	Indene[1,2,3-cd]pyrene
	(Tt)
	T137

	78–83–1
	Isobutyl alcohol/1-Propanol, 2-methyl-
	(I,Tt)
	T140

	120–58–1
	Isosafrole
	(Tt)
	T141

	143–50–0
	Kepone
	(Tt)
	T142

	303–34–1
	Lasiocarpine
	(Tt)
	T143

	123–33–1
	Maleic hidracide/3,6-Pyridazinedione, 1,2-dihydro-, 
	(Tt)
	T148

	108–31–6
	Maleic anhydride/2,5-Furandione
	(Tt)
	T147

	109–77–3
	Malononitrile/Propanodinitrile
	(Tt)
	T149

	541–73–1
	M-dichlorobenzene/Benzene, 1,3-dichloro
	(Tt)
	T071

	148–82–3
	Melphalan/L-phenylalanine, 4-[bis(2-Cloroethyl)amine] 
	(Tt)
	T150

	7439-97-6
	Mercury (all its forms)
	(Tt)
	T151

	126–98–7
	Metacrilonitrile/2-Propenenitrile, 2-methyl
	(I,Tt)
	T152

	67–56–1
	Methanel 
	(I,Tt)
	T154

	91–80–5
	Metapirilene
	(Tt)
	T155

	79–22–1
	Methyl clorocarbonate/carbon chloridric acid, methyl ester
	(I,Tt)
	T156

	71-55-6
	Methyl chloroform/1,1,1-trichloroethane
	(Tt)
	T226

	78–93–3
	Methyl ethyl ketone (MEK)/2-butanone 
	(I,Tt)
	T159

	1338–23–4
	Methyl ethyl ketone peroxide/2-butanone peroxide
	(R,Tt)
	T160

	108–10–1
	Methyl isobutyl ketone/4-Methyl-2-pentanone/4-Methylpenthanol
	(I,Tt)
	T161

	80–62–6
	Methyl metacrilate/2-Propenoic acid, 2-methyl-, methyl ester
	(I,Tt)
	T162

	74-95-3
	Methylene bromide
	(Tt)
	T068

	75–09–2
	Methylene chloride/Methane, dichloro-
	(Tt)
	T080

	74-87-3
	Methylchloride
	(I,Tt)
	T045

	74-88-4
	Methyl iodide
	(Tt)
	T138

	56–04–2
	Methythiouracile
	(Tt)
	T164

	2385-85-5
	Mirex 
	(Tt)
	T1000

	50–07–7
	Mitomycín C
	(Tt)
	T010

	70–25–7
	MNNG/Guanidine, n-methyl-n'-nitro-n-nitrose-
	(Tt)
	T163

	91–20–3
	Naphatalene
	(Tt)
	T165

	71–36–3
	n-Butyl alcohol/1-Butanol
	(I,Tt)
	T031

	98–95–3
	Nitrobenzene 
	(I,Tt)
	T169

	1116–54–7
	n-Nitrosodiethanolamine
	(Tt)
	T173

	55–18–5
	n-Nitrosodiethylamine
	(Tt)
	T174

	924–16–3
	n-Nitrosode-n-butylamine
	(Tt)
	T172

	759–73–9
	n-Nitrose-n-ethylurea
	(Tt)
	T176

	684–93–5
	n-Nitrose-n-methylurea
	(Tt)
	T177

	615–53–2
	n-Nitrose-n-methylurethane/Carbamic acid, methylnitrose-, ethyl ester
	(Tt)
	T178

	100–75–4
	n-Nitrosopiperidine/Piperidine, 1-nitrose
	(Tt)
	T179

	930–55–2
	n-Nitrosopirrolidine/Pirrolidine, 1-nitrose
	(Tt)
	T180

	107–10–8
	n-Propilamine/1-Propanamine
	(I,Tt)
	T194

	3288–58–2
	o,o-diethyl s-methyl dithiophosphate
	(Tt)
	T087

	95-57-8
	o-Chlorophenol/2-Chlorophenol
	(Tt)
	T048

	95–50–1
	o-Dichlorobenzene
	(Tt)
	T070

	95–53–4
	o-Toluidine
	(Tt)
	T328

	636-21-5
	o-Toluidine hydrochloride 
	(Tt)
	T222

	75–21–8
	Oxirane/Ethylene oxide
	(I,Tt)
	T115

	765–34–4
	Oxyranocarboxyaldehyde/Glycidilaldehyde
	(Tt)
	T126

	123–63–7
	Paraldehyde/1,3,5-Trioxane, 2,4,6-trimethyl-
	(Tt)
	T182

	59–50–7
	p-Chloro-m-cresol/4-Chloro-3-methylphenol
	(Tt)
	T039

	106–46–7
	p-Dichlorobenzene
	(Tt)
	T072

	60–11–7
	p-Dimethylaminoazobenzene
	(Tt)
	T093

	608–93–5
	Pentachlorobenzene
	(Tt)
	T183

	76–01–7
	Pentachloroethane
	(Tt)
	T184

	82–68–8
	Pentachloronitrobenzene (PCNB)
	(Tt)
	T185

	110–86–1
	Piridine
	(Tt)
	T196

	1335–32–6
	Lead subacetate/Lead, bis(acetate-o)tetrahydroxytri-
	(Tt)
	T146

	301–04–2
	Lead acetate 
	(Tt)
	T144

	7446–27–7
	Lead phosphate
	(Tt)
	T145

	100–02–7
	p-Nitrophenol/4-Nitrophenol
	(Tt)
	T170

	122–42–9
	Profam/Carbamic acid, phenyl-,1-methyl ether ester
	(Tt)
	T373

	23950–58–5
	Pronamide
	(Tt)
	T192

	78-87-5
	Propylene dichloride/1,2-Dichloropropane
	(Tt)
	T083

	114–26–1
	Propoxur/Phenol, 2-(1-methyl-etoxy)-, methyl carbamate
	(Tt)
	T411

	52888–80–9
	Prosulphocarb/Carbamotioic acid, dipropyl-, s-(phenylmethyl) ester
	(Tt)
	T387

	106–49–0
	p-Toluidine
	(Tt)
	T353

	50–55–5
	Reserpine
	(Tt)
	T200

	108–46–3
	Resorcinol
	(Tt)
	T201

	(1) 81–07–2
	Sacarina and salts/1,2-Benzisothioazol-3(2h)-one, 1,1-dioxide, and salts
	(Tt)
	T202

	94–59–7
	Safrole
	(Tt)
	T203

	7783–00–8
	Selenium dioxide
	(Tt)
	T204

	7488–56–4
	Selenium sulphur SeS2
	(R,Tt)
	T205

	7783–06–4
	Sulfur hydric acid 
	(Tt)
	T135

	563–68–8
	Thallium acetate 
	(I,Tt)
	T214

	6533–73–9
	Thallium carbonate/Carbonoic acid, dithallium(1+) salt
	(I,Tt)
	T215

	7791–12–0
	Thallium chloride 
	(Tt)
	T216

	10102–45–1
	Thallium nitrate/Nitric acid, thallium salt (1+)
	(I,Tt)
	T217

	127–18–4
	Tetrachoroethylene
	(Tt)
	T210

	109–99–9
	Tetrahydrofuran 
	(I,Tt)
	T213

	62–55–5
	Thioacetamide/Ethanothioamide
	(Tt)
	T218

	59669–26–0
	Thiodicarb
	(Tt)
	T410

	23564–05–8
	Thiophanate-methyl
	(Tt)
	T409

	74–93–1
	Thiomethanel/Methanethiol
	(I,Tt)
	T153

	62–56–6
	Tiourea
	(Tt)
	T219

	137–26–8
	Tiram
	(Tt)
	T244

	25376–45–8
	Toluene diamine
	(Tt)
	T221

	26471–62–5
	Toluene diisocyanate 
	(R,Tt)
	T223

	108–88–3
	Toluene/Methylbenzene
	(Tt)
	T220

	156-60-5
	Trans-1,2-dichoroethylene/1,2-dichoroethylene
	(Tt)
	T079

	2303–17–5
	Trialate
	(Tt)
	T389

	75-25-2
	Tribromomethane/Bromoform
	(Tt)
	T225

	79–01–6
	Trichoroethylene
	(Tt)
	T228

	75–69–4
	Tricloromonofluoromethane
	(Tt)
	T121

	121–44–8
	Triethylamine/Etanamine, n,n-diethyl-
	(I,Tt)
	T404

	72–57–1
	Tripan, blue
	(Tt)
	T236

	126–72–7
	Tris (2,3-dibromopropyl) phosphate/1-propanol, 2,3-dibromo-, phosphate (3:1)
	(Tt)
	T235

	66–75–1
	Uracile mustard 
	(Tt)
	T237

	75–01–4
	Vinyl chloride/Cloroethene
	(Tt)
	T043

	(1) 81–81–2
	Warfarine and salts, when they are present in concentrations lower than 0.3% 
	(Tt)
	T248

	1330–20–7
	Xylene isomers
	(Tt)
	T239

	1314–84–7
	Zinc phosphur Zn3P2, when present in concentrations lower or equal to 10% 
	(Tt)
	T249

	NOTES:

	1.- In the case of families of isomers of organic compounds, only the name of the group is mentioned, all the isomers must be considered toxic components (i.e. dichlorobenzenes, incluyes 1.2, 1.3, and 1.4 dichlorobenzenes). 

	2.- (1) indicates the CAS number o fan equivalent compound. 


	LISTADO 5


	
	

	CLASIFICACION POR TIPO DE RESIDUOS, SUJETOS A CONDICIONES PARTICULARES DE MANEJO
	
	

	Residuo
	CPR
	Clave

	BATERIAS, CELDAS Y PILAS

	CELDAS DE DESECHO EN LA PRODUCCION DE BATERIAS NIQUEL-CADMIO
	(T)
	RP 1/01

	PILAS O BATERIAS ZINC-OXIDO DE PLATA USADAS O DESECHADAS 
	(T)
	RP 1/02

	CATALIZADORES GASTADOS

	CATALIZADOR GASTADO CON OXIDOS DE FIERRO, CROMO Y POTASIO PROVENIENTES DEL REACTOR DE DESHIDROGENACION EN LA PRODUCCION DE ESTIRENO
	(T)
	RP 2/01

	CATALIZADOR GASTADO DE CLORURO DE MERCURIO EN LA PRODUCCION DE CLORO
	(T)
	RP 2/02

	CATALIZADOR GASTADO DE LA PURGA DE LA TORRE DE APAGADO EN LA PRODUCCION DE ACRILONITRILO
	(T)
	RP 2/03

	CATALIZADORES GASTADOS EN LA PRODUCCION DE MATERIALES PLASTICOS Y RESINAS SINTETICAS
	(T)
	RP 2/04

	CATALIZADORES GASTADOS DE VEHICULOS AUTOMOTORES 
	(T,C)
	RP 2/05

	ESCORIAS

	ESCORIAS PROVENIENTES DEL HORNO DE FUNDICION DE CHATARRA EN LA PRODUCCION DE ALUMINIO
	(T)
	RP 3/01

	ESCORIAS PROVENIENTES DEL HORNO ELECTRICO EN LA PRODUCCION DE FOSFORO
	(T)
	RP 3/02

	ESCORIAS PROVENIENTES DEL HORNO EN LA PRODUCCION SECUNDARIA DE COBRE
	(T)
	RP 3/03

	ESCORIAS PROVENIENTES DEL HORNO EN LA PRODUCCION SECUNDARIA DE PLOMO
	(T)
	RP 3/04

	LODOS

	ACABADO DE METALES Y GALVANOPLASTIA

	LODOS DE LOS TANQUES DE ENFRIAMIENTO CON ACEITES UTILIZADOS EN LAS OPERACIONES DE TRATAMIENTO EN CALIENTE DE METALES 
	(T)
	RP 4/01

	LODOS PROVENIENTES DE LAS OPERACIONES DE DECAPADO O DEL DESENGRASADO 
	(T)
	RP 4/02

	LODOS PROVENIENTES DE LOS BAÑOS DE CADMIZADO, COBRIZADO, CROMADO, ESTAÑADO, FOSFATIZADO, LATONADO, NIQUELADO, PLATEADO, TROPICALIZADO O ZINCADO DE PIEZAS METALICAS 
	(T,C)
	RP 4/03

	BENEFICIO DE METALES

	LODOS DEL ANODO ELECTROLITICO EN LA PRODUCCION PRIMARIA DE ZINC
	(T)
	RP 4/04

	LODOS DEL EQUIPO DE CONTROL DE EMISIONES DE HORNOS ELECTRICOS EN LA PRODUCCION DE HIERRO Y ACERO 
	(T)
	RP 4/05

	LODOS DEL LAVADOR DE GASES EN LA FUNDICION Y REFINADO DE ALUMINIO
	(T)
	RP 4/06

	LODOS DE LA MANUFACTURA DE ALEACIONES DE NIQUEL
	(T)
	RP 4/07

	LODOS DE LAS PURGAS DE LAS PLANTAS DE ACIDO EN LA PRODUCCION PRIMARIA DE COBRE
	(T)
	RP 4/08

	LODOS DEL EQUIPO DE CONTROL DE EMISIONES DE LA PRODUCCION DE FERROALEACIONES DE HIERRO-CROMO-SILICIO
	(T)
	RP 4/09

	LODOS PROVENIENTES DE LA LAGUNA DE EVAPORACION EN LA PRODUCCION PRIMARIA DE PLOMO
	(T)
	RP 4/10

	LODOS DEL EQUIPO DE CONTROL DE EMISIONES DEL AFINADO EN LA PRODUCCION PRIMARIA DE PLOMO
	(T)
	RP 4/11

	CURTIDURIA

	LODOS GENERADOS EN EL PROCESO DE DESENCALADO Y DEPILADO
	(C,R)
	RP 4/12

	LODOS GENERADOS EN EL PROCESO DE PELAMBRE O DEPILADO (ENCALADO)
	(C,R)
	RP 4/13

	LODOS GENERADOS EN LA ETAPA DE CURTIDO AL CROMO
	(C)
	RP 4/14

	MATERIALES PLASTICOS Y RESINAS SINTETICAS

	LODOS DE LAS AGUAS RESIDUALES DE LOS SISTEMAS DE LAVADO DE EMISIONES ATMOSFERICAS
	(T)
	RP 4/15

	LODOS DE TANQUES DE ALMACENAMIENTO DE MONOMEROS
	(T,I)
	RP 4/16

	METALMECANICA

	LODOS GENERADOS EN LAS CASETAS DE APLICACION DE PINTURA
	(T)
	RP 4/17

	LODOS PRODUCTO DE LA REGENERACION DE ACEITES DE ENFRIAMIENTO GASTADOS
	(T)
	RP 4/18

	PETROLEO, GAS Y PETROQUIMICA

	LODOS DE LOS SEPARADORES API Y CARCAMOS EN LA PRODUCCION DE PETROQUIMICOS
	(T,I)
	RP 4/19

	PINTURAS Y PRODUCTOS RELACIONADOS

	LODOS DE DESTILACION DE SOLVENTES
	(T)
	RP 4/20


	LODOS DE TRATAMIENTO DE AGUAS RESIDUALES

	ACABADO DE METALES Y GALVANOPLASTIA

	LODOS DE TRATAMIENTO DE LAS AGUAS RESIDUALES PROVENIENTES DE LAS OPERACIONES DE ENJUAGUE DE PIEZAS METALICAS PARA REMOVER SOLUCIONES CONCENTRADAS
	(T)
	RP 5/01

	PILAS Y BATERIAS

	LODOS DE TRATAMIENTO DE AGUAS RESIDUALES EN LA PRODUCCION DE BATERIAS PLOMO-ACIDO
	(T)
	RP 5/02

	LODOS DEL TRATAMIENTO DE AGUAS RESIDUALES EN LA PRODUCCION DE BATERIAS NIQUEL-CADMIO
	(T)
	RP 5/03

	QUIMICA INORGANICA

	LODOS DEL TRATAMIENTO DE LAS AGUAS RESIDUALES EN LA PRODUCCION DE ACIDO FLUORHIDRICO
	(T)
	RP 5/04

	POLVOS

	BENEFICIO DE METALES

	POLVOS DEL EQUIPO DE CONTROL DE EMISIONES DE HORNOS ELECTRICOS EN LA PRODUCCION DE HIERRO Y ACERO
	(T)
	RP 6/01

	POLVOS DEL EQUIPO DE CONTROL DE EMISIONES DEL AFINADO EN LA PRODUCCION PRIMARIA DE PLOMO
	(T)
	RP 6/02

	POLVOS DEL EQUIPO DE CONTROL DE EMISIONES DE LA PRODUCCION DE FERROALEACIONES DE HIERRO-CROMO
	(T)
	RP 6/03

	POLVOS DEL EQUIPO DE CONTROL DE EMISIONES DE LA PRODUCCION DE FERROALEACIONES DE HIERRO-CROMO-SILICIO
	(T)
	RP 6/04

	QUIMICA INORGANICA

	POLVOS RECUPERADOS EN EL PRECIPITADOR ELECTROSTATICO O CASA DE BOLSA EN LA PRODUCCION DE FOSFORO
	(T)
	RP 6/05

	OTROS RESIDUOS

	ACABADO DE METALES Y GALVANOPLASTIA

	ACEITES GASTADOS EN LAS OPERACIONES DE TRATAMIENTO EN CALIENTE DE METALES
	(T)
	RP 7/01

	SALES PRECIPITADAS DE LOS BAÑOS DE REGENERACION DE NIQUEL
	(T)
	RP 7/02

	RESIDUOS CONTENIENDO MERCURIO DE LOS PROCESOS ELECTROLITICOS
	(T)
	RP 7/03

	RESIDUOS DE CATALIZADORES AGOTADOS
	(T,C)
	RP 7/04

	BENEFICIO DE METALES

	COLAS EN LAS PLANTAS DE MANUFACTURA DE FERROALEACIONES DE HIERRO-NIQUEL
	(T)
	RP 7/05

	PURGAS DE LA PLANTA DE ACIDO EN LA PRODUCCION PRIMARIA DE ZINC
	(T)
	RP 7/06

	RESIDUO DE LIXIVIADO DE LA PLANTA DE CADMIO EN LA PRODUCCION PRIMARIA DE ZINC
	(T)
	RP 7/07

	COMPONENTES ELECTRONICOS

	RESIDUOS DE SOLDADURA EN LA PRODUCCION DE CIRCUITOS ELECTRONICOS QUE CONTENGAN PLOMO U OTROS METALES DE LA TABLA 2 DE ESTA NOM
	(T)
	RP 7/08

	RESIDUOS DE SOLVENTES EMPLEADOS EN LA LIMPIEZA DE LAS PLACAS EN LA PRODUCCION DE CIRCUITOS ELECTRONICOS
	(T)
	RP 7/09

	RESIDUOS GENERADOS EN LA PREPARACION DE PIGMENTOS MAGNETICOS Y EN LA PREPARACION DE LA MEZCLA DE COBERTURA EN LA PRODUCCION DE CINTAS MAGNETICAS
	(T)
	RP 7/10

	RESIDUOS PROVENIENTES DEL RECUBRIMIENTO DE TUBOS ELECTRONICOS DURANTE LA PRODUCCION DE LOS MISMOS
	(T)
	RP 7/11

	CURTIDURIA

	RESIDUOS QUE CONTIENEN CROMO POR ENCIMA DE LOS LMP DE LA TABLA 2 EXCEPTO SI: TODAS LAS SALES O SOLUCIONES UTILIZADAS EN EL PROCESO PRODUCTOR SEAN DE CROMO TRIVALENTE Y LOS RESIDUOS SE MANEJEN DURANTE TODO SU CICLO DE VIDA EN CONDICIONES NO OXIDANTES
	(T)
	RP 7/12

	EXPLOSIVOS

	RESIDUOS DE ACIDOS GASTADOS DE LA MANUFACTURA DE DINAMITA Y POLVORA
	(R,E)
	RP 7/13

	RESIDUOS DE LA MANUFACTURA DE CERILLOS Y PRODUCTOS PIROTECNICOS
	(R,E)
	RP 7/14

	RESIDUOS DE LA MANUFACTURA DEL PROPELENTE SOLIDO
	(R,E)
	RP 7/15

	MATERIALES PLASTICOS Y RESINAS SINTETICAS

	FONDOS DE TANQUES DE ALMACENAMIENTO DE MONOMEROS EN LA PRODUCCION DE MATERIALES PLASTICOS Y RESINAS SINTETICAS
	(T,I)
	RP 7/16

	METALMECANICA

	ACEITES GASTADOS DE CORTE Y ENFRIAMIENTO EN LAS OPERACIONES DE TROQUELADO, FRESADO, TALADRADO Y ESMERILADO
	(T)
	RP 7/17

	CARBON ACTIVADO AGOTADO PROVENIENTE DEL SISTEMA DE EMISIONES DE LA CASETA DE PINTADO
	(T)
	RP 7/18

	RESIDUOS DEL PROCESO DE EXTRUSION DE TUBERIA DE COBRE
	(T)
	RP 7/19

	RESIDUOS DE LAS OPERACIONES DE LIMPIEZA ALCALINA O ACIDA
	(C,T)
	RP 7/20

	PETROLEO, GAS Y PETROQUIMICA

	ACEITES SOLUBLES EN ACIDO (ASAS) PROVENIENTES DE LOS PROCESOS DE ALQUILACION DE HIDROCARBUROS
	(I)
	RP 7/21

	AMINAS GASTADAS, FILTROS DE AMINA CONTAMINADA, LODOS DE AMINA, SOLUCION ACUOSA DE AMINA CONTAMINADA, PRODUCTOS DE LA DEGRADACION DE LA AMINA, ASI COMO SOLIDOS RECUPERADOS (FONDOS) PROVENIENTES DEL PROCESO DE ENDULZAMIENTO DEL GAS Y CONDENSADOS AMARGOS. OTROS PRODUCTOS DE LA DEGRADACION DE AMINAS DEL PROCESO DE ENDULZAMIENTO, CRACKING Y FRACCIONAMIENTO DE AZUFRE
	(T)
	RP 7/22

	CLORADOS INTERMEDIOS PROVENIENTES DEL FONDO DE LA COLUMNA REDESTILADORA DE MONOMERO DE VINILO
	(C,T,I)
	RP 7/23

	CLORADOS PESADOS PROVENIENTES DE LOS FONDOS DE LA COLUMNA DE PURIFICACION DE DICLOROETANO
	(C,T,I)
	RP 7/24

	DERIVADOS HEXACLORADOS PROVENIENTES DE LOS FONDOS DE LA COLUMNA DE RECUPERACION DE PERCLOROETILENO
	(T)
	RP 7/25

	POLIMERO DE LA PURGA DE LA TORRE DE APAGADO EN LA PRODUCCION DE ACRILONITRILO
	(T)
	RP 7/26

	RESIDUOS DE LA DESHIDROGENACION DEL N-BUTANO EN LA PRODUCCION DE BUTADIENO
	(T)
	RP 7/27

	SEDIMENTO IMPREGNADO DE HIDROCARBUROS PROVENIENTES DE LAS CORRIDAS DE DIABLO
	(T)
	RP 7/28

	SOSAS GASTADAS Y SOSAS FENOLICAS PROVENIENTES DE LOS PROCESOS DE ENDULZAMIENTO DE HIDROCARBUROS
	(C,T)
	RP 7/29

	PILAS Y BATERIAS

	PASTA DE DESECHO EN LA PRODUCCION DE PILAS SECAS (CELDAS PRIMARIAS-ALCALINAS Y ACIDAS)
	(T)
	RP 7/30

	RESIDUOS DE LOS HORNOS DE LA PRODUCCION DE BATERIAS DE MERCURIO
	(T)
	RP 7/31

	PINTURAS Y PRODUCTOS RELACIONADOS

	FELPAS IMPREGNADAS DE PIGMENTOS DE CROMO Y PLOMO
	(T)
	RP 7/32

	RESIDUOS DE AGENTES SECANTES PARA PINTURAS, LACAS, BARNICES, MASILLAS PARA RESANAR Y PRODUCTOS DERIVADOS
	(T)
	RP 7/33

	RESIDUOS DE DISOLVENTES EMPLEADOS EN EL LAVADO DE LOS EQUIPOS DE PROCESO
	(T,C)
	RP 7/34

	RESIDUOS DE MONOMEROS AUTOPOLIMERIZABLES
	(T,R)
	RP 7/35

	RESIDUOS DE RETARDADORES DE FLAMA
	(T)
	RP 7/36

	RESIDUOS DEL EQUIPO DE CONTROL DE LA CONTAMINACION DEL AIRE
	(T)
	RP 7/37

	QUIMICA FARMACEUTICA

	CARBON ACTIVADO GASTADO DE LA PRODUCCION DE FARMOQUIMICOS Y MEDICAMENTOS QUE HAYA TENIDO CONTACTO CON PRODUCTOS QUE CONTENGAN CONSTITUYENTES TOXICOS DE LOS LISTADOS 3 Y 4 DE ESTA NORMA
	(T)
	RP 7/38

	LOS MEDICAMENTOS FUERA DE ESPECIFICACIONES O CADUCOS QUE NO APAREZCAN EN LOS LISTADOS 3 Y 4 DE ESTA NORMA OFICIAL MEXICANA
	(T)
	RP 7/39

	RESIDUOS BIOLOGICOS NO INACTIVADOS DE LA PRODUCCION DE BIOLOGICOS Y HEMODERIVADOS
	(B)
	RP 7/40

	RESIDUOS DE LA PRODUCCION DE BIOLOGICOS Y HEMODERIVADOS QUE CONTENGAN CONSTITUYENTES TOXICOS DE LOS LISTADOS 3 Y 4 DE ESTA NORMA
	(B)
	RP 7/41

	RESIDUOS DE LA PRODUCCION DE FARMOQUIMICOS Y MEDICAMENTOS QUE CONTENGAN CONSTITUYENTES TOXICOS DE LOS LISTADOS 3 Y 4 DE ESTA NORMA
	(T)
	RP 7/42

	QUIMICA INORGANICA

	FILTRO AYUDA GASTADO (TORTAS DE FILTROS) EN LA PRODUCCION DE FOSFORO Y PIGMENTOS DE CROMO Y DERIVADOS
	(T)
	RP 7/43

	RESIDUOS DE LA PRODUCCION DE CARBONILO DE NIQUEL
	(T)
	RP 7/44

	QUIMICA ORGANICA

	MEDIOS FILTRANTES GASTADOS DE LA PRODUCCION DE 2,4,6-TRIBROMOFENOL
	(T)
	RP 7/45

	RESIDUOS Y SUBPRODUCTOS DEL REACTOR EN LA PRODUCCION DEL NITROBENCENO
	(T)
	RP 7/46

	RESIDUOS DE LA DESTILACION EN LA PRODUCCION DE ANHIDRIDO MALEICO
	(T, C)
	RP 7/47

	RESIDUOS DE LA PRODUCCION DE 2,4,6-TRIBROMOFENOL
	(T)
	RP 7/48

	RESIDUOS DE LAS TORRES DE LAVADO DE GASES EN LA PRODUCCION DE METIL ETIL PIRIDINA
	(T)
	RP 7/49

	TEXTILES

	AGENTES MORDIENTES GASTADOS RESIDUALES
	(T)
	RP 7/50

	RESIDUOS ACIDOS O ALCALINOS
	( C )
	RP 7/51

	RESIDUOS DE ADHESIVOS Y POLIMEROS
	(T)
	RP 7/52

	RESIDUOS DE AGENTES ENLAZANTES Y DE CARBONIZACION
	(T)
	RP 7/53

	RESIDUOS PROVENIENTES DEL BLANQUEADO
	(C,T)
	RP 7/54

	VARIOS

	CENIZAS DE INCINERACION DE RESIDUOS
	(T)
	RP 7/55

	GASOLINA, DIESEL Y NAFTAS GASTADOS O SUCIOS PROVENIENTES DE ESTACIONES DE SERVICIO Y TALLERES AUTOMOTRICES
	(T)
	RP 7/56

	RESIDUOS DE LIQUIDO BLANQUEADOR, FIJADOR, ESTABILIZADOR Y AGUAS DE ENJUAGUE PROVENIENTES DEL REVELADO DE PAPEL FOTOGRAFICO, PLACAS RADIOGRAFICAS O DE RAYOS X Y FOTOLITOS
	(T)
	RP 7/57

	SOLUCIONES GASTADAS

	ACABADO DE METALES Y GALVANOPLASTIA

	SOLUCIONES GASTADAS DE LOS BAÑOS DE ANODIZACION DEL ALUMINIO
	(T)
	RP 8/01

	SOLUCIONES GASTADAS DE CIANURO DE LOS CRISOLES DE LIMPIEZA CON BAÑOS DE SALES EN LAS OPERACIONES DE TRATAMIENTO EN CALIENTE DE METALES
	(R,T)
	RP 8/02

	SOLUCIONES GASTADAS PROVENIENTES DE LAS OPERACIONES DE DECAPADO
	(T)
	RP 8/03

	SOLUCIONES GASTADAS PROVENIENTES DE LOS BAÑOS DE CADMIZADO, COBRIZADO, CROMADO, ESTAÑADO, FOSFATIZADO, LATONADO, NIQUELADO, PLATEADO, TROPICALIZADO O ZINCADO DE PIEZAS METALICAS
	(T,C)
	RP 8/04

	BENEFICIO DE METALES

	SOLUCION GASTADA DEL LAVADOR DE GASES QUE PROVIENE DEL PROCESO DEL AFINADO EN LA PRODUCCION PRIMARIA DE PLOMO
	(T)
	RP 8/05

	COMPONENTES ELECTRONICOS

	SOLUCIONES ACIDAS GASTADAS PROVENIENTES DE LA LIMPIEZA EN LA PRODUCCION DE SEMICONDUCTORES
	(T)
	RP 8/06

	SOLUCIONES GASTADAS PROVENIENTES DEL BAÑO DE PLAQUEADO EN LA PRODUCCION DE CIRCUITOS ELECTRONICOS
	(T)
	RP 8/07

	METALMECANICA

	SOLUCIONES GASTADAS DE LOS BAÑOS DE TEMPLADO PROVENIENTES DE LAS OPERACIONES DE ENFRIAMIENTO
	(T)
	RP 8/08

	SOLUCIONES GASTADAS PROVENIENTES DE LA EXTRUSION
	(C,T)
	RP 8/09

	PRESERVACION DE LA MADERA

	SOLUCIONES GASTADAS GENERADAS EN LOS PROCESOS DE PRESERVACION DE LA MADERA
	(T)
	RP 8/10


	LIST 5

	CLASSIFICATION BY TYPE OF WASTES, SUBJECT TO SPECIFIC CONDITIONS OF HANDLING



	waste
	CPR
	CODE

	BATTERIES, CELLS 

	WASTE CELLS IN THE PRODUCTION OF NICKEL CADMIUM BATTERIES 
	(T)
	RP 1/01

	ZINC-OXIDE BATTERIES, USED OR WASTED SILVER BATTERIES 
	(T)
	RP 1/02

	USED CATALYZERS

	USED CATALYZERS WITH IRON OXIDES, CHROME AND POTASSIUM ORGIGINATING FROM THE DEHYDROGENTATION REACTOR IN THE PRODUCTION OF STYRENE
	(T)
	RP 2/01

	USED CATALYZERS MERCURY CHLORIDE IN THE PRODUCTION OF CHLORINE
	(T)
	RP 2/02

	USED CATALYZERS FROM THE PURGE OF THE TOWER STOPPED IN THE PRODUCTION OF ACRYLNITRILE 
	(T)
	RP 2/03

	USED CATALYZERS IN THE PRODUCTION OF PLASTIC MATERIALS AND SYNTHETIC RESINS 
	(T)
	RP 2/04

	USED CATALYZERS FROM MOTOR VEHICLES 
	(T,C)
	RP 2/05

	SLAGS

	SLAGS ORIGINATING IN THE FOUNDRY OVEN OF METAL SCRAP IN THE PRODUCTION OF ALUMINUM
	(T)
	RP 3/01

	SLAGS ORIGINATING IN THE  ELECTRIC OVEN IN THE PRODUCTION OF PHOSPHURUS 
	(T)
	RP 3/02

	SLAGS ORIGINATING IN THE OVEN IN THE SECONDARY PRODUCTION OF COPPER
	(T)
	RP 3/03

	SLAGS ORIGINATING IN THE OVEN IN THE SECONDARY PRODUCTION OF LEAD
	(T)
	RP 3/04

	SLUDGES

	METAL WASTES FROM GALVANOPLASTY

	SLUDGES FROM THE COOLING TANKS WITH OIL UTILIZED IN THE OPERATIONS OF HEAT TREATMENT OF METALS
	(T)
	RP 4/01

	SLAGS ORIGINATING IN THE OPERATIONS OF PICKLING OR DEGREASING
	(T)
	RP 4/02

	SLAGS ORIGINATING IN THE CADMIUM, COPPER, CHROME, TIN, PHOSPHATE, BRASS, NICKEL, SILVER, TROPICALIZED OR ZINC COVERING OF METALLIC PIECES 
	(T,C)
	RP 4/03

	RENDERING FROM METALS

	SLUDGES FROM ELECTROLYTE ANODE IN THE PRIMARY PRODUCTION OF ZINC
	(T)
	RP 4/04

	SLUDGES FROM CONTROL EQUIPMENT OF EMISSIONS OF ELECTRIC OVENS IN THE PRODUCTION OF IRON AND STEEL
	(T)
	RP 4/05

	SLUDGES FROM THE CLEANING OF GASES IN THE FOUNDING AND REFINING OF ALUMINUM 
	(T)
	RP 4/06

	SLUDGES FROM THE MANUFACTURE OF NICKEL ALLYS
	(T)
	RP 4/07

	SLUDGES FROM THE PURGES FROM ACID PLANTS IN THE PRIMARY PRODUCTION OF COPPER
	(T)
	RP 4/08

	SLUDGES FROM CONTROL EQUIPMENT OF EMISSIONS  FROM THE PRODUCTION OF IRON ALLOYS OF IRON-CHROME-SILICON
	(T)
	RP 4/09

	SLUDGES ORIGINATING IN THE EVAPORATION BATH IN THE PRIMARY PRODUCTION OF LEAD 
	(T)
	RP 4/10

	SLUDGES FROM CONTROL EQUIPMENT OF EMISSIONS FROM THE REFINING IN THE PRIMARY PRODUCTION OF LEAD 
	(T)
	RP 4/11

	LEATHER CURING

	SLUDGES GENERATED IN THE PROCESS OF  SKINNING AND HAIR REMOVAL
	(C,R)
	RP 4/12

	SLUDGES GENERATED IN THE PROCESS HAIR REMOVAL OR LIME PIT HAIR REMOVAL
	(C,R)
	RP 4/13

	SLUDGES GENERATED IN THE CHROME CURING STAGE
	(C)
	RP 4/14

	PLASTIC MATERIALS AND SYNTHETIC RESINS

	SLUDGES ORIGINATING FROM THE WASTEWATERS OF THE CLEANING SYSTEMS OF ATMOSPHERIC EMISSIONS
	(T)
	RP 4/15

	SLUDGES FROM STORAGE  TANKS OF MONOMERS
	(T,I)
	RP 4/16

	METAL MECHANICS

	SLUDGES GENERATED IN THE PAINT SPRAY BOOTHS
	(T)
	RP 4/17

	SLUGES PRODUCT OF THE REGENERATION OF USED COOLING OILS
	(T)
	RP 4/18

	PETROLEUM, GAS, AND PETROCHEMICAL

	SLUDGES FROM THE API SEPARATORS  IN THE PRODUCTION OF PETROCHEMICALS
	(T,I)
	RP 4/19

	PAINT AND RELATED PRODUCTS

	SLUDGES FROM THE DISTILLING OF SOLVENTS
	(T)
	RP 4/20


	SLUDGES FROM THE TREATMENT OF WASTEWATERS

	WASTE FROM METALS AND GALVANOPLASTY

	SLUDGES FROM THE TREATMENT OF WASTEWATERS ORIGINATING FROM THE RINSING OPERATIONS OF METAL PIECES TO REMOVE CONCENTRATED SOLUTIONS
	(T)
	RP 5/01

	BATTERIES

	SLUDGES FROM THE TREATMENT OF WASTEWATERS  IN THE PRODUCTION OF LEAD ACID BATTERIES 
	(T)
	RP 5/02

	SLUDGES FROM THE TREATMENT OF WASTEWATERS IN THE PRODUCTION OF NICKEL CADMIUM BATTERIES
	(T)
	RP 5/03

	INORGANIC CHEMICALS

	SLUDGES FROM THE TREATMENT OF WASTEWATERS IN THE PRODUCTION OF FLOUROHYDRIC ACID
	(T)
	RP 5/04

	DUSTS

	BENEFICE OF METALS

	DUSTS FROM CONTROL EQUIPMENT OF EMISSIONS FROM ELECTRIC OVENS IN THE PRODUCTION OF IRON AND STEEL
	(T)
	RP 6/01

	DUSTS FROM CONTROL EQUIPMENT OF EMISSIONS FROM THE REFINING IN THE PRIMARY PRODUCTION OF LEAD
	(T)
	RP 6/02

	DUSTS FROM CONTROL EQUIPMENT OF EMISSIONS FROM THE PRODUCTION OF IRON-CHROME ALLOYS
	(T)
	RP 6/03

	DUSTS FROM CONTROL EQUIPMENT OF EMISSIONS FROM THE PRODUCTION OFSILICON IRON-CHROME ALLOYS 
	(T)
	RP 6/04

	INORGANIC CHEMICALS 

	DUSTS RECOVERED IN THE ELECTROSTATIC PRECIPITATOR OR CONTAINMENT BAG IN THE PRODUCITON OF PHOSPHURUS
	(T)
	RP 6/05

	OTHER WASTES

	WASTES FROM METALS AND GALVANOPLASTY

	USED OIL IN THE OPERATIONS OF HEAT TREATMENT OF METALS
	(T)
	RP 7/01

	SALTS PRECIPITATED FROM THE NICKEL REGENERATION BATHS
	(T)
	RP 7/02

	WASTES CONTAINING MERCURY FROM ELECTRLYTE PROCESSES
	(T)
	RP 7/03

	WASTES FROM SPENT CATALYZERS 
	(T,C)
	RP 7/04

	BENEFICE FROM METALS

	GLUES IN THE MANUFACTURING PLANTS OF IRON-NICKEL IRON ALLOYS
	(T)
	RP 7/05

	PURGES FROM THE ACID PLANT IN THE PRIMARY PRODUCTION OF ZINC
	(T)
	RP 7/06

	LEACHED LIQUID WASTE FROM THE CADMIUM PLANT IN THE PRIMARY PRODUCTION OF ZINC 
	(T)
	RP 7/07

	ELECTRONIC COMPONENTS

	WELDING WASTES IN THE PRODUCTION OF ELECTRONIC CIRCUITS THAT CONTAIN LEAD OR OTHER METALS FROM TABLE 2 OF THIS NOM
	(T)
	RP 7/08

	WASTES FROM SOLVENTS EMPLOYED IN THE CLEANING OF THE PLATES IN THE PRODUCTION OF ELECTRONIC CIRCUITS
	(T)
	RP 7/09

	WASTES GENERATED IN THE PREPARATION OF MAGNETIC PIGMENTS AND IN THE WASTES GENERATED IN THE PREPARATION OF MAGNETIC PIGMENTS AND IN THE PREPARATION OF THE COVERING MIXTURE IN THE PRODUCTION OF MAGNETIC TAPES
	(T)
	RP 7/10

	WASTES ORIGINATING FROM THE COATING OF ELECTRONIC TUBES DURING THE PRODUCTION OF THE SAME
	(T)
	RP 7/11

	TANNING

	WASTES THAT CONTAIN CHROME ABOVE THE MPL FROM TABLE 2 EXCEPT WHEN: ALL THE SALTS OR SOLUTIONS UTILIZED IN THE PRODUCTION PROCESS ARE OF CHROME TRIVALENTE AND THE WASTES ARE HANDLED DURING THE WHOLE LIFE CYCLE UNDER NON OXIDIZING CONDITIONS
	(T)
	RP 7/12

	EXPLOSIVES

	WASTES FROM SPENT ACIDS FROM THE MANUFACTURE OF DYNAMITE AND GUNPOWDER
	(R,E)
	RP 7/13

	WASTES FROM THE MANUFACTURE OF MATCHES AND PYROTECHNICAL PRODUCTS
	(R,E)
	RP 7/14

	WASTES FROM THE MANUFACTURE OF SOLID PROPELLANT 
	(R,E)
	RP 7/15

	 PLASTIC MATERIALS AND SYNTHETIC RESINS 

	BASES OF STORAGE TANKS OF MONOMERS IN THE PRODUCTION OF PLASTIC MATERIALS AND SYNTHETIC RESINS
	(T,I)
	RP 7/16

	MECHANICAL WORK

	SPENT OIL FROM CUTTING AND COOLING IN THE OPERATIONS OF CASTING, MILLING, DRILLING, AND GRINDING
	(T)
	RP 7/17

	SPENT ACTIVATED CHARCOAL ORIGINATING FROM THE SYSTEM OF EMISSIONS OF THE PAINT BOOTH
	(T)
	RP 7/18

	WASTES FROM THE EXTRUSION PROCESS OF COPPER PIPE
	(T)
	RP 7/19

	WASTES FROM THE OPERATIONS OF ALKALINE OR ACID CLEANING 
	(C,T)
	RP 7/20

	PETROLEUM, GAS, AND PETROCHEMICALS 

	OILS SOLUBLE IN ACID ORIGINATING FROM THE PROCESSES OF HYDROCARBON DISTILLING


	(I)
	RP 7/21

	SPENT AMINES, CONTAMINATED AMINE FILTERS, AMINE SLUDGES, AQUAEOUS SOLUTION OF CONTAMINATED AMINE, PRODUCTS FROM THE DEGRADATION OF AMINE, AS WELL AS RECOVERED SOLIDS ORIGINATING FROM THE SWEETENING PROCES OF GAS AND BITTER CONDENSATIONS. OTHER PRODUCTS FROM THE DEGRATION OF AMINES FROM THE SWEETENING PROCESS, CRACKING AND SEPARATION OF SULFUR
	(T)
	RP 7/22

	INTERMEDIATE CHLORIDES ORIGINATING FROM THE BASE OF THE DISTILLATION COLUMN OF VINYL MONOMER
	(C,T,I)
	RP 7/23

	HEAVY CHLORIDES ORIGINATING FROM THE BASE OF THE PURIFICATION COLUMN OF DICHLOROETHANE
	(C,T,I)
	RP 7/24

	HEXACHLORIDE DERIVATIVES ORIGINATING FROM THE BASES OF THE PERCHLOROETHYLYENE RECOVERY COLUMN
	(T)
	RP 7/25

	POLYMER FROM THE PURGE OF THE EXTINGUISHING TOWER IN THE PRODUCTION OF ACRYLONITRILE
	(T)
	RP 7/26

	WASTES FROM THE DEHYDROGENATION OF THE N-BUTANE IN THE PRODUCTION OF BUTADIENE
	(T)
	RP 7/27

	SEDIMENT IMPREGNATED WITH HYDROCARBONS ORIGINATING FROM THE TRAPS
	(T)
	RP 7/28

	SPENT SODAS AND PHENOLIC SODAS ORIGINATING FROM THE SWEETENING PROCESS OF HYDROCARBONS
	(C,T)
	RP 7/29

	BATTERIES

	DRY WASTE FROM THE PRODUCTION OF DRY BATTERIES (PRIMARY CELLS – ALKALINES AND ACIDS)
	(T)
	RP 7/30

	WASTES FROM THE OVENS OF THE PRODUCTION OF MERCURY BATTERIES 
	(T)
	RP 7/31

	PAINTS AND RELATED PRODUCTS

	FELT IMPREGNATED WITH CHROME AND LEAD PIGMENTS 
	(T)
	RP 7/32

	WASTES FROM DRYING AGENTS FOR PAINTS, LACQUERS, VARNISHES, FILLERS AND DERIVATIVE PRODUCTS
	(T)
	RP 7/33

	WASTES FROM SOLVENTS EMPLOYED IN THE CLEANING OF THE EQUIPMENT OF THE PROCESS
	(T,C)
	RP 7/34

	WASTES OF AUTOPOLYMERIZABLE MONOMERS 
	(T,R)
	RP 7/35

	WASTES FROM FLAME RETARDERS
	(T)
	RP 7/36

	WASTES FROM THE CONTROL EQUIPMENT FROM THE CONTAMINATION OF THE AIR
	(T)
	RP 7/37

	PHARMACEUTICAL CHEMISTRY

	SPENT ACTIVATED CHARCOAL FROM THE PRODUCTION OF PHARMOCHEMICALS AND MEDICATIONS THAT HAVE HAD CONTACT WITH PRODUCTS THAT CONTAIN TOXIC COMPONENTS OF THE LISTS 3 AND 4 OF THIS STANDARD
	(T)
	RP 7/38

	THE MEDICATIONS OUTSIDE OF SPECIFICATIONS OR EXPIRED THAT DO NOT APPEAR IN LISTS 3 AND 4 OF THIS OFFICIAL MEXICAN STANDARD 
	(T)
	RP 7/39

	NON ACTIVATED BIOLOGICAL WASTES FROM THE PRODUCTION OF BIOLOGICAL AND BLOOD DERIVATIVES
	(B)
	RP 7/40

	WASTES FROM THE PRODUCTION OF BIOLOGICAL AND BLOOD DERIVATIVES THAT CONTAIN TOXIC COMPONENTS FROM LISTS 3 AND 4 OF THIS STANDARD 
	(B)
	RP 7/41

	WASTES FROM THE PRODUCTION OF PHARMACEUTICALS AND MEDICATIONS THAT CONTAIN TOXIC COMPONENTS FROM LISTS 3 AND 4 OF THIS STANDARD 
	(T)
	RP 7/42

	INORGANIC CHEMICALS

	SPENT AUXILIARY FILTER (GROUPS OF FILTERS) IN THE PRODUCTION OF PHOSPHORUS AND PIGMENTS OF CHROME AND DERIVATIVES
	(T)
	RP 7/43

	WASTES FROM TEH PRODUCIOTN OF NICKEL CARBONYL 
	(T)
	RP 7/44

	ORGANIC CHEMICALS

	SPENT FILTERING MEDIA FRO THE PRODUCTION OF 2,4,6-TRIBROMOPHENOL
	(T)
	RP 7/45

	WASTES AND BYPRODUCTS FROM THE REACTOR IN THE PRODUCITON OF NITROBENAENE
	(T)
	RP 7/46

	WASTES FROM THE DISTILLIN IN THE PRODUCTION OF MALEIC ANHYDRIDE 
	(T, C)
	RP 7/47

	WASTES FROM THE PRODUCTION OF 2,4,6 – TRIBROMOPHENOL 
	(T)
	RP 7/48

	WASTES FROM THE GAS CLEANING TOWERS IN THE PRODUCTION OF METHYL ETHYL PIRIDINE
	(T)
	RP 7/49

	TEXTILES

	WASTES FROM SPENT MORDANT AGENTS
	(T)
	RP 7/50

	ACID OR ALKALINE WASTES 
	( C )
	RP 7/51

	WASTES FROM ADHESIVES AND POLYMERS
	(T)
	RP 7/52

	WASTES FROM CARBONIZATION BONDING AGENTS
	(T)
	RP 7/53

	WASTES ORIGINATING FROM BLEACHING
	(C,T)
	RP 7/54

	VARIOUS

	ASHES FROM INCINERATION OF WASTES 
	(T)
	RP 7/55

	SPENT OR DIRTY GASOLINE, DIESEL AND NAPHTAS ORIGINATING FROM SERVICE STATIONS AND AUTOMOTIVE SHOPS
	(T)
	RP 7/56

	WASTES FROM LIQUID BLEACH, FIXER, STABILIZER, AND RINSE WATERS ORIGINATING IN THE DEVELOPMENT OF PHOTOGRAPHIC PAPER, RADIOGRAPHIC PLATES OR X-RAY AND PHOTOLITE PLATES
	(T)
	RP 7/57

	SPENT SOLUTIONS

	FINISHING OF METALS AND GALVANOPLASTY

	SPENT SOLUTIONS OF THE ALUMINUM ANODIZATION BATHS
	(T)
	RP 8/01

	SPENT SOLUTIONS OF CYANIDE FROM THE CLEANING CRUCIBLES WITH SALTS BATHS IN THE HEAT TREATMENT OPERATIONS OF METALS 
	(R,T)
	RP 8/02

	SPENT SOLUTIONS ORIGINATING FROM THE OPERATIONS OF PICKLING 
	(T)
	RP 8/03

	SPENT SOLUTIONS ORIGINATING FROM THE CADMIUM, COPPER, CHROME, BRASS, PHOSPHATE, TIN, NICKEL, SILVER, TROPICALIZING OR ZINC OF METALLIC PIECES
	(T,C)
	RP 8/04

	BENEFICE OF METALS

	SPENT SOLUTION OF THE GASES CLEANING THAT ORIGINATES FROM THE PROCESS OF THE REFINING IN THE PRIMARY PRODUCTION OF LEAD
	(T)
	RP 8/05

	ELECTRONIC COMPONENTS

	SPENT ACID SOLUTIONS ORIGINATING FROM THE CLEANING IN THE PRODUCTION OF SEMI-CONDUCTORS
	(T)
	RP 8/06

	SPENT SOLUTIONS ORIGINATING FROM THE PLATING BATH IN THE PRODUCTION OF ELECTRONIC CIRCUITS
	(T)
	RP 8/07

	MECHANICAL METAL WORK

	SPENT SOLUTIONS FROM THE TEMPERING BATHS ORIGINATING FROM THE OPERATONS OF COOLING. 
	(T)
	RP 8/08

	SPENT SOLUTIONS ORIGINATING FROM EXTRUSION 
	(C,T)
	RP 8/09

	PRESERVATION OF WOOD

	SPENT SOLUTIONS GENERATED IN THE PROCESSES OF THE PRESERVATION OF WOOD 
	(T)
	RP 8/10
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	DIAGRAMA DE FLUJO DEL PROCEDIMIENTO PARA IDENTIFICAR 
LA PELIGROSIDAD DE UN RESIDUO (LISTADOS Y CARACTERIZACION
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	Para los residuos peligrosos de los Listados 1 y 2 se podrán solicitar Condiciones Particulares de Manejo, según lo establecido en el Reglamento.


	FIGURE 1

	FLOW CHART OF THE PROCEDURE FOR IDENTIFYING THE HAZARD OF A WASTE (LISTS AND CHARACTERIZATION)
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	FOR THE HAZARDOUS WASTES FROM LISTS 1 AND 2 SPECIFIC CONDITIONS OF HANDLING MAY BE REQUESTED FOLLOWING THAT ESTABLISHED IN THE REGULATION. 


	ANEXO 1

	BASES PARA LISTAR RESIDUOS PELIGROSOS POR “FUENTE ESPECIFICA” Y “FUENTE NO ESPECIFICA”, EN FUNCION DE SUS TOXICIDADES AMBIENTAL, AGUDA O CRONICA



	Clave
	Constituyentes por los que se listaron los residuos

	E1/01
	Cianuro (complejos)

	E1/02
	Cromo hexavalente, plomo

	E1/03
	Cromo hexavalente, plomo, cadmio

	E1/04
	Plomo, benceno, benzo(a)pireno, dibenz(a,h)antraceno, benzo(a)antraceno, benzo(b)flouranteno, benzo(k)fluoranteno, 3-metilclorantreno, 7,12-dimetilbenz(a)antraceno

	E2/01
	Arsénico, benceno, benzo(a)antraceno, benzo(b)fluoranteno, benzo(k)fluoranteno, benzo(a)pireno, cianuro, compuestos fenólicos, dibenz(a,h)antraceno, fenol, indeno(1,2,3-cd)pireno, naftaleno

	E3/01
	N.A.

	E3/02
	Plomo

	E3/03
	N.A.

	E4/01
	Benceno y arsénico

	E4/02
	Benceno, benzo(a)pireno, criseno, plomo, cromo

	E4/03
	Benceno, benzo(a)pireno, criseno, plomo, cromo

	E4/04
	Cromo hexavalente, plomo

	E4/05
	Plomo, benceno, benzo(a)pireno, dibenz(a,h)antraceno, benzo(a)antraceno, benzo(b)flouranteno, benzo(k)fluoranteno, 3-metilclorantreno, 7,12-dimetilbenz(a)antraceno. 

	E4/06
	Cromo hexavalente

	E4/07
	Cromo hexavalente, plomo

	E4/08
	Cromo hexavalente, plomo

	E4/09
	Cloroformo, formaldehído, cloruro de metileno, cloruro de metilo, paraldehído, ácido fórmico

	E4/10
	Cloroformo, formaldehído, cloruro de metileno, cloruro de metilo, paraldehído, ácido fórmico, cloracetaldehído

	E4/11
	Clorometano, diclorometano, triclorometano, tetracloruro de carbono, cloroetileno, 1,1- dicloroetano, 1,2-dicloroetano, trans-1-1-dicloroetileno, 1,1-dicloroetileno, 1,1,1-tricloroetano, 1,1,2-tricloroetano, tricloroetileno, 1,1,1,2-tetracloroetano, 1,1,2,2-tetracloroetano, tetracloroetileno, pentacloroetano, hexacloroetano, cloruro de alilo (3-cloropropano), dicloropropano, dicloropropeno, 2-cloro-1,3-butadieno, hexacloro-1,3-butadieno, hexaclorociclopentadieno, hexaclorociclohexano, benceno, clorobenceno, diclorobencenos, 1,2,4-triclorobenceno, tetraclorobenceno, pentaclorobenceno, hexaclorobenceno, tolueno, naftaleno

	E5/01
	Plomo, cromo hexavalente

	E6/01
	Arsénico, hexaclorociclopentadieno, creosota, criseno, naftaleno, fluoranteno, benzo(b)fluoranteno, benzo(a)pireno, indeno(1,2,3-cd)pireno, benzo(a)antraceno, dibenz(a)antraceno, acenaftaleno tolueno, ésteres de ácidos fósforoditioico y fósforotioico, forato, formaldehído, toxafeno

	E6/02
	Arsénico, hexaclorociclopentadieno, clordano, heptacloro, tolueno, ésteres de ácidos fósforoditioico y fósforotioico, forato, formaldehído, 2,4-diclorofenol, 2,6-diclorofenol, 2,4,6-triclorofenol, toxafeno, etilentiourea, dimetil sulfato y bromuro de metilo

	E7/01
	Pentaclorofenol, fenol, 2-clorofenol, p-cloro-m-cresol, 2,4-dimetilfenil, 2,4-dinitrofenol, triclorofenoles, tetraclorofenoles, 2,4-dinitrofenol, creosota, criseno, naftaleno, fluoranteno, benzo(b)fluoranteno, benzo(a)pireno, indeno(1,2,3-cd)pireno, benzo(a)antraceno, dibenz(a)antraceno, acenaftaleno

	E8/01
	Arsénico

	E8/02
	Arsénico

	E9/01
	Arsénico, plomo

	E9/02
	Antimonio

	E9/03
	Mercurio

	E9/04
	Mercurio

	E9/05
	Cloroformo, tetracloruro de carbono, hexacloroetano, tricloroetano, tetracloroetileno, dicloroetileno, 1,1,2,2-tetracloroetano

	E9/06
	Cromo hexavalente, plomo

	E9/07
	Cromo hexavalente, plomo

	E9/08
	Cromo hexavalente

	E9/09
	Cromo hexavalente

	E9/10
	Cianuro (complejos), cromo hexavalente

	E9/11
	Cromo hexavalente, plomo

	E9/12
	Cromo hexavalente

	E9/13
	Talio

	E10/01
	Acrilonitrilo, acetonitrilo, ácido cianhídrico

	E10/02
	Acrilonitrilo, acetonitrilo, ácido cianhídrico

	E10/03
	Acetonitrilo, acrilamida

	E10/04
	Anhídrido ftálico, anhídrido maléico

	E10/05
	Anhídrido ftálico, 1,4-naftoquinona

	E10/06
	Anhídrido ftálico, anhídrido maléico

	E10/07
	Anhídrido ftálico

	E10/08
	Anilina, difenilamina, nitrobenceno, fenilenediamina

	E10/09
	Anilina, nitrobenceno, fenilenediamina

	E10/10
	Tetracloruro de carbono, formaldehído, cloruro de metilo, cloruro de metileno, piridina, trietilamina

	E10/11
	Benceno, butilato, eptc, molinato, pebulato, vernolato

	E10/12
	Benomil, carbendazim, carbofurán, carbosulfán, cloroformo, cloruro de metileno

	E10/13
	Benomil, carbaril, carbendazim, carbofurán, carbosulfán, formaldehído, cloruro de metileno, trietilamina

	E10/14
	Antimonio, arsénico, metam-sodio, ziram

	E10/15
	Benceno, diclorobencenos, triclorobencenos, tetraclorobencenos, pentaclorobenceno, hexaclorobenceno, cloruro de bencilo

	E10/16
	Benceno, monoclorobenceno, diclorobencenos, 2,4,6-triclorofenol

	E10/17
	Cloruro de bencilo, clorobenceno, tolueno, triclorobenceno

	E10/18
	1,2-dicloroetano, tricloroetileno, hexaclorobutadieno, hexaclorobenceno

	E10/19
	Dicloroetileno, 1,1,1-tricloroetano, 1,1,2-tricloroetano, tetracloroetanos (1,1,2,2-tetracloroetano y 1,1,1,2-tetracloroetano), tricloroetileno, tetracloroetileno, tetracloruro de carbono, cloroformo, cloruro de vinilo, cloruro de vinilideno

	E10/20
	1,2,3,4,6,7,8-Heptaclorodibenzo-p-dioxina (1,2,3,4,6,7,8-HpCDD), 1,2,3,4,6,7,8-Heptaclorodibenzofurano (1,2,3,4,6,7,8-HpCDF), 1,2,3,4,6,7,8,9-Heptaclorodibenzofurano (1,2,3,4,6,7,8,9-HpCDF, HxCDDs (todas las Hexaclorodibenzo-p-dioxinas, HxCDFs (todos los Hexaclorodibenzofuranos, PeCDDs (todas las pentaclorodibenzo-p-dioxinas), OCDD (1,2,3,4,6,7,8,9-Octaclorodibenzo-p-dioxina), OCDF (1,2,3,4,6,7,8,9-Octaclorodibenzofurano), PeCDFs (todos los pentaclorodibenzofuranos), TCDDs (todas las Tetraclorodibenzo-p-dioxinas), TCDFs (todos los tetraclorodibenzofuranos)

	E10/21
	Mercurio

	E10/22
	Dibromuro de etileno

	E10/23
	Dibromuro de etileno

	E10/24
	Dibromuro de etileno

	E10/25
	Tetracloruro de carbono, tetracloroetileno, cloroformo, fosgeno

	E10/26
	Diisocianato de tolueno, toluen-2,4-diamina

	E10/27
	1,1-Dimetilhidracina

	E10/28
	1,1-Dimetilhidracina

	E10/29
	1,1-Dimetilhidracina

	E10/30
	1,1-Dimetilhidracina

	E10/31
	2,4 Dinitrotolueno

	E10/32
	Epiclorohidrina, cloroéteres [bis(clorometil)éter y bis(2-cloroetil)éteres], tricloropropano, dicloropropanoles

	E10/33
	Breas de fenol (hidrocarburos poliaromáticos)

	E10/34
	Antimonio, tetracloruro de carbono, cloroformo

	E10/35
	Paraldehído, piridinas, 2-picolina

	E10/36
	Anilina, benceno, difenilamina, nitrobenceno, fenilendiamina

	E10/37
	meta-Dinitrobenceno, 2,4-dinitrotolueno

	E10/38
	Hexaclorobenceno, hexaclorobutadieno, tetracloruro de carbono, hexacloroetano, percloroetileno

	E10/39
	2,4-Toluendiamina, o-toluidina, p-toluidina, anilina

	E10/40
	2,4-Toluendiamina, o-toluidina, p-toluidina, anilina

	E10/41
	2,4-Toluendiamina, o-toluidina, p-toluidina

	E10/42
	2,4-Toluendiamina

	E10/43
	Triclorobenceno, cloruro de bencilo, cloroformo, clorometano, clorobenceno, 1,4-diclorobenceno, hexaclorobenceno, pentaclorobenceno, 1,2,4,5-tetraclorobenceno, tolueno

	E10/44
	Benceno, tetracloruro de carbono, cloroformo, hexaclorobenceno, pentaclorobenceno, tolueno, 1,2,4,5-tetraclorobenceno, tetracloroetileno

	E10/45
	Tetracloruro de carbono, cloroformo, clorometano, 1,4-diclorobenceno, hexaclorobenceno, pentaclorobenceno, 1,2,4,5-tetraclorobenceno, 1,1,2,2-tetracloroetano, tetracloroetileno, 1,2,4-triclorobenceno

	E10/46
	1,1,1-tricloroetano, cloruro de vinilo

	E10/47
	1,1,2-tricloroetano, 1,1,1,2-tetracloroetano, 1,1,2,2-tetracloroetano

	E10/48
	1,2-dicloroetano, 1,1,1-tricloroetano, 1,1,2-tricloroetano

	E10/49
	1,2-dicloroetano, 1,1,1-tricloroetano, cloruro de vinilo, cloruro de vinilideno, cloroformo

	E10/50
	Hexaclorobenceno, hexaclorobutadieno, hexacloroetano, 1,1,1,2-tetracloroetano, 1,1,2,2-tetracloroetano, dicloruro de etileno

	NE 01
	Asbestos

	NE 02
	Asbestos

	NE 03
	Asbestos

	NE 04
	Cianuro (complejos)

	NE 05
	Cadmio, cromo hexavalente, níquel, cianuro (complejos)

	NE 06
	Cromo hexavalente, cianuro (complejos)

	NE 07
	Cianuro (sales)

	NE 08
	Cianuro (sales)

	NE 09
	Cianuro (sales)

	NE 10
	Cianuro (sales)

	NE 11
	Cianuro (sales)

	NE 12
	Pentaclorodibenzo-p-dioxinas, hexaclorodibenzo-p-dioxinas, pentaclorodibenzofuranos, hexaclorodibenzofuranos, pentaclorofenol y sus derivados

	NE 13
	Tetraclorodibenzo-p-dioxinas, pentaclorodibenzo-p-dioxinas, hexaclorodibenzo-p-dioxinas, tetraclorodibenzofuranos, pentaclorodibenzofuranos, hexaclorodibenzofuranos

	NE 14
	Tetraclorodibenzo-p-dioxinas, pentaclorodibenzo-p-dioxinas, tetraclorodibenzofuranos, pentaclorodibenzofuranos, triclorofenoles, tetraclorofenoles y sus derivados ácidos, ésteres, éteres, aminas y otras sales clorofenóxicas

	NE 15
	Clorometano, diclorometano, triclorometano, tetracloruro de carbono, cloroetileno, 1,1 dicloroetano, 1,2-dicloroetano, trans-1,2-dicloroetileno, 1,1-dicloroetileno, 1,1,1-tricloroetano, 1,1,2-tricloroetano, tricloroetileno, 1,1,1,2-tetracloroetano, 1,1,2,2-tetracloroetano, tetracloroetileno, pentacloroetano, hexacloroetano, cloruro de alilo (3-cloropropeno), dicloropropano, dicloropropeno, 2-cloro-1,3-butadieno, hexacloro-1,3-butadieno, hexaclorociclopentadieno, benceno, clorobenceno, diclorobenceno, 1,2,4-triclorobenceno, tetraclorobenceno, pentaclorobenceno, hexaclorobenceno, tolueno, naftaleno

	NE 16
	Tetraclorodibenzo-p-dioxinas, pentaclorodibenzo-p-dioxinas, hexaclorodibenzo-p-dioxinas, tetraclorodibenzofuranos, pentaclorodibenzofuranos, hexaclorodibenzofuranos

	NE 17
	Benzo(a)antraceno, benzo(a)pireno, dibenz(a,h)antraceno, indeno(1,2,3-cd)pireno, pentaclorofenol, arsénico, cromo, tetraclorodibenzo-p-dioxinas, pentaclorodibenzo-p-dioxinas, hexaclorodibenzo-p-dioxinas, heptaclorodibenzo-p-dioxinas, tetraclorodibenzofuranos, pentaclorodibenzofuranos, hexaclorodibenzofuranos, heptaclorodibenzofuranos

	NE 18
	Benzo(a)antraceno, benzo(k)fluoranteno, benzo(a)pireno, dibenz(a,h)antraceno, indeno(1,2,3-cd)pireno, naftaleno, arsénico, cromo

	NE 19
	Arsénico, cromo, plomo

	NE 20
	Todos los constituyentes que aparezcan en esta Norma Oficial Mexicana

	NE 21
	Tetraclorodibenzo-p-dioxinas, pentaclorodibenzo-p-dioxinas, hexaclorodibenzo-p-dioxinas, tetraclorodibenzofuranos, pentaclorodibenzofuranos, hexaclorodibenzofuranos, triclorofenoles, tetraclorofenoles, pentaclorofenoles y sus derivados ácidos, ésteres, éteres, aminas y otras sales clorofenóxicas

	N.A.: 


	No Aplica. Los residuos son peligrosos porque presentan características de Corrosividad, Reactividad, Explosividad y/o Inflamabilidad.


	APPENDIX I



	CRITERIA FOR LISTING HAZARDOUS WASTES FOR “SPECIFIC SOURCE” AND “NON-SPECIFIC SOURCE” DEPENDING ON THEIR ENVIRONMENTAL TOXICITY, ACUTE OR CHRONIC



	CODE
	Components for which wastes are listed 

	E1/01
	Cyanide (complex)

	E1/02
	Chromium hexavalent, lead

	E1/03
	Chromium hexavalent, lead, cadmium

	E1/04
	Lead, benzene, benzo(a)pyrene, dibenz(a,h)anthracene, benzo(a)anthracene, benzo(b)flouranthene, benzo(k)flouranthene, 3-methylchloranthene, 7,12-dimetilbenz(a)anthracene

	E2/01
	Arsenic, benzene, benzo(a)anthracene, benzo(b)flouranthene, benzo(k)flouranthene, benzo(a)pyrene, cyanide, Phenolic compounds, dibenz(a,h)anthracene, phenol, indene(1,2,3-cd)pyrene, naphatalene

	E3/01
	N.A.

	E3/02
	Lead

	E3/03
	N.A.

	E4/01
	Benzene y arsenic

	E4/02
	Benzene, benzo(a)pyrene, crisene, lead, chrome

	E4/03
	Benzene, benzo(a)pyrene, crisene, lead, chrome

	E4/04
	Chromium hexavalent, lead

	E4/05
	Lead, benzene, benzo(a)pyrene, dibenz(a,h)anthracene, benzo(a)anthracene, benzo(b)flouranthene, benzo(k)flouranthene, 3-methylchloranthene, 7,12-dimethyllbenz(a)anthracene. 

	E4/06
	Chromium hexavalent

	E4/07
	Chromium hexavalent, lead

	E4/08
	Chromium hexavalent, lead

	E4/09
	Chloroform, formaldehyde, methylene chloride, methyl chloride, paraldehyde, formic acid

	E4/10
	Chloroform, formaldehyde, methylene chloride, methyl chloride, paraldehyde, formic acid, chloracetaldehyde

	E4/11
	Chloromethane, dichloromethane, trichloromethane, carbon tetrachloride, choroethylene, 1,1- dichloroethane, 1,2-dichloroethane, trans-1-1-dichoroethylene, 1,1-dichoroethylene, 1,1,1-trichloroethane, 1,1,2-trichloroethane, trichoroethylene, 1,1,1,2-tetrachlorethane, 1,1,2,2-tetrachlorethane, tetrachoroethylene, pentachloroethane, hexachlorethane, allyl chloride (3-chloropropane), dichloropropane, dichloropropene, 2-chloro-1,3-butadiene, hexachloro-1,3-butadiene, hexachlorociclopentadiene, hexachlorocyclohexane, benzene, chlorobenzene, dichlorobenzenes, 1,2,4-trichlorobenzene, tetrachlorobenzene, pentachlorobenzene, hexachlorobenzene, toluene, naphatalene

	E5/01
	Lead, chromium hexavalent

	E6/01
	Arsenic, hexachlorocyclopentadiene, creosote, crisene, naphatalene, flouranthene, benzo(b)flouranthene, benzo(a)pyrene, indene(1,2,3-cd)pyrene, benzo-anthracene, dibenzo-anthracene, acenaphatalene toluene, phosphorus dithioic and phosphorus oics acid esters,  phorate, formaldehyde, toxaphene

	E6/02
	Arsenic, hexachlorocyclopentadiene, chlordane, heptachlor, toluene, phosphorus dithioic and phosphorus oics acid esters, phorate, formaldehyde, 2,4-dichlorophenol, 2,6-dichlorophenol, 2,4,6-trichlorophenol, toxaphene, ethylene thiourea, dimethyl sulphate and methyl bromide

	E7/01
	Pentachlorophenol, phenol, 2-clorophenol, p-chloro-m-cresol, 2,4-dimethylphenyl, 2,4-dinitrophenol, trichlorophenols, tetrachlorophenols, 2,4-dinitrophenol, creosote, crisene, naphatalene, flouranthene, benzo(b)flouranthene, benzo(a)pyrene, indene(1,2,3-cd)pyrene, benzo(a)anthracene, dibenz(a)anthracene, acenaphatalene

	E8/01
	Arsenic

	E8/02
	Arsenic

	E9/01
	Arsenic, lead

	E9/02
	Antimony

	E9/03
	Mercury

	E9/04
	Mercury

	E9/05
	Chloroform, carbon tetrachloride, hexachlorethane, trichloroethane, tetrachoroethylene, dichoroethylene, 1,1,2,2-tetrachlorethane

	E9/06
	Chromium hexavalent, lead

	E9/07
	Chromium hexavalent, lead

	E9/08
	Chromium hexavalent

	E9/09
	Chromium hexavalent

	E9/10
	Cyanide (complex), chromium hexavalent

	E9/11
	Chromium hexavalent, lead

	E9/12
	Chromium hexavalent

	E9/13
	Thallium

	E10/01
	Acrylonitrile, acetonitrile, hydrocyanic acid

	E10/02
	Acrilonitrile, acetonitrile, hydrocyanic acid

	E10/03
	Acetonitrile, acrylamide

	E10/04
	Phtalic anhydride, malefic anhydride

	E10/05
	Phtalic anhydride, 1,4-naphtoquinone

	E10/06
	Phtalic anhydride, maleic anhydride

	E10/07
	Phtalic anhydride

	E10/08
	Aniline, diphenylamine, nitrobenzene, phenylenediamine

	E10/09
	Aniline, nitrobenzene, phenylenediamine

	E10/10
	Carbon tetrachloride, formaldehyde, methyl chloride, methylene chloride, piridine, triethylamine

	E10/11
	Benzene, butylate, S-ethyl di-N,N-propylthiocarbamate, molinate, pebulate, vernolate

	E10/12
	Benomyl, carbendazim, carbofuran, carbosulfan, chloroform, methylene chloride

	E10/13
	Benomyl, carbaryl, carbendazim, carbofuran, carbosulfan, formaldehyde, methylene chloride, triethylamine

	E10/14
	Antimony, arsenic, metam-sodium, ziram

	E10/15
	Benzene, dichlorobenzenes, trichlorobenzenes, tetrachlorobenzenes, pentachlorobenzene, hexachlorobenzene, benzyl chloride

	E10/16
	Benzene, monochlorobenzene, dichlorobenzenes, 2,4,6-trichlorophenol

	E10/17
	Benzyl chloride, chlorobenzene, toluene, trichlorobenzene

	E10/18
	1,2-dichloroethane, trichoroethylene, hexachlorobutadiene, hexachlorobenzene

	E10/19
	Diclhoroethylene, 1,1,1-trichloroethane, 1,1,2-trichloroethane, tetrachlorethanes (1,1,2,2-tetrachlorethane y 1,1,1,2-tetrachlorethane), trichoroethylene, tetrachoroethylene, carbon tetrachloride, chloroform, vinyl chloride, vinylidene chloride

	E10/20
	1,2,3,4,6,7,8-Heptachlorodibenzo-p-dioxine (1,2,3,4,6,7,8-HpCDD), 1,2,3,4,6,7,8-Heptachlordibenzofuran (1,2,3,4,6,7,8-HpCDF), 1,2,3,4,6,7,8,9-Heptachlordibenzofuran (1,2,3,4,6,7,8,9-HpCDF, HxCDDs (all the Hexachlorodibenzo-p-dioxins, HxCDFs (all the Hexachlorodibenzofurans, PeCDDs (all the pentachlorodibenzene-p-dioxins), OCDD (1,2,3,4,6,7,8,9-Octachlorodibenzo-p-dioxin), OCDF (1,2,3,4,6,7,8,9-Octaclorodibenzofurano), PeCDFs (all the pentachlorodibenzofurans), TCDDs (all the Tetrachlorodibenzo-p-dioxins), TCDFs (all the tetrachlorodibenzofurans)

	E10/21
	Mercury

	E10/22
	Ethylene dibromide

	E10/23
	Ethylene dibromide

	E10/24
	Ethylene dibromide

	E10/25
	Carbon tetrachloride, tetrachoroethylene, chloroform, phosgene

	E10/26
	Toluene diisocyanate, toluene-2,4-diamine

	E10/27
	1,1-Dimethylhidracine

	E10/28
	1,1-Dimethylhidracine

	E10/29
	1,1-Dimethylhidracine

	E10/30
	1,1-Dimethylhidracine

	E10/31
	2,4 Dinitrotoluene

	E10/32
	Epichlorohidrine, cloroethers [bis(chloromethyl)ether y bis(2-cloroethyl)ethers], trichloropropane, dichloropropanals

	E10/33
	phenol  tars (polyaromatic hydrocarbons)

	E10/34
	Antimony, carbon tetrachloride, chloroform

	E10/35
	Paraldehyde, piridines, 2-picoline

	E10/36
	Aniline, benzene, diphenilamine, nitrobenzene, phenilendiamine

	E10/37
	meta-Dinitrobenzene, 2,4-dinitrotoluene

	E10/38
	Hexachlorobenzene, hexachlorobutadiene, carbon tetrachloride, hexachlorethane, perchoroethylene

	E10/39
	2,4-Toluene diamine, o-toluidine, p-toluidine, aniline

	E10/40
	2,4-Toluene diamine, o-toluidine, p-toluidine, aniline

	E10/41
	2,4-Toluene diamine, o-toluidine, p-toluidine

	E10/42
	2,4-Toluene diamine

	E10/43
	Trichlorobenzene, benzyl chloride, chloroform, chloromethane, chlorobenzene, 1,4-dichlorobenzene, hexachlorobenzene, pentachlorobenzene, 1,2,4,5-tetrachlorobenzene, toluene

	E10/44
	Benzene, carbon tetrachloride, chloroform, hexachlorobenzene, pentachlorobenzene, toluene, 1,2,4,5-tetrachlorobenzene, tetrachoroethylene

	E10/45
	Carbon tetrachloride, chloroform, chloromethane, 1,4-dichlorobenzene, hexachlorobenzene, pentachlorobenzene, 1,2,4,5-tetrachlorobenzene, 1,1,2,2-tetrachlorethane, tetrachoroethylene, 1,2,4-trichlorobenzene

	E10/46
	1,1,1-trichloroethane, vinyl chloride

	E10/47
	1,1,2-trichloroethane, 1,1,1,2-tetrachlorethane, 1,1,2,2-tetrachlorethane

	E10/48
	1,2-dichloroethane, 1,1,1-trichloroethane, 1,1,2-trichloroethane

	E10/49
	1,2-dichloroethane, 1,1,1-trichloroethane, vinyl chloride, vinylidene chloride, chloroform

	E10/50
	Hexachlorobenzene, hexachlorobutadiene, hexachlorethane, 1,1,1,2-tetrachlorethane, 1,1,2,2-tetrachlorethane, ethylene dichloride

	NE 01
	Asbestos

	NE 02
	Asbestos

	NE 03
	Asbestos

	NE 04
	Cyanide (complex)

	NE 05
	Cadmium, chromium hexavalent, nickel, cyanide (complex)

	NE 06
	Chromium hexavalent, cyanide (complex)

	NE 07
	Cyanide (salts)

	NE 08
	Cyanide (salts)

	NE 09
	Cyanide (salts)

	NE 10
	Cyanide (salts)

	NE 11
	Cyanide (salts)

	NE 12
	Pentachlorodibenzene-p-dioxins, hexachlorodibenzo-p-dioxins, pentachlorodibenzofurans, hexachlorodibenzofurans, pentachlorophenol and its derivatives

	NE 13
	Tetrachlorodibenzene-p-dioxins, pentachlorodibenzene-p-dioxins, hexachlorodibenzo-p-dioxins, tetrachlorodibenzofurans, pentachlorodibenzofurans, hexachlorodibenzofurans

	NE 14
	Tetrachlorodibenzene-p-dioxins, pentachlorodibenzene-p-dioxins, tetrachlorodibenzofurans, pentachlorodibenzofurans, trichlorophenols, tetrachlorophenols and their derivatives,  acids, esters, ethers, amines and other chlorophenoxic salts

	NE 15
	Chloromethane, dichloromethane, trichloromethane, carbon tetrachloride, choroethylene, 1,1 dichloroethane, 1,2-dichloroethane, trans-1,2-dichloroethylene, 1,1-dichloroethylene, 1,1,1-trichloroethane, 1,1,2-trichloroethane, trichloroethylene, 1,1,1,2-tetrachlorethane, 1,1,2,2-tetrachlorethane, tetrachoroethylene, pentachloroethane, hexachlorethane, allyl chloride (3-chloropropene), dichloropropane, dichloropropene, 2-cloro-1,3-butadiene, hexachloro-1,3-butadiene, hexachlorociyclopentadiene, benzene, chlorobenzene, dichlorobenzene, 1,2,4-trichlorobenzene, tetrachlorobenzene, pentachlorobenzene, hexachlorobenzene, toluene, naphatalene

	NE 16
	Tetrachlorodibenzene-p-dioxins, pentachlorodibenzene-p-dioxins, hexachlorodibenzo-p-dioxins, tetraclorodibenzofurans, pentachlorodibenzofurans, hexachlorodibenzofurans

	NE 17
	Benzo(a)anthracene, benzo(a)pyrene, dibenz(a,h)anthracene, indene(1,2,3-cd)pyrene, pentachlorophenol, arsenic, chrome, tetrachlorodibenzene-p-dioxins, pentachlorodibenzene-p-dioxins, hexachlorodibenzo-p-dioxins, heptachlordibenzo-p-dioxins, tetraclorodibenzofurans, pentaclorodibenzofurans, hexachlorodibenzofurans, heptachlordibenzofurans

	NE 18
	Benzo(a)anthracene, benzo(k)flouranthene, benzo(a)pyrene, dibenz(a,h)anthracene, indene(1,2,3-cd)pyrene, naphatalene, arsenic, chrome

	NE 19
	Arsenic, chrome, lead

	NE 20
	All the components that appear in this Official Mexican Standard 

	NE 21
	Tetrachlorodibenzene-p-dioxins, pentachlorodibenzene-p-dioxins, hexachlorodibenzo-p-dioxins, tetrachlorodibenzofurans, pentachlorodibenzofurans, hexachlorodibenzofurans, trichlorophenols, tetrachlorophenols, pentachlorophenols and their derivatives acids, esters, ethers, amines and other chlorophenoxic salts 

	
	

	N.A.: 


	Does not apply. The wastes are hazardous because they present characteristics of Corrosivity, Explosivity, and/or flammability 


______________
Hazardous waste
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